{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["废水排放"],"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"废水排放","index":0,"n_rows":80,"n_cols":25,"rows_kept":80,"merged":[[0,0,0,24]],"flags":["formulas_cached_only"]}
["执法监测废水排放数据","","","","","","","","","","","","","","","","","","","","","","","",""]
["监测年","监测月","监测日","市","县","企业名称","企业类别","行业类别","名录类别","监测点名称","排放标准类型","排放标准名称","标准条目","废水工作负荷","废水流量","废水水温","监测项目","项目监测日期","排放浓度","取值单位","排放上限","排放下限","是否有评价限值","是否超标","超标倍数"]
["2024","07","24","新余市","渝水区","新余钢铁集团有限公司中心医院","工业企业","8411|综合医院","水环境","南院污水处理站废水排放口(DW005)","国家标准","医疗机构水污染物排放标准(GB18466-2005)","（表2）综合医疗机构和其他医疗机构水污染物排放限值（日均值）,含氯消毒剂,消毒接触池的接触时间大于等于1小时，接触池出口,预处理标准","82","","37.1","悬浮物","2024-07-24","17","mg/L","60","","是","否",""]
["2024","07","24","新余市","渝水区","新余钢铁集团有限公司中心医院","工业企业","8411|综合医院","水环境","南院污水处理站废水排放口(DW005)","国家标准","医疗机构水污染物排放标准(GB18466-2005)","（表2）综合医疗机构和其他医疗机构水污染物排放限值（日均值）,含氯消毒剂,消毒接触池的接触时间大于等于1小时，接触池出口,预处理标准","82","","37.1","pH值","2024-07-24","8.0","无量纲","9","6","是","否",""]
["2024","07","24","新余市","渝水区","新余钢铁集团有限公司中心医院","工业企业","8411|综合医院","水环境","南院污水处理站废水排放口(DW005)","国家标准","医疗机构水污染物排放标准(GB18466-2005)","（表2）综合医疗机构和其他医疗机构水污染物排放限值（日均值）,含氯消毒剂,消毒接触池的接触时间大于等于1小时，接触池出口,预处理标准","82","","37.1","挥发酚","2024-07-24","<0.01","mg/L","1.0","","是","否",""]
["2024","07","24","新余市","渝水区","新余钢铁集团有限公司中心医院","工业企业","8411|综合医院","水环境","北院污水处理站废水排放口(DW004)","国家标准","医疗机构水污染物排放标准(GB18466-2005)","（表2）综合医疗机构和其他医疗机构水污染物排放限值（日均值）,含氯消毒剂,消毒接触池的接触时间大于等于1小时，接触池出口,预处理标准","85","","33.9","五日生化需氧量（BOD5）","2024-07-24","1.4","mg/L","100","","是","否",""]
["2024","07","24","新余市","渝水区","新余钢铁集团有限公司中心医院","工业企业","8411|综合医院","水环境","北院污水处理站废水排放口(DW004)","国家标准","医疗机构水污染物排放标准(GB18466-2005)","（表2）综合医疗机构和其他医疗机构水污染物排放限值（日均值）,含氯消毒剂,消毒接触池的接触时间大于等于1小时，接触池出口,预处理标准","85","","33.9","pH值","2024-07-24","7.9","无量纲","9","6","是","否",""]
["2024","07","24","新余市","渝水区","新余钢铁集团有限公司中心医院","工业企业","8411|综合医院","水环境","北院污水处理站废水排放口(DW004)","国家标准","医疗机构水污染物排放标准(GB18466-2005)","（表2）综合医疗机构和其他医疗机构水污染物排放限值（日均值）,含氯消毒剂,消毒接触池的接触时间大于等于1小时，接触池出口,预处理标准","85","","33.9","粪大肠菌群数","2024-07-24","24000","MPN/L","5000","","是","是","3.80"]
["2024","07","24","新余市","渝水区","新余钢铁集团有限公司中心医院","工业企业","8411|综合医院","水环境","南院污水处理站废水排放口(DW005)","国家标准","医疗机构水污染物排放标准(GB18466-2005)","（表2）综合医疗机构和其他医疗机构水污染物排放限值（日均值）,含氯消毒剂,消毒接触池的接触时间大于等于1小时，接触池出口,预处理标准","82","","37.1","石油类","2024-07-24","<0.06","mg/L","20","","是","否",""]
["2024","07","24","新余市","渝水区","新余钢铁集团有限公司中心医院","工业企业","8411|综合医院","水环境","北院污水处理站废水排放口(DW004)","国家标准","医疗机构水污染物排放标准(GB18466-2005)","（表2）综合医疗机构和其他医疗机构水污染物排放限值（日均值）,含氯消毒剂,消毒接触池的接触时间大于等于1小时，接触池出口,预处理标准","85","","33.9","氰化物（总氰化合物）","2024-07-24","<0.001","mg/L","0.5","","是","否",""]
["2024","07","24","新余市","渝水区","新余钢铁集团有限公司中心医院","工业企业","8411|综合医院","水环境","南院污水处理站废水排放口(DW005)","国家标准","医疗机构水污染物排放标准(GB18466-2005)","（表2）综合医疗机构和其他医疗机构水污染物排放限值（日均值）,含氯消毒剂,消毒接触池的接触时间大于等于1小时，接触池出口,预处理标准","82","","37.1","五日生化需氧量（BOD5）","2024-07-24","2.2","mg/L","100","","是","否",""]
["2024","07","24","新余市","渝水区","新余钢铁集团有限公司中心医院","工业企业","8411|综合医院","水环境","北院污水处理站废水排放口(DW004)","国家标准","医疗机构水污染物排放标准(GB18466-2005)","（表2）综合医疗机构和其他医疗机构水污染物排放限值（日均值）,含氯消毒剂,消毒接触池的接触时间大于等于1小时，接触池出口,预处理标准","85","","33.9","石油类","2024-07-24","<0.06","mg/L","20","","是","否",""]
["2024","07","24","新余市","渝水区","新余钢铁集团有限公司中心医院","工业企业","8411|综合医院","水环境","南院污水处理站废水排放口(DW005)","地方标准","城东污水处理厂接管标准(009)","城东污水处理厂接管标准","82","","37.1","氨氮","2024-07-24","3.82","mg/L","25","","是","否",""]
["2024","07","24","新余市","渝水区","新余钢铁集团有限公司中心医院","工业企业","8411|综合医院","水环境","南院污水处理站废水排放口(DW005)","国家标准","医疗机构水污染物排放标准(GB18466-2005)","（表2）综合医疗机构和其他医疗机构水污染物排放限值（日均值）,含氯消毒剂,消毒接触池的接触时间大于等于1小时，接触池出口,预处理标准","82","","37.1","化学需氧量","2024-07-24","42","mg/L","250","","是","否",""]
["2024","07","24","新余市","渝水区","新余钢铁集团有限公司中心医院","工业企业","8411|综合医院","水环境","南院污水处理站废水排放口(DW005)","国家标准","医疗机构水污染物排放标准(GB18466-2005)","（表2）综合医疗机构和其他医疗机构水污染物排放限值（日均值）,含氯消毒剂,消毒接触池的接触时间大于等于1小时，接触池出口,预处理标准","82","","37.1","氰化物（总氰化合物）","2024-07-24","<0.001","mg/L","0.5","","是","否",""]
["2024","07","24","新余市","渝水区","新余钢铁集团有限公司中心医院","工业企业","8411|综合医院","水环境","北院污水处理站废水排放口(DW004)","国家标准","医疗机构水污染物排放标准(GB18466-2005)","（表2）综合医疗机构和其他医疗机构水污染物排放限值（日均值）,含氯消毒剂,消毒接触池的接触时间大于等于1小时，接触池出口,预处理标准","85","","33.9","动植物油","2024-07-24","<0.06","mg/L","20","","是","否",""]
["2024","07","24","新余市","渝水区","新余钢铁集团有限公司中心医院","工业企业","8411|综合医院","水环境","北院污水处理站废水排放口(DW004)","国家标准","医疗机构水污染物排放标准(GB18466-2005)","（表2）综合医疗机构和其他医疗机构水污染物排放限值（日均值）,含氯消毒剂,消毒接触池的接触时间大于等于1小时，接触池出口,预处理标准","85","","33.9","悬浮物","2024-07-24","15","mg/L","60","","是","否",""]
["2024","07","24","新余市","渝水区","新余钢铁集团有限公司中心医院","工业企业","8411|综合医院","水环境","北院污水处理站废水排放口(DW004)","国家标准","医疗机构水污染物排放标准(GB18466-2005)","（表2）综合医疗机构和其他医疗机构水污染物排放限值（日均值）,含氯消毒剂,消毒接触池的接触时间大于等于1小时，接触池出口,预处理标准","85","","33.9","阴离子表面活性剂（LAS）","2024-07-24","1.64","mg/L","10","","是","否",""]
["2024","07","24","新余市","渝水区","新余钢铁集团有限公司中心医院","工业企业","8411|综合医院","水环境","北院污水处理站废水排放口(DW004)","地方标准","城东污水处理厂接管标准(009)","城东污水处理厂接管标准","85","","33.9","氨氮","2024-07-24","2.59","mg/L","25","","是","否",""]
["2024","07","24","新余市","渝水区","新余钢铁集团有限公司中心医院","工业企业","8411|综合医院","水环境","南院污水处理站废水排放口(DW005)","国家标准","医疗机构水污染物排放标准(GB18466-2005)","（表2）综合医疗机构和其他医疗机构水污染物排放限值（日均值）,含氯消毒剂,消毒接触池的接触时间大于等于1小时，接触池出口,预处理标准","82","","37.1","粪大肠菌群数","2024-07-24","237","MPN/L","5000","","是","否",""]
["2024","07","24","新余市","渝水区","新余钢铁集团有限公司中心医院","工业企业","8411|综合医院","水环境","南院污水处理站废水排放口(DW005)","国家标准","医疗机构水污染物排放标准(GB18466-2005)","（表2）综合医疗机构和其他医疗机构水污染物排放限值（日均值）,含氯消毒剂,消毒接触池的接触时间大于等于1小时，接触池出口,预处理标准","82","","37.1","阴离子表面活性剂（LAS）","2024-07-24","0.16","mg/L","10","","是","否",""]
["2024","07","24","新余市","渝水区","新余钢铁集团有限公司中心医院","工业企业","8411|综合医院","水环境","北院污水处理站废水排放口(DW004)","国家标准","医疗机构水污染物排放标准(GB18466-2005)","（表2）综合医疗机构和其他医疗机构水污染物排放限值（日均值）,含氯消毒剂,消毒接触池的接触时间大于等于1小时，接触池出口,预处理标准","85","","33.9","化学需氧量","2024-07-24","27","mg/L","250","","是","否",""]
["2024","07","24","新余市","渝水区","新余钢铁集团有限公司中心医院","工业企业","8411|综合医院","水环境","北院污水处理站废水排放口(DW004)","国家标准","医疗机构水污染物排放标准(GB18466-2005)","（表2）综合医疗机构和其他医疗机构水污染物排放限值（日均值）,含氯消毒剂,消毒接触池的接触时间大于等于1小时，接触池出口,预处理标准","85","","33.9","挥发酚","2024-07-24","<0.01","mg/L","1.0","","是","否",""]
["2024","07","24","新余市","渝水区","新余钢铁集团有限公司中心医院","工业企业","8411|综合医院","水环境","南院污水处理站废水排放口(DW005)","国家标准","医疗机构水污染物排放标准(GB18466-2005)","（表2）综合医疗机构和其他医疗机构水污染物排放限值（日均值）,含氯消毒剂,消毒接触池的接触时间大于等于1小时，接触池出口,预处理标准","82","","37.1","动植物油","2024-07-24","<0.06","mg/L","20","","是","否",""]
["2024","07","24","新余市","渝水区","新余袁河医院有限公司","工业企业","8411|综合医院","水环境","综合污水处理站废水排放口001","国家标准","医疗机构水污染物排放标准(GB18466-2005)","（表2）综合医疗机构和其他医疗机构水污染物排放限值（日均值）,含氯消毒剂,消毒接触池的接触时间大于等于1小时，接触池出口,预处理标准","21","","31.8","石油类","2024-07-24","<0.06","mg/L","20","","是","否",""]
["2024","07","24","新余市","渝水区","新余袁河医院有限公司","工业企业","8411|综合医院","水环境","综合污水处理站废水排放口001","国家标准","医疗机构水污染物排放标准(GB18466-2005)","（表2）综合医疗机构和其他医疗机构水污染物排放限值（日均值）,含氯消毒剂,消毒接触池的接触时间大于等于1小时，接触池出口,预处理标准","21","","31.8","pH值","2024-07-24","7.0","无量纲","9","6","是","否",""]
["2024","07","24","新余市","渝水区","新余袁河医院有限公司","工业企业","8411|综合医院","水环境","综合污水处理站废水排放口001","国家标准","医疗机构水污染物排放标准(GB18466-2005)","（表2）综合医疗机构和其他医疗机构水污染物排放限值（日均值）,含氯消毒剂,消毒接触池的接触时间大于等于1小时，接触池出口,预处理标准","21","","31.8","五日生化需氧量（BOD5）","2024-07-24","1.7","mg/L","100","","是","否",""]
["2024","07","24","新余市","渝水区","新余袁河医院有限公司","工业企业","8411|综合医院","水环境","综合污水处理站废水排放口001","国家标准","医疗机构水污染物排放标准(GB18466-2005)","（表2）综合医疗机构和其他医疗机构水污染物排放限值（日均值）,含氯消毒剂,消毒接触池的接触时间大于等于1小时，接触池出口,预处理标准","21","","31.8","挥发酚","2024-07-24","<0.01","mg/L","1.0","","是","否",""]
["2024","07","24","新余市","渝水区","新余袁河医院有限公司","工业企业","8411|综合医院","水环境","综合污水处理站废水排放口001","国家标准","医疗机构水污染物排放标准(GB18466-2005)","（表2）综合医疗机构和其他医疗机构水污染物排放限值（日均值）,含氯消毒剂,消毒接触池的接触时间大于等于1小时，接触池出口,预处理标准","21","","31.8","化学需氧量","2024-07-24","16","mg/L","250","","是","否",""]
["2024","07","24","新余市","渝水区","新余袁河医院有限公司","工业企业","8411|综合医院","水环境","综合污水处理站废水排放口001","国家标准","医疗机构水污染物排放标准(GB18466-2005)","（表2）综合医疗机构和其他医疗机构水污染物排放限值（日均值）,含氯消毒剂,消毒接触池的接触时间大于等于1小时，接触池出口,预处理标准","21","","31.8","阴离子表面活性剂（LAS）","2024-07-24","0.15","mg/L","10","","是","否",""]
["2024","07","24","新余市","渝水区","新余袁河医院有限公司","工业企业","8411|综合医院","水环境","综合污水处理站废水排放口001","国家标准","医疗机构水污染物排放标准(GB18466-2005)","（表2）综合医疗机构和其他医疗机构水污染物排放限值（日均值）,含氯消毒剂,消毒接触池的接触时间大于等于1小时，接触池出口,预处理标准","21","","31.8","粪大肠菌群数","2024-07-24","12","MPN/L","5000","","是","否",""]
["2024","07","24","新余市","渝水区","新余袁河医院有限公司","工业企业","8411|综合医院","水环境","综合污水处理站废水排放口001","国家标准","医疗机构水污染物排放标准(GB18466-2005)","（表2）综合医疗机构和其他医疗机构水污染物排放限值（日均值）,含氯消毒剂,消毒接触池的接触时间大于等于1小时，接触池出口,预处理标准","21","","31.8","动植物油","2024-07-24","<0.06","mg/L","20","","是","否",""]
["2024","07","24","新余市","渝水区","新余袁河医院有限公司","工业企业","8411|综合医院","水环境","综合污水处理站废水排放口001","国家标准","医疗机构水污染物排放标准(GB18466-2005)","（表2）综合医疗机构和其他医疗机构水污染物排放限值（日均值）,含氯消毒剂,消毒接触池的接触时间大于等于1小时，接触池出口,预处理标准","21","","31.8","悬浮物","2024-07-24","20","mg/L","60","","是","否",""]
["2024","07","24","新余市","渝水区","新余袁河医院有限公司","工业企业","8411|综合医院","水环境","综合污水处理站废水排放口001","国家标准","医疗机构水污染物排放标准(GB18466-2005)","（表2）综合医疗机构和其他医疗机构水污染物排放限值（日均值）,含氯消毒剂,消毒接触池的接触时间大于等于1小时，接触池出口,预处理标准","21","","31.8","氰化物（总氰化合物）","2024-07-24","<0.001","mg/L","0.5","","是","否",""]
["2024","07","24","新余市","渝水区","新余袁河医院有限公司","工业企业","8411|综合医院","水环境","综合污水处理站废水排放口001","地方标准","城东污水处理厂接管标准(009)","城东污水处理厂接管标准","21","","31.8","氨氮","2024-07-24","0.485","mg/L","25","","是","否",""]
["2024","07","25","新余市","","江西东鹏新材料有限责任公司南源路厂","工业企业","2613|无机盐制造","水环境","废水总排口(DW001)","地方标准","新余高新区污水处理厂接管标准(001)","污水处理厂接管进水限值","88","","38.3","总氮（以N计）","2024-07-25","1.15","mg/L","50","","是","否",""]
["2024","07","25","新余市","","江西东鹏新材料有限责任公司南源路厂","工业企业","2613|无机盐制造","水环境","废水总排口(DW001)","国家标准","无机化学工业污染物排放标准(GB31573-2015)"," （表1）水污染物排放限值,间接排放","88","","38.3","氟化物","2024-07-25","4.00","mg/L","6","","是","否",""]
["2024","07","25","新余市","","江西东鹏新材料有限责任公司南源路厂","工业企业","2613|无机盐制造","水环境","废水总排口(DW001)","国家标准","无机化学工业污染物排放标准(GB31573-2015)"," （表1）水污染物排放限值,间接排放","88","","38.3","悬浮物","2024-07-25","10","mg/L","100","","是","否",""]
["2024","07","25","新余市","","江西东鹏新材料有限责任公司南源路厂","工业企业","2613|无机盐制造","水环境","车间排口","国家标准","无机化学工业污染物排放标准(GB31573-2015)"," （表1）水污染物排放限值,间接排放","88","","","总镉","2024-07-25","0.00008","mg/L","0.05","","是","否",""]
["2024","07","25","新余市","","江西东鹏新材料有限责任公司南源路厂","工业企业","2613|无机盐制造","水环境","废水总排口(DW001)","国家标准","无机化学工业污染物排放标准(GB31573-2015)"," （表1）水污染物排放限值,间接排放","88","","38.3","pH值","2024-07-25","7.4","无量纲","9","6","是","否",""]
["2024","07","25","新余市","","江西东鹏新材料有限责任公司南源路厂","工业企业","2613|无机盐制造","水环境","废水总排口(DW001)","国家标准","污水综合排放标准(GB8978-1996)","（表4）第二类污染物最高允许排放浓度（1998年1月1日后建的单位）,一切排污单位 ,一级标准","88","","38.3","对-二甲苯","2024-07-25","<0.002","mg/L","0.4","","是","否",""]
["2024","07","25","新余市","","江西东鹏新材料有限责任公司南源路厂","工业企业","2613|无机盐制造","水环境","废水总排口(DW001)","国家标准","污水综合排放标准(GB8978-1996)","（表4）第二类污染物最高允许排放浓度（1998年1月1日后建的单位）,一切排污单位 ,一级标准","88","","38.3","挥发酚","2024-07-25","0.234","mg/L","0.5","","是","否",""]
["2024","07","25","新余市","","江西东鹏新材料有限责任公司南源路厂","工业企业","2613|无机盐制造","水环境","车间排口","国家标准","无机化学工业污染物排放标准(GB31573-2015)"," （表1）水污染物排放限值,间接排放","88","","","六价铬","2024-07-25","0.009","mg/L","0.1","","是","否",""]
["2024","07","25","新余市","","江西东鹏新材料有限责任公司南源路厂","工业企业","2613|无机盐制造","水环境","车间排口","地方标准","工业废水铊污染物排放标准(DB36/1149-2019)","总铊","88","","","总铊","2024-07-25","0.00009","mg/L","0.005","","是","否",""]
["2024","07","25","新余市","","江西东鹏新材料有限责任公司南源路厂","工业企业","2613|无机盐制造","水环境","废水总排口(DW001)","国家标准","无机化学工业污染物排放标准(GB31573-2015)"," （表1）水污染物排放限值,间接排放","88","","38.3","总磷（以P计）","2024-07-25","0.15","mg/L","2","","是","否",""]
["2024","07","25","新余市","","江西东鹏新材料有限责任公司南源路厂","工业企业","2613|无机盐制造","水环境","车间排口","国家标准","无机化学工业污染物排放标准(GB31573-2015)"," （表1）水污染物排放限值,间接排放","88","","","总锑","2024-07-25","0.0198","mg/L","0.3","","是","否",""]
["2024","07","25","新余市","","江西东鹏新材料有限责任公司南源路厂","工业企业","2613|无机盐制造","水环境","废水总排口(DW001)","国家标准","污水综合排放标准(GB8978-1996)","（表4）第二类污染物最高允许排放浓度（1998年1月1日后建的单位）,一切排污单位 ,一级标准","88","","38.3","间-二甲苯","2024-07-25","0.010","mg/L","0.4","","是","否",""]
["2024","07","25","新余市","","江西东鹏新材料有限责任公司南源路厂","工业企业","2613|无机盐制造","水环境","车间排口","国家标准","无机化学工业污染物排放标准(GB31573-2015)"," （表1）水污染物排放限值,间接排放","88","","","总铅","2024-07-25","<0.00009","mg/L","0.5","","是","否",""]
["2024","07","25","新余市","","江西东鹏新材料有限责任公司南源路厂","工业企业","2613|无机盐制造","水环境","废水总排口(DW001)","国家标准","无机化学工业污染物排放标准(GB31573-2015)"," （表1）水污染物排放限值,间接排放","88","","38.3","氰化物（总氰化合物）","2024-07-25","<0.001","mg/L","0.5","","是","否",""]
["2024","07","25","新余市","","江西东鹏新材料有限责任公司南源路厂","工业企业","2613|无机盐制造","水环境","废水总排口(DW001)","地方标准","新余高新区污水处理厂接管标准(001)","污水处理厂接管进水限值","88","","38.3","氨氮（NH3-N）","2024-07-25","0.273","mg/L","35","","是","否",""]
["2024","07","25","新余市","","江西东鹏新材料有限责任公司南源路厂","工业企业","2613|无机盐制造","水环境","废水总排口(DW001)","国家标准","污水综合排放标准(GB8978-1996)","（表4）第二类污染物最高允许排放浓度（1998年1月1日后建的单位）,一切排污单位 ,一级标准","88","","38.3","邻-二甲苯","2024-07-25","0.013","mg/L","0.4","","是","否",""]
["2024","07","25","新余市","","江西东鹏新材料有限责任公司南源路厂","工业企业","2613|无机盐制造","水环境","废水总排口(DW001)","国家标准","无机化学工业污染物排放标准(GB31573-2015)"," （表1）水污染物排放限值,间接排放","88","","38.3","硫化物","2024-07-25","<0.01","mg/L","1","","是","否",""]
["2024","07","25","新余市","","江西东鹏新材料有限责任公司南源路厂","工业企业","2613|无机盐制造","水环境","废水总排口(DW001)","国家标准","无机化学工业污染物排放标准(GB31573-2015)"," （表1）水污染物排放限值,间接排放","88","","38.3","石油类","2024-07-25","<0.06","mg/L","6","","是","否",""]
["2024","07","25","新余市","","江西东鹏新材料有限责任公司南源路厂","工业企业","2613|无机盐制造","水环境","车间排口","国家标准","无机化学工业污染物排放标准(GB31573-2015)"," （表1）水污染物排放限值,间接排放","88","","","总汞","2024-07-25","0.00010","mg/L","0.005","","是","否",""]
["2024","07","25","新余市","","江西东鹏新材料有限责任公司南源路厂","工业企业","2613|无机盐制造","水环境","车间排口","国家标准","无机化学工业污染物排放标准(GB31573-2015)"," （表1）水污染物排放限值,间接排放","88","","","总砷","2024-07-25","0.0011","mg/L","0.3","","是","否",""]
["2024","07","25","新余市","","江西东鹏新材料有限责任公司南源路厂","工业企业","2613|无机盐制造","水环境","废水总排口(DW001)","国家标准","无机化学工业污染物排放标准(GB31573-2015)"," （表1）水污染物排放限值,间接排放","88","","38.3","化学需氧量","2024-07-25","42","mg/L","200","","是","否",""]
["2024","07","02","新余市","","江西新余国泰特种化工有限责任公司","工业企业","267|炸药、火工及焰火产品制造","水环境","GTX车间排口","国家标准","兵器工业水污染物排放标准火工药剂(GB14470.2-2002)","（表2）2003年7月1日起建设的火工药剂生产企业及其新、改、扩建项目水污染物最高允许日均排放浓度,叠氮化钠","6","","","肼（联氨）","2024-07-02","<0.003","mg/L","3.0","","是","否",""]
["2024","07","02","新余市","","江西新余国泰特种化工有限责任公司","工业企业","267|炸药、火工及焰火产品制造","水环境","废水总排口","国家标准","兵器工业水污染物排放标准火工药剂(GB14470.2-2002)","（表2）2003年7月1日起建设的火工药剂生产企业及其新、改、扩建项目水污染物最高允许日均排放浓度,三硝基间苯二酚","8","","24","硝基酚类","2024-07-02","<0.07","mg/L","3.0","","是","否",""]
["2024","07","02","新余市","","江西新余国泰特种化工有限责任公司","工业企业","267|炸药、火工及焰火产品制造","水环境","废水总排口","地方标准","污水综合排放标准(GB8978-1996)","表4第二类污染物最高允许排放浓度,一级标准","8","","24","氨氮（NH3-N）","2024-07-02","0.846","mg/L","15","","是","否",""]
["2024","07","02","新余市","","江西新余国泰特种化工有限责任公司","工业企业","267|炸药、火工及焰火产品制造","水环境","GTX车间排口","","","","6","","","锑","2024-07-02","0.00028","mg/L","","","否","",""]
["2024","07","02","新余市","","江西新余国泰特种化工有限责任公司","工业企业","267|炸药、火工及焰火产品制造","水环境","废水总排口","地方标准","污水综合排放标准(GB8978-1996)","表4第二类污染物最高允许排放浓度,一级标准","8","","24","石油类","2024-07-02","<0.06","mg/L","5","","是","否",""]
["2024","07","02","新余市","","江西新余国泰特种化工有限责任公司","工业企业","267|炸药、火工及焰火产品制造","水环境","废水总排口","地方标准","污水综合排放标准(GB8978-1996)","表4第二类污染物最高允许排放浓度,一级标准","8","","24","化学需氧量","2024-07-02","19","mg/L","100","","是","否",""]
["2024","07","02","新余市","","江西新余国泰特种化工有限责任公司","工业企业","267|炸药、火工及焰火产品制造","水环境","GTX车间排口","国家标准","兵器工业水污染物排放标准火工药剂(GB14470.2-2002)","（表2）2003年7月1日起建设的火工药剂生产企业及其新、改、扩建项目水污染物最高允许日均排放浓度,亚铁氰化铅","6","","","总铅","2024-07-02","0.00278","mg/L","1.0","","是","否",""]
["2024","07","02","新余市","","江西新余国泰特种化工有限责任公司","工业企业","267|炸药、火工及焰火产品制造","水环境","废水总排口","地方标准","污水综合排放标准(GB8978-1996)","表4第二类污染物最高允许排放浓度,一级标准","8","","24","总锌","2024-07-02","0.0341","mg/L","2.0","","是","否",""]
["2024","07","02","新余市","","江西新余国泰特种化工有限责任公司","工业企业","267|炸药、火工及焰火产品制造","水环境","废水总排口","地方标准","污水综合排放标准(GB8978-1996)","表4第二类污染物最高允许排放浓度,一级标准","8","","24","色度","2024-07-02","6","倍","50","","是","否",""]
["2024","07","02","新余市","","江西新余国泰特种化工有限责任公司","工业企业","267|炸药、火工及焰火产品制造","水环境","GTX车间排口","地方标准","江西省地方标准《工业废水铊污染物排放标准》[地标][地标](DB36/1149——2019)","工业废水铊污染物排放","6","","","铊","2024-07-02","<0.00002","mg/L","0.005","","是","否",""]
["2024","07","02","新余市","","江西新余国泰特种化工有限责任公司","工业企业","267|炸药、火工及焰火产品制造","水环境","废水总排口","地方标准","污水综合排放标准(GB8978-1996)","表4第二类污染物最高允许排放浓度,一级标准","8","","24","悬浮物","2024-07-02","12","mg/L","70","","是","否",""]
["2024","07","02","新余市","","江西新余国泰特种化工有限责任公司","工业企业","267|炸药、火工及焰火产品制造","水环境","废水总排口","地方标准","污水综合排放标准(GB8978-1996)","表4第二类污染物最高允许排放浓度,一级标准","8","","24","五日生化需氧量（BOD5）","2024-07-02","1.5","mg/L","20","","是","否",""]
["2024","07","02","新余市","","江西新余国泰特种化工有限责任公司","工业企业","267|炸药、火工及焰火产品制造","水环境","废水总排口","地方标准","污水综合排放标准(GB8978-1996)","表4第二类污染物最高允许排放浓度,一级标准","8","","24","pH值","2024-07-02","7.5","无量纲","9","6","是","否",""]
["2024","07","24","新余市","","新余市人民医院","工业企业","8411|综合医院","水环境","废水排放口001(DW001)","国家标准","医疗机构水污染物排放标准(GB18466-2005)","（表2）综合医疗机构和其他医疗机构水污染物排放限值（日均值）,含氯消毒剂,消毒接触池的接触时间大于等于1小时，接触池出口,预处理标准","67","","32.7","石油类","2024-07-24","<0.06","mg/L","20","","是","否",""]
["2024","07","24","新余市","","新余市人民医院","工业企业","8411|综合医院","水环境","废水排放口001(DW001)","国家标准","医疗机构水污染物排放标准(GB18466-2005)","（表2）综合医疗机构和其他医疗机构水污染物排放限值（日均值）,含氯消毒剂,消毒接触池的接触时间大于等于1小时，接触池出口,预处理标准","67","","32.7","粪大肠菌群数","2024-07-24","24000","MPN/L","5000","","是","是","3.80"]
["2024","07","24","新余市","","新余市人民医院","工业企业","8411|综合医院","水环境","废水排放口001(DW001)","国家标准","医疗机构水污染物排放标准(GB18466-2005)","（表2）综合医疗机构和其他医疗机构水污染物排放限值（日均值）,含氯消毒剂,消毒接触池的接触时间大于等于1小时，接触池出口,预处理标准","67","","32.7","氰化物（总氰化合物）","2024-07-24","<0.001","mg/L","0.5","","是","否",""]
["2024","07","24","新余市","","新余市人民医院","工业企业","8411|综合医院","水环境","废水排放口001(DW001)","国家标准","医疗机构水污染物排放标准(GB18466-2005)","（表2）综合医疗机构和其他医疗机构水污染物排放限值（日均值）,含氯消毒剂,消毒接触池的接触时间大于等于1小时，接触池出口,预处理标准","67","","32.7","动植物油","2024-07-24","<0.06","mg/L","20","","是","否",""]
["2024","07","24","新余市","","新余市人民医院","工业企业","8411|综合医院","水环境","废水排放口001(DW001)","国家标准","医疗机构水污染物排放标准(GB18466-2005)","（表2）综合医疗机构和其他医疗机构水污染物排放限值（日均值）,含氯消毒剂,消毒接触池的接触时间大于等于1小时，接触池出口,预处理标准","67","","32.7","挥发酚","2024-07-24","<0.01","mg/L","1.0","","是","否",""]
["2024","07","24","新余市","","新余市人民医院","工业企业","8411|综合医院","水环境","废水排放口001(DW001)","国家标准","医疗机构水污染物排放标准(GB18466-2005)","（表2）综合医疗机构和其他医疗机构水污染物排放限值（日均值）,含氯消毒剂,消毒接触池的接触时间大于等于1小时，接触池出口,预处理标准","67","","32.7","阴离子表面活性剂（LAS）","2024-07-24","0.50","mg/L","10","","是","否",""]
["2024","07","24","新余市","","新余市人民医院","工业企业","8411|综合医院","水环境","废水排放口001(DW001)","国家标准","医疗机构水污染物排放标准(GB18466-2005)","（表2）综合医疗机构和其他医疗机构水污染物排放限值（日均值）,含氯消毒剂,消毒接触池的接触时间大于等于1小时，接触池出口,预处理标准","67","","32.7","五日生化需氧量（BOD5）","2024-07-24","3.4","mg/L","100","","是","否",""]
["2024","07","24","新余市","","新余市人民医院","工业企业","8411|综合医院","水环境","废水排放口001(DW001)","国家标准","医疗机构水污染物排放标准(GB18466-2005)","（表2）综合医疗机构和其他医疗机构水污染物排放限值（日均值）,含氯消毒剂,消毒接触池的接触时间大于等于1小时，接触池出口,预处理标准","67","","32.7","化学需氧量","2024-07-24","67","mg/L","250","","是","否",""]
["2024","07","24","新余市","","新余市人民医院","工业企业","8411|综合医院","水环境","废水排放口001(DW001)","国家标准","医疗机构水污染物排放标准(GB18466-2005)","（表2）综合医疗机构和其他医疗机构水污染物排放限值（日均值）,含氯消毒剂,消毒接触池的接触时间大于等于1小时，接触池出口,预处理标准","67","","32.7","悬浮物","2024-07-24","42","mg/L","60","","是","否",""]
["2024","07","24","新余市","","新余市人民医院","工业企业","8411|综合医院","水环境","废水排放口001(DW001)","国家标准","医疗机构水污染物排放标准(GB18466-2005)","（表2）综合医疗机构和其他医疗机构水污染物排放限值（日均值）,含氯消毒剂,消毒接触池的接触时间大于等于1小时，接触池出口,预处理标准","67","","32.7","pH值","2024-07-24","7.2","无量纲","9","6","是","否",""]
["2024","07","24","新余市","","新余市人民医院","工业企业","8411|综合医院","水环境","废水排放口001(DW001)","地方标准","城东污水处理厂接管标准(009)","城东污水处理厂接管标准","67","","32.7","氨氮","2024-07-24","33.6","mg/L","25","","是","是","0.34"]