{"text_format":"3","workbook":"xls","n_sheets":5,"sheets":["废气排放","废水排放","周边环境","噪声","无组织"],"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"废气排放","index":0,"n_rows":66,"n_cols":29,"rows_kept":66,"merged":[[0,0,0,28]],"flags":["formulas_cached_only"]}
["执法监测废气排放数据","","","","","","","","","","","","","","","","","","","","","","","","","","","",""]
["监测年","监测月","监测日","市","县","企业名称","企业类别","行业类别","名录类别","监测点名称","排放标准类型","排放标准名称","标准条目","废气生产负荷","废气流量","废气温度","废气湿度","废气含氧量","废气流速","监测项目名称","项目监测日期","废气实测结果","废气折算结果","取值单位","排放上限","排放下限","是否有评价限值","是否超标","超标倍数"]
["2024","06","06","新余市","渝水区","江西沃格光电股份有限公司（西城大道）","工业企业","3976|光电子器件制造","水环境,环境风险管控","废气监测点1(DA001)","国家标准","大气污染物综合排放标准(GB16297-1996)","（表2）新污染源大气污染物排放限值（1997年1月1日起）,最高允许排放浓度,除碳黑尘、燃料尘、玻璃棉尘、石英粉尘、矿渣棉尘外其他,排气筒20m,二级,5.9","61","18536","28","5","20.94","9.5","颗粒物","2024-06-06","<20","<20","mg/m3","120","","是","否",""]
["2024","06","06","新余市","渝水区","江西沃格光电股份有限公司（西城大道）","工业企业","3976|光电子器件制造","水环境,环境风险管控","废气监测点1(DA001)","国家标准","大气污染物综合排放标准(GB16297-1996)","（表2）新污染源大气污染物排放限值（1997年1月1日起）,最高允许排放浓度,除普钙工厂其他,排气筒20m,二级,0.17","61","18536","28","5","20.94","9.5","氟化物","2024-06-06","2.64","2.64","mg/m3","9.0","","是","否",""]
["2024","06","06","新余市","渝水区","江西沃格光电股份有限公司（西城大道）","工业企业","3976|光电子器件制造","水环境,环境风险管控","废气监测点4(DA004)","国家标准","大气污染物综合排放标准(GB16297-1996)","（表2）新污染源大气污染物排放限值（1997年1月1日起）,最高允许排放浓度,除火炸药厂其他,排气筒20m,二级,2.6","61","19020","23","8","20.92","4.7","硫酸雾","2024-06-06","<0.2","<0.2","mg/m3","45","","是","否",""]
["2024","06","06","新余市","渝水区","江西沃格光电股份有限公司（西城大道）","工业企业","3976|光电子器件制造","水环境,环境风险管控","废气监测点1(DA001)","国家标准","大气污染物综合排放标准(GB16297-1996)","（表2）新污染源大气污染物排放限值（1997年1月1日起）,最高允许排放浓度,除火炸药厂其他,排气筒20m,二级,2.6","61","18536","28","5","20.94","9.5","硫酸雾","2024-06-06","5.36","5.36","mg/m3","45","","是","否",""]
["2024","06","06","新余市","渝水区","江西沃格光电股份有限公司（西城大道）","工业企业","3976|光电子器件制造","水环境,环境风险管控","废气监测点1(DA001)","国家标准","大气污染物综合排放标准(GB16297-1996)","（表2）新污染源大气污染物排放限值（1997年1月1日起）,最高允许排放浓度,硝酸使用和其他,排气筒20m,二级,1.3","61","18536","28","5","20.94","9.5","氮氧化物","2024-06-06","<3","<3","mg/m3","240","","是","否",""]
["2024","06","06","新余市","渝水区","江西沃格光电股份有限公司（西城大道）","工业企业","3976|光电子器件制造","水环境,环境风险管控","废气监测点4(DA004)","国家标准","大气污染物综合排放标准(GB16297-1996)","（表2）新污染源大气污染物排放限值（1997年1月1日起）,最高允许排放浓度,通用,排气筒20m,二级,0.43","61","19020","23","8","20.92","4.7","氯化氢","2024-06-06","<0.2","<0.2","mg/m3","100","","是","否",""]
["2024","06","06","新余市","渝水区","江西沃格光电股份有限公司（西城大道）","工业企业","3976|光电子器件制造","水环境,环境风险管控","废气监测点2(DA002)","国家标准","大气污染物综合排放标准(GB16297-1996)","（表2）新污染源大气污染物排放限值（1997年1月1日起）,最高允许排放浓度,硝酸使用和其他,排气筒20m,二级,1.3","61","5459","27","5.5","20.95","2.8","氮氧化物","2024-06-06","<3","<3","mg/m3","240","","是","否",""]
["2024","06","06","新余市","渝水区","江西沃格光电股份有限公司（西城大道）","工业企业","3976|光电子器件制造","水环境,环境风险管控","废气监测点2(DA002)","国家标准","大气污染物综合排放标准(GB16297-1996)","（表2）新污染源大气污染物排放限值（1997年1月1日起）,最高允许排放浓度,除碳黑尘、燃料尘、玻璃棉尘、石英粉尘、矿渣棉尘外其他,排气筒20m,二级,5.9","61","5459","27","5.5","20.95","2.8","颗粒物","2024-06-06","<20","<20","mg/m3","120","","是","否",""]
["2024","06","06","新余市","渝水区","江西沃格光电股份有限公司（西城大道）","工业企业","3976|光电子器件制造","水环境,环境风险管控","废气监测点2(DA002)","国家标准","大气污染物综合排放标准(GB16297-1996)","（表2）新污染源大气污染物排放限值（1997年1月1日起）,最高允许排放浓度,除火炸药厂其他,排气筒20m,二级,2.6","61","5459","27","5.5","20.95","2.8","硫酸雾","2024-06-06","<0.2","<0.2","mg/m3","45","","是","否",""]
["2024","06","06","新余市","渝水区","江西沃格光电股份有限公司（西城大道）","工业企业","3976|光电子器件制造","水环境,环境风险管控","废气监测点1(DA001)","国家标准","大气污染物综合排放标准(GB16297-1996)","（表2）新污染源大气污染物排放限值（1997年1月1日起）,最高允许排放浓度,通用,排气筒20m,二级,0.43","61","18536","28","5","20.94","9.5","氯化氢","2024-06-06","1.21","1.21","mg/m3","100","","是","否",""]
["2024","06","06","新余市","渝水区","江西沃格光电股份有限公司（西城大道）","工业企业","3976|光电子器件制造","水环境,环境风险管控","废气监测点4(DA004)","国家标准","大气污染物综合排放标准(GB16297-1996)","（表2）新污染源大气污染物排放限值（1997年1月1日起）,最高允许排放浓度,除普钙工厂其他,排气筒20m,二级,0.17","61","19020","23","8","20.92","4.7","氟化物","2024-06-06","2.38","2.38","mg/m3","9.0","","是","否",""]
["2024","06","06","新余市","渝水区","江西沃格光电股份有限公司（西城大道）","工业企业","3976|光电子器件制造","水环境,环境风险管控","废气监测点4(DA004)","国家标准","大气污染物综合排放标准(GB16297-1996)","（表2）新污染源大气污染物排放限值（1997年1月1日起）,最高允许排放浓度,除碳黑尘、燃料尘、玻璃棉尘、石英粉尘、矿渣棉尘外其他,排气筒20m,二级,5.9","61","19020","23","8","20.92","4.7","颗粒物","2024-06-06","<20","<20","mg/m3","120","","是","否",""]
["2024","06","06","新余市","渝水区","江西沃格光电股份有限公司（西城大道）","工业企业","3976|光电子器件制造","水环境,环境风险管控","废气监测点2(DA002)","国家标准","大气污染物综合排放标准(GB16297-1996)","（表2）新污染源大气污染物排放限值（1997年1月1日起）,最高允许排放浓度,除普钙工厂其他,排气筒20m,二级,0.17","61","5459","27","5.5","20.95","2.8","氟化物","2024-06-06","1.94","1.94","mg/m3","9.0","","是","否",""]
["2024","06","06","新余市","渝水区","江西沃格光电股份有限公司（西城大道）","工业企业","3976|光电子器件制造","水环境,环境风险管控","废气监测点2(DA002)","国家标准","大气污染物综合排放标准(GB16297-1996)","（表2）新污染源大气污染物排放限值（1997年1月1日起）,最高允许排放浓度,通用,排气筒20m,二级,0.43","61","5459","27","5.5","20.95","2.8","氯化氢","2024-06-06","<0.2","<0.2","mg/m3","100","","是","否",""]
["2024","06","06","新余市","渝水区","江西沃格光电股份有限公司（西城大道）","工业企业","3976|光电子器件制造","水环境,环境风险管控","废气监测点4(DA004)","国家标准","大气污染物综合排放标准(GB16297-1996)","（表2）新污染源大气污染物排放限值（1997年1月1日起）,最高允许排放浓度,硝酸使用和其他,排气筒20m,二级,1.3","61","19020","23","8","20.92","4.7","氮氧化物","2024-06-06","<3","<3","mg/m3","240","","是","否",""]
["2024","06","20","新余市","渝水区","江西新钢南方新材料有限公司","工业企业","313|钢压延加工","水环境","CA2涂层段","国家标准","轧钢工业大气污染物排放标准(GB28665-2012)","（表1、表2）现有和新建企业有组织大气污染物排放浓度限值,涂镀层机组、酸洗机组","100","2569","30","5.8","","3","铬酸雾","2024-06-20","0.0516","0.0516","mg/m3","0.07","","是","否",""]
["2024","06","20","新余市","渝水区","江西新钢南方新材料有限公司","工业企业","313|钢压延加工","水环境","CA1连续退火线","国家标准","轧钢工业大气污染物排放标准(GB28665-2012)","（修改单）新建企业有组织大气污染物排放浓度限值,热处理炉,其他热处理炉","100","21084","201","2.3","10.66","9.2","二氧化硫","2024-06-20","<3","<3","mg/m3","100","","是","否",""]
["2024","06","20","新余市","渝水区","江西新钢南方新材料有限公司","工业企业","313|钢压延加工","水环境","CA1连续退火线","国家标准","轧钢工业大气污染物排放标准(GB28665-2012)","（表1、表2）现有和新建企业有组织大气污染物排放浓度限值,拉矫、精整、抛丸、修磨、焊接机及其他生产设施","100","22075","201","2.3","10.61","9.6","颗粒物","2024-06-20","5.1","2.9","mg/m3","20","","是","否",""]
["2024","06","20","新余市","渝水区","江西新钢南方新材料有限公司","工业企业","313|钢压延加工","水环境","CA1连续退火线","国家标准","轧钢工业大气污染物排放标准(GB28665-2012)","（修改单）新建企业有组织大气污染物排放浓度限值,热处理炉,其他热处理炉","100","21084","201","2.3","10.66","9.2","氮氧化物","2024-06-20","100","58","mg/m3","200","","是","否",""]
["2024","06","05","新余市","渝水区","新余超能通新能源有限公司","工业企业","3841|锂离子电池制造","环境风险管控","废气监测点1(DA001)","国家标准","电池工业污染物排放标准(GB30484-2013)","（表4）现有企业大气污染物排放限值,锂离子/锂电池直接排放限值","80","1848","38","3.5","","1.9","非甲烷总烃","2024-06-05","2.32","2.32","mg/m3","50","","是","否",""]
["2024","06","19","新余市","渝水区","新余益欣金属材料有限公司","工业企业","3360|金属表面处理及热处理加工","环境风险管控","酸洗废气排放口002(DA002)","国家标准","轧钢工业大气污染物排放标准(GB28665-2012)","（表1、表2）现有和新建企业有组织大气污染物排放浓度限值,酸洗机组","60","31616","43.9","3.5","","11.27","氯化氢","2024-06-19","1.67","1.67","mg/m3","20","","是","否",""]
["2024","06","19","新余市","渝水区","新余益欣金属材料有限公司","工业企业","3360|金属表面处理及热处理加工","环境风险管控","热浸镀锌废气排放口003(DA003)","国家标准","恶臭污染物排放标准(GB14554-93)","（表2）恶臭污染物排放标准值,排气筒高度15m","60","30476","69.6","3.7","","9.88","氨（氨气）","2024-06-19","0.48","0.48","kg/h","4.9","","是","否",""]
["2024","06","19","新余市","渝水区","新余益欣金属材料有限公司","工业企业","3360|金属表面处理及热处理加工","环境风险管控","热浸镀锌废气排放口003(DA003)","国家标准","轧钢工业大气污染物排放标准(GB28665-2012)","（表1、表2）现有和新建企业有组织大气污染物排放浓度限值,酸洗机组","60","30476","69.6","3.7","","9.88","氯化氢","2024-06-19","0.94","0.94","mg/m3","20","","是","否",""]
["2024","06","19","新余市","渝水区","新余益欣金属材料有限公司","工业企业","3360|金属表面处理及热处理加工","环境风险管控","热浸镀锌废气排放口003(DA003)","国家标准","轧钢工业大气污染物排放标准(GB28665-2012)","（表1、表2）现有和新建企业有组织大气污染物排放浓度限值,热处理炉","60","30476","69.6","3.7","","9.88","颗粒物","2024-06-19","1.7","1.7","mg/m3","20","","是","否",""]
["2024","06","24","新余市","","江西澳力特缸套有限公司","工业企业","367|汽车零部件及配件制造","水环境,土壤污染监管","废气排放口","国家标准","电镀污染物排放标准(GB21900-2008)","（表4、表5）现有和新建企业大气污染排放限值,排气筒高度达到高出周围200m半径范围的建筑5m以上的要求","15","3969","26","5.6","","2.6","铬酸雾","2024-06-24","0.0415","0.0415","mg/m3","0.05","","是","否",""]
["2024","06","24","新余市","","江西澳力特缸套有限公司","工业企业","367|汽车零部件及配件制造","水环境,土壤污染监管","废气排放口","国家标准","电镀污染物排放标准(GB21900-2008)","（表4、表5）现有和新建企业大气污染排放限值,排气筒高度达到高出周围200m半径范围的建筑5m以上的要求","15","3969","26","5.6","","2.6","氯化氢","2024-06-24","6.96","6.96","mg/m3","30","","是","否",""]
["2024","06","26","新余市","","江西路达新能源科技有限公司","工业企业","3099|其他非金属矿物制品制造","大气环境","反应釜废气排口(DA002)","国家标准","大气污染物综合排放标准(GB16297-1996)","（表2）新污染源大气污染物排放限值（1997年1月1日起）,最高允许排放浓度,沥青及碳素制品生产和加工,排气筒15m,二级,0.000050","52.5","3985","14.9","2.61","","6.1","苯并(a)芘","2024-06-26","0.00019","0.00019","mg/m3","0.0003","","是","否",""]
["2024","06","26","新余市","","江西路达新能源科技有限公司","工业企业","3099|其他非金属矿物制品制造","大气环境","反应釜废气排口(DA002)","国家标准","工业炉窑大气污染物排放标准(GB9078-1996)","（表4）各种工业炉窑有害污染物最高排放浓度,1997年1月1日起新、改、扩建的工业炉窑,标准级别二","52.5","3502","14.9","2.75","","5.4","沥青烟","2024-06-26","<12.8","<12.8","mg/m3","50","","是","否",""]
["2024","06","26","新余市","","江西人和铜业有限公司黄铜棒生产厂","工业企业","3240|有色金属合金制造","大气环境","熔化废气排放口(DA001)","国家标准","大气污染物综合排放标准(GB16297-1996)","（表2）新污染源大气污染物排放限值（1997年1月1日起）,最高允许排放浓度,其他","100","53995","48.9","3.4","","12","颗粒物","2024-06-26","1.5","1.5","mg/m3","120","","是","否",""]
["2024","06","26","新余市","","江西人和铜业有限公司黄铜棒生产厂","工业企业","3240|有色金属合金制造","大气环境","熔化废气排放口(DA001)","国家标准","大气污染物综合排放标准(GB16297-1996)","（表2）新污染源大气污染物排放限值（1997年1月1日起）,最高允许排放浓度,通用,排气筒15m,二级,0.31","100","54744","50.6","3.4","","12.2","锡及其化合物","2024-06-26","0.00638","0.00638","mg/m3","8.5","","是","否",""]
["2024","05","24","新余市","","江西新钢环保科技有限公司","工业企业","42|废弃资源综合利用业","大气环境,土壤污染监管","5#排放口004(DA004)","国家标准","钢铁烧结、球团工业大气污染物排放标准(GB28662-2012)","（表2）新建企业大气污染物排放浓度限值,烧结机球团焙烧设备","81","51612","141","6.97","10","3","二噁英类","2024-05-24","0.16","0.044","ng-TEQ/m3","0.5","","是","否",""]
["2024","06","12","新余市","","江西新华新材料科技股份有限公司","工业企业","3340|金属丝绳及其制品制造","环境风险管控","镀锌烟气排放口(DA004)","国家标准","轧钢工业大气污染物排放标准(GB28665-2012)","（表1、表2）现有和新建企业有组织大气污染物排放浓度限值,热处理炉","82","4327","43.7","4.8","","5.28","颗粒物","2024-06-12","18.2","18.2","mg/m3","20","","是","否",""]
["2024","06","12","新余市","","江西新华新材料科技股份有限公司","工业企业","3340|金属丝绳及其制品制造","环境风险管控","酸雾吸收塔排放口(DA005)","国家标准","轧钢工业大气污染物排放标准(GB28665-2012)","（表1、表2）现有和新建企业有组织大气污染物排放浓度限值,酸洗机组","82","1919","40.3","7","","5.3","氯化氢","2024-06-12","4.13","4.13","mg/m3","20","","是","否",""]
["2024","06","12","新余市","","江西新华新材料科技股份有限公司","工业企业","3340|金属丝绳及其制品制造","环境风险管控","镀锌烟气排放口(DA004)","国家标准","恶臭污染物排放标准(GB14554-93)","（表2）恶臭污染物排放标准值,排气筒高度15m","82","4327","43.7","4.8","","5.28","氨（氨气）","2024-06-12","0.061","0.061","kg/h","4.9","","是","否",""]
["2024","06","12","新余市","","江西新华新材料科技股份有限公司","工业企业","3340|金属丝绳及其制品制造","环境风险管控","磷化烘干废气排放塔(DA003)","国家标准","轧钢工业大气污染物排放标准(GB28665-2012)","（表1、表2）现有和新建企业有组织大气污染物排放浓度限值,热处理炉","82","8956","33.5","4.9","","5.92","颗粒物","2024-06-12","3.4","3.4","mg/m3","20","","是","否",""]
["2024","06","13","新余市","","江西新华新材料科技股份有限公司","工业企业","3340|金属丝绳及其制品制造","环境风险管控","燃烧锅炉烟气排放口(DA001)","国家标准","锅炉大气污染物排放标准(GB13271-2014)","（表2）新建锅炉大气污染物排放浓度限值（2014年7月1日起新建锅炉）,烟囱或烟道,燃气锅炉","82","1635","154.2","13.3","3.8","4.23","颗粒物","2024-06-13","2.2","2.2","mg/m3","20","","是","否",""]
["2024","06","13","新余市","","江西新华新材料科技股份有限公司","工业企业","3340|金属丝绳及其制品制造","环境风险管控","燃烧锅炉烟气排放口(DA001)","国家标准","锅炉大气污染物排放标准(GB13271-2014)","（表2）新建锅炉大气污染物排放浓度限值（2014年7月1日起新建锅炉）,烟囱排放口,燃气锅炉","82","1635","154.2","13.3","3.8","4.23","林格曼黑度","2024-06-13","<1","<1","mg/m3","1","","是","否",""]
["2024","06","13","新余市","","江西新华新材料科技股份有限公司","工业企业","3340|金属丝绳及其制品制造","环境风险管控","燃烧锅炉烟气排放口(DA001)","国家标准","锅炉大气污染物排放标准(GB13271-2014)","（表2）新建锅炉大气污染物排放浓度限值（2014年7月1日起新建锅炉）,烟囱或烟道,燃气锅炉","82","1635","154.2","13.3","3.8","4.23","二氧化硫","2024-06-13","<3","<3","mg/m3","50","","是","否",""]
["2024","06","13","新余市","","江西新华新材料科技股份有限公司","工业企业","3340|金属丝绳及其制品制造","环境风险管控","燃烧锅炉烟气排放口(DA001)","国家标准","锅炉大气污染物排放标准(GB13271-2014)","（表2）新建锅炉大气污染物排放浓度限值（2014年7月1日起新建锅炉）,烟囱或烟道,燃气锅炉","82","1635","154.2","13.3","3.8","4.23","氮氧化物","2024-06-13","85","87","mg/m3","200","","是","否",""]
["2024","06","13","新余市","","江西新华新材料科技股份有限公司","工业企业","3340|金属丝绳及其制品制造","环境风险管控","酸雾塔排放口(DA002)","国家标准","轧钢工业大气污染物排放标准(GB28665-2012)","（表1、表2）现有和新建企业有组织大气污染物排放浓度限值,酸洗机组","82","14646","25.8","7.2","","9.69","氯化氢","2024-06-13","1.46","1.46","mg/m3","20","","是","否",""]
["2024","06","18","新余市","","江西增鑫科技股份有限公司","工业企业","3574|畜牧机械制造","环境风险管控","镀锌排口2(DA014)","国家标准","轧钢工业大气污染物排放标准(GB28665-2012)","（表1、表2）现有和新建企业有组织大气污染物排放浓度限值,拉矫、精整、抛丸、修磨、焊接机及其他生产设施","80","35998","40.9","3.3","","9.06","颗粒物","2024-06-18","1.5","1.5","mg/m3","20","","是","否",""]
["2024","06","18","新余市","","江西增鑫科技股份有限公司","工业企业","3574|畜牧机械制造","环境风险管控","镀锌排口2(DA014)","国家标准","恶臭污染物排放标准(GB14554-93)","（表2）恶臭污染物排放标准值,排气筒高度15m","80","35998","40.9","3.3","","9.06","氨（氨气）","2024-06-18","0.39","0.39","kg/h","4.9","","是","否",""]
["2024","06","18","新余市","","江西增鑫科技股份有限公司","工业企业","3574|畜牧机械制造","环境风险管控","燃气排口2(DA011)","国家标准","轧钢工业大气污染物排放标准(GB28665-2012)","（表1、表2）现有和新建企业有组织大气污染物排放浓度限值,热处理炉","80","2678","318.6","12.3","5.9","11.71","二氧化硫","2024-06-18","<3","<3","mg/m3","150","","是","否",""]
["2024","06","18","新余市","","江西增鑫科技股份有限公司","工业企业","3574|畜牧机械制造","环境风险管控","燃气排口2(DA011)","国家标准","轧钢工业大气污染物排放标准(GB28665-2012)","（表1、表2）现有和新建企业有组织大气污染物排放浓度限值,热处理炉","80","2678","318.6","12.3","5.9","11.71","颗粒物","2024-06-18","2.7","2.7","mg/m3","20","","是","否",""]
["2024","06","18","新余市","","江西增鑫科技股份有限公司","工业企业","3574|畜牧机械制造","环境风险管控","酸雾吸收塔A (DA005)","国家标准","轧钢工业大气污染物排放标准(GB28665-2012)","（表1、表2）现有和新建企业有组织大气污染物排放浓度限值,酸洗机组","80","65774","32.8","3.4","","16.19","氯化氢","2024-06-18","1.71","1.71","mg/m3","20","","是","否",""]
["2024","06","18","新余市","","江西增鑫科技股份有限公司","工业企业","3574|畜牧机械制造","环境风险管控","燃气排口2(DA011)","国家标准","轧钢工业大气污染物排放标准(GB28665-2012)","（表3）大气污染物特别排放限值,热处理炉","80","2678","318.6","12.3","5.9","11.71","氮氧化物","2024-06-18","47","48","mg/m3","300","","是","否",""]
["2024","06","07","新余市","","新余钢铁股份有限公司","工业企业","3120|炼钢","水环境,大气环境,土壤污染监管","烧结厂7#烧结机(DA047)","国家标准","钢铁烧结、球团工业大气污染物排放标准(GB28662-2012)","（表2）新建企业大气污染物排放浓度限值,烧结机球团焙烧设备","100","1057686","117.5","16.41","15.8","18","二噁英类","2024-06-07","0.41","0.39","ng-TEQ/m3","0.5","","是","否",""]
["2024","06","25","新余市","","新余景耀新材料有限公司","工业企业","3130|钢压延加工","环境风险管控","轧机油雾排气筒2#(DA003)","国家标准","轧钢工业大气污染物排放标准(GB28665-2012)","（表1、表2）现有和新建企业有组织大气污染物排放浓度限值,轧制机组","90.9","1417","17.9","4.1","","4.6","油雾","2024-06-25","0.3","0.3","mg/m3","30","","是","否",""]
["2024","06","21","新余市","","新余市郁海环保科技有限公司","工业企业","7724|危险废物治理","环境风险管控","酸雾废气排放口001(DA001)","国家标准","大气污染物综合排放标准(GB16297-1996)","（表2）新污染源大气污染物排放限值（1997年1月1日起）,最高允许排放浓度,除火炸药厂其他,排气筒15m,二级,1.5","9","369","29.3","4.9","","1.94","硫酸雾","2024-06-21","2.55","2.55","mg/m3","45","","是","否",""]
["2024","06","13","新余市","","新余新钢金属制品有限公司","工业企业","3340|金属丝绳及其制品制造","环境风险管控","钢丝厂1号热处理炉烟气排放口(DA003)","国家标准","轧钢工业大气污染物排放标准(GB28665-2012)","（表1、表2）现有和新建企业有组织大气污染物排放浓度限值,热处理炉","82.1","4616","187.4","5.7","17.9","6.06","氮氧化物","2024-06-13","11","44","mg/m3","300","","是","否",""]
["2024","06","13","新余市","","新余新钢金属制品有限公司","工业企业","3340|金属丝绳及其制品制造","环境风险管控","钢丝厂1号热处理炉烟气排放口(DA003)","国家标准","轧钢工业大气污染物排放标准(GB28665-2012)","（表1、表2）现有和新建企业有组织大气污染物排放浓度限值,热处理炉","82.1","4616","187.4","5.7","17.9","6.06","二氧化硫","2024-06-13","<3","<12","mg/m3","150","","是","否",""]
["2024","06","13","新余市","","新余新钢金属制品有限公司","工业企业","3340|金属丝绳及其制品制造","环境风险管控","钢丝厂1号热处理炉烟气排放口(DA003)","国家标准","轧钢工业大气污染物排放标准(GB28665-2012)","（表1、表2）现有和新建企业有组织大气污染物排放浓度限值,热处理炉","82.1","4616","187.4","5.7","17.9","6.06","颗粒物","2024-06-13","3.5","14.4","mg/m3","20","","是","否",""]
["2024","06","14","新余市","","新余新钢金属制品有限公司","工业企业","3340|金属丝绳及其制品制造","环境风险管控","钢丝厂2号热处理炉烟气排放口(DA004)","国家标准","轧钢工业大气污染物排放标准(GB28665-2012)","（表1、表2）现有和新建企业有组织大气污染物排放浓度限值,热处理炉","82.1","1210","328.7","5.9","8.2","6.37","颗粒物","2024-06-14","2.5","2.7","mg/m3","20","","是","否",""]
["2024","06","14","新余市","","新余新钢金属制品有限公司","工业企业","3340|金属丝绳及其制品制造","环境风险管控","钢丝厂2号热处理炉烟气排放口(DA004)","国家标准","轧钢工业大气污染物排放标准(GB28665-2012)","（表1、表2）现有和新建企业有组织大气污染物排放浓度限值,热处理炉","82.1","1210","328.7","5.9","8.2","6.37","氮氧化物","2024-06-14","106","109","mg/m3","300","","是","否",""]
["2024","06","14","新余市","","新余新钢金属制品有限公司","工业企业","3340|金属丝绳及其制品制造","环境风险管控","钢丝厂2号热处理炉烟气排放口(DA004)","国家标准","轧钢工业大气污染物排放标准(GB28665-2012)","（表1、表2）现有和新建企业有组织大气污染物排放浓度限值,热处理炉","82.1","1210","328.7","5.9","8.2","6.37","二氧化硫","2024-06-14","<3","<3","mg/m3","150","","是","否",""]
["2024","06","14","新余市","","新余新钢金属制品有限公司","工业企业","3340|金属丝绳及其制品制造","环境风险管控","酸雾吸收塔排放口(DA001)","国家标准","轧钢工业大气污染物排放标准(GB28665-2012)","（表1、表2）现有和新建企业有组织大气污染物排放浓度限值,酸洗机组","82.1","19131","27.8","7.1","","12.75","氯化氢","2024-06-14","2.04","2.04","mg/m3","20","","是","否",""]
["2024","06","17","新余市","","新余新钢金属制品有限公司","工业企业","3340|金属丝绳及其制品制造","环境风险管控","磷化烘干废气排放口(DA002)","国家标准","轧钢工业大气污染物排放标准(GB28665-2012)","（表1、表2）现有和新建企业有组织大气污染物排放浓度限值,热处理炉","82.1","1788","54.5","6.2","","5.11","二氧化硫","2024-06-17","<3","<3","mg/m3","150","","是","否",""]
["2024","06","17","新余市","","新余新钢金属制品有限公司","工业企业","3340|金属丝绳及其制品制造","环境风险管控","酸雾吸收塔2号排放口(DA008)","国家标准","轧钢工业大气污染物排放标准(GB28665-2012)","（表1、表2）现有和新建企业有组织大气污染物排放浓度限值,酸洗机组","82.1","15639","28.9","7.3","","13.61","氯化氢","2024-06-17","3.07","3.07","mg/m3","20","","是","否",""]
["2024","06","17","新余市","","新余新钢金属制品有限公司","工业企业","3340|金属丝绳及其制品制造","环境风险管控","磷化烘干废气排放口(DA002)","国家标准","轧钢工业大气污染物排放标准(GB28665-2012)","（表1、表2）现有和新建企业有组织大气污染物排放浓度限值,热处理炉","82.1","1788","54.5","6.2","","5.11","颗粒物","2024-06-17","1.7","1.7","mg/m3","20","","是","否",""]
["2024","06","17","新余市","","新余新钢金属制品有限公司","工业企业","3340|金属丝绳及其制品制造","环境风险管控","磷化烘干废气排放口(DA002)","国家标准","轧钢工业大气污染物排放标准(GB28665-2012)","（表3）大气污染物特别排放限值,热处理炉","82.1","1788","54.5","6.2","","5.11","氮氧化物","2024-06-17","<3","<3","mg/m3","300","","是","否",""]
["2024","06","17","新余市","","新余新钢金属制品有限公司","工业企业","3340|金属丝绳及其制品制造","环境风险管控","燃烧锅炉烟气排放口(DA007)","国家标准","锅炉大气污染物排放标准(GB13271-2014)","（表3）大气污染物特别排放限值,烟囱或烟道,燃气锅炉","82.1","2116","118.6","14.4","4.5","5.08","二氧化硫","2024-06-17","<3","<3","mg/m3","50","","是","否",""]
["2024","06","17","新余市","","新余新钢金属制品有限公司","工业企业","3340|金属丝绳及其制品制造","环境风险管控","燃烧锅炉烟气排放口(DA007)","国家标准","锅炉大气污染物排放标准(GB13271-2014)","（表2）新建锅炉大气污染物排放浓度限值（2014年7月1日起新建锅炉）,烟囱或烟道,燃气锅炉","82.1","2116","118.6","14.4","4.5","5.08","颗粒物","2024-06-17","1.9","2.0","mg/m3","20","","是","否",""]
["2024","06","17","新余市","","新余新钢金属制品有限公司","工业企业","3340|金属丝绳及其制品制造","环境风险管控","燃烧锅炉烟气排放口(DA007)","国家标准","锅炉大气污染物排放标准(GB13271-2014)","（表2）新建锅炉大气污染物排放浓度限值（2014年7月1日起新建锅炉）,烟囱排放口,燃气锅炉","82.1","2116","118.6","14.4","4.5","5.08","林格曼黑度","2024-06-17","<1","<1","级","1","","是","否",""]
["2024","06","17","新余市","","新余新钢金属制品有限公司","工业企业","3340|金属丝绳及其制品制造","环境风险管控","燃烧锅炉烟气排放口(DA007)","国家标准","锅炉大气污染物排放标准(GB13271-2014)","（表2）新建锅炉大气污染物排放浓度限值（2014年7月1日起新建锅炉）,烟囱或烟道,燃气锅炉","82.1","2116","118.6","14.4","4.5","5.08","氮氧化物","2024-06-17","122","130","mg/m3","200","","是","否",""]

{"sheet":"废水排放","index":1,"n_rows":175,"n_cols":25,"rows_kept":175,"merged":[[0,0,0,24]],"flags":["formulas_cached_only"]}
["执法监测废水排放数据",null,"","","","","","","","","","","","","","","","","","","","","","",""]
["监测年","监测月","监测日","市","县","企业名称","企业类别","行业类别","名录类别","监测点名称","排放标准类型","排放标准名称","标准条目","废水工作负荷","废水流量","废水水温","监测项目","项目监测日期","排放浓度","取值单位","排放上限","排放下限","是否有评价限值","是否超标","超标倍数"]
["2024","06","03","新余市","渝水区","江西省华赣环境集团新余生态环境产业有限公司","工业企业","7723|固体废物治理","水环境","废水总排放口(DW002)","地方标准","新余鑫远水务有限公司（新余城西污水处理厂）纳管标准(DBxysw)","新余鑫远水务有限公司（新余城西污水处理厂）纳管标准","80","","14.3","氰化物","2024-06-03","<0.001","mg/L","0.5","","是","否",""]
["2024","06","03","新余市","渝水区","江西省华赣环境集团新余生态环境产业有限公司","工业企业","7723|固体废物治理","水环境","废水总排放口(DW002)","国家标准","污水综合排放标准(GB8978-1996)","（表2）第二类污染物最高允许排放浓度（1997年12月31日之前建的单位）,其他排污单位,一级标准","80","","14.3","氟化物","2024-06-03","0.45","mg/L","10","","是","否",""]
["2024","06","03","新余市","渝水区","江西省华赣环境集团新余生态环境产业有限公司","工业企业","7723|固体废物治理","水环境","车间排放口(DW001)","国家标准","污水综合排放标准(GB8978-1996)","（表1）第一类污染物最高允许排放浓度","80","","14.7","总汞","2024-06-03","0.00045","mg/L","0.05","","是","否",""]
["2024","06","03","新余市","渝水区","江西省华赣环境集团新余生态环境产业有限公司","工业企业","7723|固体废物治理","水环境","废水总排放口(DW002)","地方标准","新余鑫远水务有限公司（新余城西污水处理厂）纳管标准(DBxysw)","新余鑫远水务有限公司（新余城西污水处理厂）纳管标准","80","","14.3","总氮（以N计）","2024-06-03","1.26","mg/L","35","","是","否",""]
["2024","06","03","新余市","渝水区","江西省华赣环境集团新余生态环境产业有限公司","工业企业","7723|固体废物治理","水环境","废水总排放口(DW002)","地方标准","新余鑫远水务有限公司（新余城西污水处理厂）纳管标准(DBxysw)","新余鑫远水务有限公司（新余城西污水处理厂）纳管标准","80","","14.3","总磷（以P计）","2024-06-03","0.03","mg/L","3.5","","是","否",""]
["2024","06","03","新余市","渝水区","江西省华赣环境集团新余生态环境产业有限公司","工业企业","7723|固体废物治理","水环境","车间排放口(DW001)","国家标准","污水综合排放标准(GB8978-1996)","（表1）第一类污染物最高允许排放浓度","80","","14.7","总镉","2024-06-03","0.0130","mg/L","0.1","","是","否",""]
["2024","06","03","新余市","渝水区","江西省华赣环境集团新余生态环境产业有限公司","工业企业","7723|固体废物治理","水环境","废水总排放口(DW002)","国家标准","污水综合排放标准(GB8978-1996)","（表1）第一类污染物最高允许排放浓度","80","","14.3","总镍","2024-06-03","<0.05","mg/L","1.0","","是","否",""]
["2024","06","03","新余市","渝水区","江西省华赣环境集团新余生态环境产业有限公司","工业企业","7723|固体废物治理","水环境","车间排放口(DW001)","国家标准","污水综合排放标准(GB8978-1996)","（表1）第一类污染物最高允许排放浓度","80","","14.7","总铅","2024-06-03","0.140","mg/L","1.0","","是","否",""]
["2024","06","03","新余市","渝水区","江西省华赣环境集团新余生态环境产业有限公司","工业企业","7723|固体废物治理","水环境","车间排放口(DW001)","国家标准","污水综合排放标准(GB8978-1996)","（表1）第一类污染物最高允许排放浓度","80","","14.7","六价铬","2024-06-03","0.021","mg/L","0.5","","是","否",""]
["2024","06","03","新余市","渝水区","江西省华赣环境集团新余生态环境产业有限公司","工业企业","7723|固体废物治理","水环境","废水总排放口(DW002)","地方标准","新余鑫远水务有限公司（新余城西污水处理厂）纳管标准(DBxysw)","新余鑫远水务有限公司（新余城西污水处理厂）纳管标准","80","","14.3","五日生化需氧量","2024-06-03","2.2","mg/L","130","","是","否",""]
["2024","06","03","新余市","渝水区","江西省华赣环境集团新余生态环境产业有限公司","工业企业","7723|固体废物治理","水环境","废水总排放口(DW002)","国家标准","污水综合排放标准(GB8978-1996)","（表2）第二类污染物最高允许排放浓度（1997年12月31日之前建的单位）,其他排污单位,二级标准","80","","14.3","pH值","2024-06-03","6.8","无量纲","9","6","是","否",""]
["2024","06","03","新余市","渝水区","江西省华赣环境集团新余生态环境产业有限公司","工业企业","7723|固体废物治理","水环境","废水总排放口(DW002)","地方标准","新余鑫远水务有限公司（新余城西污水处理厂）纳管标准(DBxysw)","新余鑫远水务有限公司（新余城西污水处理厂）纳管标准","80","","14.3","化学需氧量","2024-06-03","11","mg/L","350","","是","否",""]
["2024","06","03","新余市","渝水区","江西省华赣环境集团新余生态环境产业有限公司","工业企业","7723|固体废物治理","水环境","废水总排放口(DW002)","国家标准","污水综合排放标准(GB8978-1996)","（表2）第二类污染物最高允许排放浓度（1997年12月31日之前建的单位）,一切排污单位 ,一级标准","80","","14.3","总铜","2024-06-03","<0.05","mg/L","0.5","","是","否",""]
["2024","06","03","新余市","渝水区","江西省华赣环境集团新余生态环境产业有限公司","工业企业","7723|固体废物治理","水环境","废水总排放口(DW002)","地方标准","新余鑫远水务有限公司（新余城西污水处理厂）纳管标准(DBxysw)","新余鑫远水务有限公司（新余城西污水处理厂）纳管标准","80","","14.3","氨氮（NH3-N）","2024-06-03","0.389","mg/L","30","","是","否",""]
["2024","06","03","新余市","渝水区","江西省华赣环境集团新余生态环境产业有限公司","工业企业","7723|固体废物治理","水环境","废水总排放口(DW002)","国家标准","污水综合排放标准(GB8978-1996)","（表2）第二类污染物最高允许排放浓度（1997年12月31日之前建的单位）,其他排污单位,一级标准","80","","14.3","悬浮物","2024-06-03","25","mg/L","260","","是","否",""]
["2024","06","03","新余市","渝水区","江西省华赣环境集团新余生态环境产业有限公司","工业企业","7723|固体废物治理","水环境","车间排放口(DW001)","国家标准","污水综合排放标准(GB8978-1996)","（表1）第一类污染物最高允许排放浓度","80","","14.7","总砷","2024-06-03","0.0166","mg/L","0.5","","是","否",""]
["2024","06","03","新余市","渝水区","江西省华赣环境集团新余生态环境产业有限公司","工业企业","7723|固体废物治理","水环境","车间排放口(DW001)","国家标准","污水综合排放标准(GB8978-1996)","（表1）第一类污染物最高允许排放浓度","80","","14.7","总铬","2024-06-03","0.034","mg/L","1.5","","是","否",""]
["2024","06","03","新余市","渝水区","江西省华赣环境集团新余生态环境产业有限公司","工业企业","7723|固体废物治理","水环境","废水总排放口(DW002)","国家标准","污水综合排放标准(GB8978-1996)","（表4）第二类污染物最高允许排放浓度（1998年1月1日后建的单位）,一切排污单位 ,一级标准","80","","14.3","总锌","2024-06-03","<0.05","mg/L","2.0","","是","否",""]
["2024","06","03","新余市","渝水区","江西省华赣环境集团新余生态环境产业有限公司","工业企业","7723|固体废物治理","水环境","废水总排放口(DW002)","国家标准","污水综合排放标准(GB8978-1996)","（表2）第二类污染物最高允许排放浓度（1997年12月31日之前建的单位）,其他排污单位,二级标准","80","","14.3","石油类","2024-06-03","0.76","mg/L","10","","是","否",""]
["2024","06","06","新余市","渝水区","江西沃格光电股份有限公司（西城大道）","工业企业","3976|光电子器件制造","水环境,环境风险管控","废水监测点1","地方标准","新余高新区污水处理厂接管标准(001)","污水处理厂接管进水限值","42","","22","化学需氧量","2024-06-06","28","mg/L","500","","是","否",""]
["2024","06","06","新余市","渝水区","江西沃格光电股份有限公司（西城大道）","工业企业","3976|光电子器件制造","水环境,环境风险管控","废水监测点1","地方标准","新余高新区污水处理厂接管标准(001)","污水处理厂接管进水限值","42","","22","悬浮物","2024-06-06","12","mg/L","300","","是","否",""]
["2024","06","06","新余市","渝水区","江西沃格光电股份有限公司（西城大道）","工业企业","3976|光电子器件制造","水环境,环境风险管控","废水监测点1","国家标准","污水综合排放标准(GB8978-1996)","（表4）第二类污染物最高允许排放浓度（1998年1月1日后建的单位）,其他排污单位,一级标准","42","","22","氟化物","2024-06-06","0.730","mg/L","10","","是","否",""]
["2024","06","06","新余市","渝水区","江西沃格光电股份有限公司（西城大道）","工业企业","3976|光电子器件制造","水环境,环境风险管控","废水监测点1","地方标准","新余高新区污水处理厂接管标准(001)","污水处理厂接管进水限值","42","","22","pH值","2024-06-06","7.4","无量纲","9","","是","否",""]
["2024","06","06","新余市","渝水区","江西沃格光电股份有限公司（西城大道）","工业企业","3976|光电子器件制造","水环境,环境风险管控","废水监测点1","地方标准","新余高新区污水处理厂接管标准(001)","污水处理厂接管进水限值","42","","22","五日生化需氧量（BOD5）","2024-06-06","1.4","mg/L","250","","是","否",""]
["2024","06","06","新余市","渝水区","江西沃格光电股份有限公司（西城大道）","工业企业","3976|光电子器件制造","水环境,环境风险管控","废水监测点1","地方标准","新余高新区污水处理厂接管标准(001)","污水处理厂接管进水限值","42","","22","总氮（以N计）","2024-06-06","1.80","mg/L","50","","是","否",""]
["2024","06","06","新余市","渝水区","江西沃格光电股份有限公司（西城大道）","工业企业","3976|光电子器件制造","水环境,环境风险管控","废水监测点1","国家标准","污水综合排放标准(GB8978-1996)","（表4）第二类污染物最高允许排放浓度（1998年1月1日后建的单位）,一切排污单位 ,一级标准","42","","22","阴离子表面活性剂（LAS）","2024-06-06","0.08","mg/L","5.0","","是","否",""]
["2024","06","06","新余市","渝水区","江西沃格光电股份有限公司（西城大道）","工业企业","3976|光电子器件制造","水环境,环境风险管控","废水监测点1","地方标准","新余高新区污水处理厂接管标准(001)","污水处理厂接管进水限值","42","","22","氨氮（NH3-N）","2024-06-06","0.539","mg/L","35","","是","否",""]
["2024","06","06","新余市","渝水区","江西沃格光电股份有限公司（西城大道）","工业企业","3976|光电子器件制造","水环境,环境风险管控","废水监测点1","地方标准","新余高新区污水处理厂接管标准(001)","污水处理厂接管进水限值","42","","22","总磷（以P计）","2024-06-06","0.04","mg/L","7","","是","否",""]
["2024","06","19","新余市","渝水区","江西新余国科科技股份有限公司","工业企业","2671|炸药及火工产品制造","水环境","总排口","地方标准","污水综合排放标准(GB8978-1996)","表4第二类污染物最高允许排放浓度,一级标准","33.3","","23.8","五日生化需氧量（BOD5）","2024-06-19","0.8","mg/L","20","","是","否",""]
["2024","06","19","新余市","渝水区","江西新余国科科技股份有限公司","工业企业","2671|炸药及火工产品制造","水环境","总排口","地方标准","污水综合排放标准(GB8978-1996)","表4第二类污染物最高允许排放浓度,一级标准","33.3","","23.8","悬浮物","2024-06-19","10","mg/L","70","","是","否",""]
["2024","06","19","新余市","渝水区","江西新余国科科技股份有限公司","工业企业","2671|炸药及火工产品制造","水环境","总排口","地方标准","污水综合排放标准(GB8978-1996)","表4第二类污染物最高允许排放浓度,一级标准","33.3","","23.8","化学需氧量","2024-06-19","12","mg/L","100","","是","否",""]
["2024","06","19","新余市","渝水区","江西新余国科科技股份有限公司","工业企业","2671|炸药及火工产品制造","水环境","总排口","地方标准","污水综合排放标准(GB8978-1996)","表4第二类污染物最高允许排放浓度,一级标准","33.3","","23.8","pH值","2024-06-19","7.2","无量纲","9","6","是","否",""]
["2024","06","19","新余市","渝水区","江西新余国科科技股份有限公司","工业企业","2671|炸药及火工产品制造","水环境","表面处理车间","","","","50","","","锑","2024-06-19","<0.00015","mg/L","","","否","",""]
["2024","06","19","新余市","渝水区","江西新余国科科技股份有限公司","工业企业","2671|炸药及火工产品制造","水环境","总排口","地方标准","污水综合排放标准(GB8978-1996)","表4第二类污染物最高允许排放浓度,一级标准","33.3","","23.8","总铜","2024-06-19","0.0927","mg/L","0.5","","是","否",""]
["2024","06","19","新余市","渝水区","江西新余国科科技股份有限公司","工业企业","2671|炸药及火工产品制造","水环境","表面处理车间","地方标准","污水综合排放标准(GB8978-1996)","表1第一类污染物最高允许排放浓度,最高允许排放浓度","50","","","总铬","2024-06-19","0.182","mg/L","1.5","","是","否",""]
["2024","06","19","新余市","渝水区","江西新余国科科技股份有限公司","工业企业","2671|炸药及火工产品制造","水环境","总排口","地方标准","污水综合排放标准(GB8978-1996)","表4第二类污染物最高允许排放浓度,一级标准","33.3","","23.8","氨氮（NH3-N）","2024-06-19","0.171","mg/L","15","","是","否",""]
["2024","06","19","新余市","渝水区","江西新余国科科技股份有限公司","工业企业","2671|炸药及火工产品制造","水环境","总排口","国家标准","兵器工业水污染物排放标准火工药剂(GB14470.2-2002)","（表2）2003年7月1日起建设的火工药剂生产企业及其新、改、扩建项目水污染物最高允许日均排放浓度,三硝基间苯二酚铅","33.3","","23.8","硝基酚类","2024-06-19","<0.07","mg/L","3.0","","是","否",""]
["2024","06","19","新余市","渝水区","江西新余国科科技股份有限公司","工业企业","2671|炸药及火工产品制造","水环境","表面处理车间","地方标准","污水综合排放标准(GB8978-1996)","表1第一类污染物最高允许排放浓度,最高允许排放浓度","50","","","六价铬","2024-06-19","0.156","mg/L","0.5","","是","否",""]
["2024","06","19","新余市","渝水区","江西新余国科科技股份有限公司","工业企业","2671|炸药及火工产品制造","水环境","总排口","地方标准","污水综合排放标准(GB8978-1996)","表4第二类污染物最高允许排放浓度,一级标准","33.3","","23.8","石油类","2024-06-19","<0.06","mg/L","5","","是","否",""]
["2024","06","19","新余市","渝水区","江西新余国科科技股份有限公司","工业企业","2671|炸药及火工产品制造","水环境","表面处理车间","地方标准","江西省地方标准《工业废水铊污染物排放标准》[地标][地标](DB36/1149——2019)","工业废水铊污染物排放","50","","","铊","2024-06-19","0.00003","mg/L","0.005","","是","否",""]
["2024","06","19","新余市","渝水区","江西新余国科科技股份有限公司","工业企业","2671|炸药及火工产品制造","水环境","总排口","地方标准","污水综合排放标准(GB8978-1996)","表4第二类污染物最高允许排放浓度,一级标准","33.3","","23.8","色度","2024-06-19","6","倍","50","","是","否",""]
["2024","06","05","新余市","渝水区","新余超能通新能源有限公司","工业企业","3841|锂离子电池制造","环境风险管控","废水监测点1","国家标准","电池工业污染物排放标准(GB30484-2013)","（表1）现有企业水污染排放限值,企业废水总排放口,锂离子/锂电池直接排放限值","80","","17.1","pH值","2024-06-05","7.0","无量纲","9","6","是","否",""]
["2024","06","05","新余市","渝水区","新余超能通新能源有限公司","工业企业","3841|锂离子电池制造","环境风险管控","废水监测点1","国家标准","电池工业污染物排放标准(GB30484-2013)","（表2）新建企业水污染排放限值,企业废水总排放口,锌锰/锌银/锌空气电池间接排放限值","80","","17.1","总氮（以N计）","2024-06-05","2.39","mg/L","40","","是","否",""]
["2024","06","05","新余市","渝水区","新余超能通新能源有限公司","工业企业","3841|锂离子电池制造","环境风险管控","废水监测点1","国家标准","电池工业污染物排放标准(GB30484-2013)","（表1）现有企业水污染排放限值,企业废水总排放口,锂离子/锂电池间接排放限值","80","","17.1","化学需氧量","2024-06-05","22","mg/L","150","","是","否",""]
["2024","06","05","新余市","渝水区","新余超能通新能源有限公司","工业企业","3841|锂离子电池制造","环境风险管控","废水监测点1","国家标准","电池工业污染物排放标准(GB30484-2013)","（表1）现有企业水污染排放限值,企业废水总排放口,锌锰/锌银/锌空气电池间接排放限值","80","","17.1","悬浮物","2024-06-05","85","mg/L","140","","是","否",""]
["2024","06","05","新余市","渝水区","新余超能通新能源有限公司","工业企业","3841|锂离子电池制造","环境风险管控","废水监测点1","国家标准","电池工业污染物排放标准(GB30484-2013)","（表1）现有企业水污染排放限值,企业废水总排放口,锌锰/锌银/锌空气电池间接排放限值","80","","17.1","总磷（以P计）","2024-06-05","0.28","mg/L","2.0","","是","否",""]
["2024","06","05","新余市","渝水区","新余超能通新能源有限公司","工业企业","3841|锂离子电池制造","环境风险管控","废水监测点1","国家标准","电池工业污染物排放标准(GB30484-2013)","（表3）水污染物特别排放限值,企业废水总排放口,铅蓄电池间接排放限值","80","","17.1","氨氮","2024-06-05","1.39","mg/L","28","","是","否",""]
["2024","06","05","新余市","渝水区","新余超能通新能源有限公司","工业企业","3841|锂离子电池制造","环境风险管控","废水监测点1","国家标准","电池工业污染物排放标准(GB30484-2013)","（表1）现有企业水污染排放限值,企业废水总排放口,锌锰/锌银/锌空气电池直接排放限值","80","","17.1","总锰","2024-06-05","0.03","mg/L","2.0","","是","否",""]
["2024","06","05","新余市","渝水区","新余超能通新能源有限公司","工业企业","3841|锂离子电池制造","环境风险管控","车间废水排放口(DW001)","","","","80","","17.1","锑","2024-06-05","0.0007","mg/L","","","否","",""]
["2024","06","05","新余市","渝水区","新余超能通新能源有限公司","工业企业","3841|锂离子电池制造","环境风险管控","车间废水排放口(DW001)","地方标准","江西省地方标准《工业废水铊污染物排放标准》[地标][地标](DB36/1149——2019)","工业废水铊污染物排放","80","","17.1","铊","2024-06-05","<0.00083","mg/L","0.005","","是","否",""]
["2024","06","18","新余市","渝水区","新余市钢城实业有限公司","工业企业","3340|金属丝绳及其制品制造","环境风险管控","生产废水总排放口001(DW001)","国家标准","钢铁工业水污染物排放标准(GB13456-2012)","（表1、表2）现有和新建企业水污染物排放浓度限值及单位产品基准排水量,企业废水总排放口,间接排放限值","55","0.003","26.2","总铁","2024-06-18","0.664","mg/L","10","","是","否",""]
["2024","06","18","新余市","渝水区","新余市钢城实业有限公司","工业企业","3340|金属丝绳及其制品制造","环境风险管控","生产废水总排放口001(DW001)","国家标准","钢铁工业水污染物排放标准(GB13456-2012)","（表1、表2）现有和新建企业水污染物排放浓度限值及单位产品基准排水量,企业废水总排放口,间接排放限值","55","0.003","26.2","总氮（以N计）","2024-06-18","15.7","mg/L","35","","是","否",""]
["2024","06","18","新余市","渝水区","新余市钢城实业有限公司","工业企业","3340|金属丝绳及其制品制造","环境风险管控","生产废水总排放口001(DW001)","国家标准","钢铁工业水污染物排放标准(GB13456-2012)","（表1、表2）现有和新建企业水污染物排放浓度限值及单位产品基准排水量,企业废水总排放口,间接排放限值","55","0.003","26.2","化学需氧量","2024-06-18","57","mg/L","200","","是","否",""]
["2024","06","18","新余市","渝水区","新余市钢城实业有限公司","工业企业","3340|金属丝绳及其制品制造","环境风险管控","生产废水总排放口001(DW001)","国家标准","钢铁工业水污染物排放标准(GB13456-2012)","（表1、表2）现有和新建企业水污染物排放浓度限值及单位产品基准排水量,企业废水总排放口,间接排放限值","55","0.003","26.2","氟化物","2024-06-18","0.22","mg/L","20","","是","否",""]
["2024","06","18","新余市","渝水区","新余市钢城实业有限公司","工业企业","3340|金属丝绳及其制品制造","环境风险管控","生产废水总排放口001(DW001)","国家标准","钢铁工业水污染物排放标准(GB13456-2012)","（表1、表2）现有和新建企业水污染物排放浓度限值及单位产品基准排水量,企业废水总排放口,间接排放限值","55","0.003","26.2","悬浮物","2024-06-18","7","mg/L","100","","是","否",""]
["2024","06","18","新余市","渝水区","新余市钢城实业有限公司","工业企业","3340|金属丝绳及其制品制造","环境风险管控","生产废水总排放口001(DW001)","国家标准","钢铁工业水污染物排放标准(GB13456-2012)","（表1、表2）现有和新建企业水污染物排放浓度限值及单位产品基准排水量,企业废水总排放口,间接排放限值","55","0.003","26.2","总氰化物","2024-06-18","0.004","mg/L","0.5","","是","否",""]
["2024","06","18","新余市","渝水区","新余市钢城实业有限公司","工业企业","3340|金属丝绳及其制品制造","环境风险管控","生产废水总排放口001(DW001)","国家标准","钢铁工业水污染物排放标准(GB13456-2012)","（表1、表2）现有和新建企业水污染物排放浓度限值及单位产品基准排水量,企业废水总排放口,间接排放限值","55","0.003","26.2","pH值","2024-06-18","8.4","无量纲","9","6","是","否",""]
["2024","06","18","新余市","渝水区","新余市钢城实业有限公司","工业企业","3340|金属丝绳及其制品制造","环境风险管控","生产废水总排放口001(DW001)","国家标准","钢铁工业水污染物排放标准(GB13456-2012)","（表1、表2）现有和新建企业水污染物排放浓度限值及单位产品基准排水量,企业废水总排放口,间接排放限值","55","0.003","26.2","氨氮（NH3-N）","2024-06-18","3.12","mg/L","15","","是","否",""]
["2024","06","18","新余市","渝水区","新余市钢城实业有限公司","工业企业","3340|金属丝绳及其制品制造","环境风险管控","生产废水总排放口001(DW001)","国家标准","钢铁工业水污染物排放标准(GB13456-2012)","（表1、表2）现有和新建企业水污染物排放浓度限值及单位产品基准排水量,企业废水总排放口,间接排放限值","55","0.003","26.2","总磷（以P计）","2024-06-18","0.08","mg/L","2.0","","是","否",""]
["2024","06","18","新余市","渝水区","新余市钢城实业有限公司","工业企业","3340|金属丝绳及其制品制造","环境风险管控","生产废水总排放口001(DW001)","国家标准","钢铁工业水污染物排放标准(GB13456-2012)","（表1、表2）现有和新建企业水污染物排放浓度限值及单位产品基准排水量,企业废水总排放口,间接排放限值","55","0.003","26.2","总铜","2024-06-18","0.00862","mg/L","1.0","","是","否",""]
["2024","06","18","新余市","渝水区","新余市钢城实业有限公司","工业企业","3340|金属丝绳及其制品制造","环境风险管控","生产废水总排放口001(DW001)","国家标准","钢铁工业水污染物排放标准(GB13456-2012)","（表1、表2）现有和新建企业水污染物排放浓度限值及单位产品基准排水量,企业废水总排放口,间接排放限值","55","0.003","26.2","总锌","2024-06-18","0.0107","mg/L","4.0","","是","否",""]
["2024","06","18","新余市","渝水区","新余市钢城实业有限公司","工业企业","3340|金属丝绳及其制品制造","环境风险管控","生产废水总排放口001(DW001)","国家标准","钢铁工业水污染物排放标准(GB13456-2012)","（表1、表2）现有和新建企业水污染物排放浓度限值及单位产品基准排水量,企业废水总排放口,间接排放限值","55","0.003","26.2","石油类","2024-06-18","<0.06","mg/L","10","","是","否",""]
["2024","06","13","新余市","渝水区","新余市环境卫生管理处（生活垃圾卫生填埋场）","固废处置厂","7820|环境卫生管理","水环境,地下水,环境风险管控","废水处理设施排放口","国家标准","生活垃圾填埋场污染控制标准(GB16889-2008)","现有和新建生活垃圾填埋场水污染物排放浓度限值","93","0.004","23.3","总汞","2024-06-13","<0.00004","mg/L","0.001","","是","否",""]
["2024","06","13","新余市","渝水区","新余市环境卫生管理处（生活垃圾卫生填埋场）","固废处置厂","7820|环境卫生管理","水环境,地下水,环境风险管控","废水处理设施排放口","国家标准","生活垃圾填埋场污染控制标准(GB16889-2008)","现有和新建生活垃圾填埋场水污染物排放浓度限值","93","0.004","23.3","总铅","2024-06-13","0.00019","mg/L","0.1","","是","否",""]
["2024","06","13","新余市","渝水区","新余市环境卫生管理处（生活垃圾卫生填埋场）","固废处置厂","7820|环境卫生管理","水环境,地下水,环境风险管控","废水处理设施排放口","国家标准","生活垃圾填埋场污染控制标准(GB16889-2008)","现有和新建生活垃圾填埋场水污染物排放浓度限值","93","0.004","23.3","化学需氧量","2024-06-13","44","mg/L","100","","是","否",""]
["2024","06","13","新余市","渝水区","新余市环境卫生管理处（生活垃圾卫生填埋场）","固废处置厂","7820|环境卫生管理","水环境,地下水,环境风险管控","废水处理设施排放口","国家标准","生活垃圾填埋场污染控制标准(GB16889-2008)","现有和新建生活垃圾填埋场水污染物排放浓度限值","93","0.004","23.3","总铬","2024-06-13","0.006","mg/L","0.1","","是","否",""]
["2024","06","13","新余市","渝水区","新余市环境卫生管理处（生活垃圾卫生填埋场）","固废处置厂","7820|环境卫生管理","水环境,地下水,环境风险管控","废水处理设施排放口","国家标准","生活垃圾填埋场污染控制标准(GB16889-2008)","现有和新建生活垃圾填埋场水污染物排放浓度限值","93","0.004","23.3","总砷","2024-06-13","<0.0003","mg/L","0.1","","是","否",""]
["2024","06","13","新余市","渝水区","新余市环境卫生管理处（生活垃圾卫生填埋场）","固废处置厂","7820|环境卫生管理","水环境,地下水,环境风险管控","废水处理设施排放口","国家标准","生活垃圾填埋场污染控制标准(GB16889-2008)","现有和新建生活垃圾填埋场水污染物排放浓度限值","93","0.004","23.3","总氮（以N计）","2024-06-13","13.0","mg/L","40","","是","否",""]
["2024","06","13","新余市","渝水区","新余市环境卫生管理处（生活垃圾卫生填埋场）","固废处置厂","7820|环境卫生管理","水环境,地下水,环境风险管控","废水处理设施排放口","国家标准","生活垃圾填埋场污染控制标准(GB16889-2008)","现有和新建生活垃圾填埋场水污染物排放浓度限值","93","0.004","23.3","六价铬","2024-06-13","<0.004","mg/L","0.05","","是","否",""]
["2024","06","13","新余市","渝水区","新余市环境卫生管理处（生活垃圾卫生填埋场）","固废处置厂","7820|环境卫生管理","水环境,地下水,环境风险管控","废水处理设施排放口","国家标准","生活垃圾填埋场污染控制标准(GB16889-2008)","现有和新建生活垃圾填埋场水污染物排放浓度限值","93","0.004","23.3","总镉","2024-06-13","<0.00005","mg/L","0.01","","是","否",""]
["2024","06","13","新余市","渝水区","新余市环境卫生管理处（生活垃圾卫生填埋场）","固废处置厂","7820|环境卫生管理","水环境,地下水,环境风险管控","废水处理设施排放口","国家标准","生活垃圾填埋场污染控制标准(GB16889-2008)","现有和新建生活垃圾填埋场水污染物排放浓度限值","93","0.004","23.3","五日生化需氧量（BOD5）","2024-06-13","1.3","mg/L","30","","是","否",""]
["2024","06","13","新余市","渝水区","新余市环境卫生管理处（生活垃圾卫生填埋场）","固废处置厂","7820|环境卫生管理","水环境,地下水,环境风险管控","废水处理设施排放口","国家标准","生活垃圾填埋场污染控制标准(GB16889-2008)","现有和新建生活垃圾填埋场水污染物排放浓度限值","93","0.004","23.3","总磷（以P计）","2024-06-13","0.02","mg/L","3","","是","否",""]
["2024","06","13","新余市","渝水区","新余市环境卫生管理处（生活垃圾卫生填埋场）","固废处置厂","7820|环境卫生管理","水环境,地下水,环境风险管控","废水处理设施排放口","国家标准","生活垃圾填埋场污染控制标准(GB16889-2008)","现有和新建生活垃圾填埋场水污染物排放浓度限值","93","0.004","23.3","粪大肠菌群数","2024-06-13","164","个/L","10000","","是","否",""]
["2024","06","13","新余市","渝水区","新余市环境卫生管理处（生活垃圾卫生填埋场）","固废处置厂","7820|环境卫生管理","水环境,地下水,环境风险管控","废水处理设施排放口","国家标准","生活垃圾填埋场污染控制标准(GB16889-2008)","现有和新建生活垃圾填埋场水污染物排放浓度限值","93","0.004","23.3","悬浮物","2024-06-13","13","mg/L","30","","是","否",""]
["2024","06","13","新余市","渝水区","新余市环境卫生管理处（生活垃圾卫生填埋场）","固废处置厂","7820|环境卫生管理","水环境,地下水,环境风险管控","废水处理设施排放口","国家标准","生活垃圾填埋场污染控制标准(GB16889-2008)","现有和新建生活垃圾填埋场水污染物排放浓度限值","93","0.004","23.3","色度","2024-06-13","5","倍","40","","是","否",""]
["2024","06","13","新余市","渝水区","新余市环境卫生管理处（生活垃圾卫生填埋场）","固废处置厂","7820|环境卫生管理","水环境,地下水,环境风险管控","废水处理设施排放口","国家标准","生活垃圾填埋场污染控制标准(GB16889-2008)","现有和新建生活垃圾填埋场水污染物排放浓度限值","93","0.004","23.3","氨氮（NH3-N）","2024-06-13","0.216","mg/L","25","","是","否",""]
["2024","06","20","新余市","渝水区","新余市裕富金属制品有限公司","工业企业","3130|钢压延加工","环境风险管控","废水监测点2(DW002)","国家标准","钢铁工业水污染物排放标准(GB13456-2012)","（表1、表2）现有和新建企业水污染物排放浓度限值及单位产品基准排水量,车间或生产设施废水排放口,间接排放限值","23.1","","26.7","总汞","2024-06-20","<0.00004","mg/L","0.05","","是","否",""]
["2024","06","20","新余市","渝水区","新余市裕富金属制品有限公司","工业企业","3130|钢压延加工","环境风险管控","废水监测点2(DW002)","国家标准","钢铁工业水污染物排放标准(GB13456-2012)","（表1、表2）现有和新建企业水污染物排放浓度限值及单位产品基准排水量,车间或生产设施废水排放口,间接排放限值","23.1","","26.7","六价铬","2024-06-20","<0.004","mg/L","0.5","","是","否",""]
["2024","06","20","新余市","渝水区","新余市裕富金属制品有限公司","工业企业","3130|钢压延加工","环境风险管控","废水监测点1(DW001)","国家标准","钢铁工业水污染物排放标准(GB13456-2012)","（表1、表2）现有和新建企业水污染物排放浓度限值及单位产品基准排水量,企业废水总排放口,间接排放限值","23.1","","26.4","总氮（以N计）","2024-06-20","3.13","mg/L","35","","是","否",""]
["2024","06","20","新余市","渝水区","新余市裕富金属制品有限公司","工业企业","3130|钢压延加工","环境风险管控","废水监测点1(DW001)","国家标准","钢铁工业水污染物排放标准(GB13456-2012)","（表1、表2）现有和新建企业水污染物排放浓度限值及单位产品基准排水量,企业废水总排放口,间接排放限值","23.1","","26.4","总铁","2024-06-20","0.129","mg/L","10","","是","否",""]
["2024","06","20","新余市","渝水区","新余市裕富金属制品有限公司","工业企业","3130|钢压延加工","环境风险管控","废水监测点1(DW001)","国家标准","钢铁工业水污染物排放标准(GB13456-2012)","（表1、表2）现有和新建企业水污染物排放浓度限值及单位产品基准排水量,企业废水总排放口,间接排放限值","23.1","","26.4","化学需氧量","2024-06-20","17","mg/L","200","","是","否",""]
["2024","06","20","新余市","渝水区","新余市裕富金属制品有限公司","工业企业","3130|钢压延加工","环境风险管控","废水监测点2(DW002)","国家标准","钢铁工业水污染物排放标准(GB13456-2012)","（表1、表2）现有和新建企业水污染物排放浓度限值及单位产品基准排水量,车间或生产设施废水排放口,间接排放限值","23.1","","26.7","总铅","2024-06-20","0.00077","mg/L","1.0","","是","否",""]
["2024","06","20","新余市","渝水区","新余市裕富金属制品有限公司","工业企业","3130|钢压延加工","环境风险管控","废水监测点1(DW001)","国家标准","钢铁工业水污染物排放标准(GB13456-2012)","（表1、表2）现有和新建企业水污染物排放浓度限值及单位产品基准排水量,企业废水总排放口,间接排放限值","23.1","","26.4","总铜","2024-06-20","0.00150","mg/L","1.0","","是","否",""]
["2024","06","20","新余市","渝水区","新余市裕富金属制品有限公司","工业企业","3130|钢压延加工","环境风险管控","废水监测点1(DW001)","国家标准","钢铁工业水污染物排放标准(GB13456-2012)","（表1、表2）现有和新建企业水污染物排放浓度限值及单位产品基准排水量,企业废水总排放口,间接排放限值","23.1","","26.4","氨氮（NH3-N）","2024-06-20","0.16","mg/L","15","","是","否",""]
["2024","06","20","新余市","渝水区","新余市裕富金属制品有限公司","工业企业","3130|钢压延加工","环境风险管控","废水监测点1(DW001)","国家标准","钢铁工业水污染物排放标准(GB13456-2012)","（表1、表2）现有和新建企业水污染物排放浓度限值及单位产品基准排水量,企业废水总排放口,间接排放限值","23.1","","26.4","氟化物","2024-06-20","0.38","mg/L","20","","是","否",""]
["2024","06","20","新余市","渝水区","新余市裕富金属制品有限公司","工业企业","3130|钢压延加工","环境风险管控","废水监测点1(DW001)","国家标准","钢铁工业水污染物排放标准(GB13456-2012)","（表1、表2）现有和新建企业水污染物排放浓度限值及单位产品基准排水量,企业废水总排放口,间接排放限值","23.1","","26.4","石油类","2024-06-20","<0.06","mg/L","10","","是","否",""]
["2024","06","20","新余市","渝水区","新余市裕富金属制品有限公司","工业企业","3130|钢压延加工","环境风险管控","废水监测点2(DW002)","国家标准","钢铁工业水污染物排放标准(GB13456-2012)","（表1、表2）现有和新建企业水污染物排放浓度限值及单位产品基准排水量,车间或生产设施废水排放口,间接排放限值","23.1","","26.7","总铬","2024-06-20","0.020","mg/L","1.5","","是","否",""]
["2024","06","20","新余市","渝水区","新余市裕富金属制品有限公司","工业企业","3130|钢压延加工","环境风险管控","废水监测点2(DW002)","国家标准","钢铁工业水污染物排放标准(GB13456-2012)","（表1、表2）现有和新建企业水污染物排放浓度限值及单位产品基准排水量,车间或生产设施废水排放口,间接排放限值","23.1","","26.7","总砷","2024-06-20","0.0005","mg/L","0.5","","是","否",""]
["2024","06","20","新余市","渝水区","新余市裕富金属制品有限公司","工业企业","3130|钢压延加工","环境风险管控","废水监测点2(DW002)","国家标准","钢铁工业水污染物排放标准(GB13456-2012)","（表1、表2）现有和新建企业水污染物排放浓度限值及单位产品基准排水量,车间或生产设施废水排放口,间接排放限值","23.1","","26.7","总镍","2024-06-20","0.00093","mg/L","1.0","","是","否",""]
["2024","06","20","新余市","渝水区","新余市裕富金属制品有限公司","工业企业","3130|钢压延加工","环境风险管控","废水监测点1(DW001)","国家标准","钢铁工业水污染物排放标准(GB13456-2012)","（表1、表2）现有和新建企业水污染物排放浓度限值及单位产品基准排水量,企业废水总排放口,间接排放限值","23.1","","26.4","总氰化物","2024-06-20","0.007","mg/L","0.5","","是","否",""]
["2024","06","20","新余市","渝水区","新余市裕富金属制品有限公司","工业企业","3130|钢压延加工","环境风险管控","废水监测点1(DW001)","国家标准","钢铁工业水污染物排放标准(GB13456-2012)","（表1、表2）现有和新建企业水污染物排放浓度限值及单位产品基准排水量,企业废水总排放口,间接排放限值","23.1","","26.4","悬浮物","2024-06-20","13","mg/L","100","","是","否",""]
["2024","06","20","新余市","渝水区","新余市裕富金属制品有限公司","工业企业","3130|钢压延加工","环境风险管控","废水监测点1(DW001)","国家标准","钢铁工业水污染物排放标准(GB13456-2012)","（表1、表2）现有和新建企业水污染物排放浓度限值及单位产品基准排水量,企业废水总排放口,间接排放限值","23.1","","26.4","总锌","2024-06-20","0.0994","mg/L","4.0","","是","否",""]
["2024","06","20","新余市","渝水区","新余市裕富金属制品有限公司","工业企业","3130|钢压延加工","环境风险管控","废水监测点1(DW001)","国家标准","钢铁工业水污染物排放标准(GB13456-2012)","（表1、表2）现有和新建企业水污染物排放浓度限值及单位产品基准排水量,企业废水总排放口,间接排放限值","23.1","","26.4","pH值","2024-06-20","7.8","无量纲","9","6","是","否",""]
["2024","06","20","新余市","渝水区","新余市裕富金属制品有限公司","工业企业","3130|钢压延加工","环境风险管控","废水监测点1(DW001)","国家标准","钢铁工业水污染物排放标准(GB13456-2012)","（表1、表2）现有和新建企业水污染物排放浓度限值及单位产品基准排水量,企业废水总排放口,间接排放限值","23.1","","26.4","总磷（以P计）","2024-06-20","0.58","mg/L","2.0","","是","否",""]
["2024","06","20","新余市","渝水区","新余市裕富金属制品有限公司","工业企业","3130|钢压延加工","环境风险管控","废水监测点2(DW002)","国家标准","钢铁工业水污染物排放标准(GB13456-2012)","（表1、表2）现有和新建企业水污染物排放浓度限值及单位产品基准排水量,车间或生产设施废水排放口,间接排放限值","23.1","","26.7","总镉","2024-06-20","0.00006","mg/L","0.1","","是","否",""]
["2024","06","27","新余市","分宜县","江西恩达麻世纪科技股份有限公司","工业企业","1732|麻织造加工","水环境","废水总排口监测点(DW001)","国家标准","纺织染整工业水污染物排放标准(GB4287-2012)","（表2）新建企业水污染物排放浓度限值及单位产品基准排水量,企业废水总排放口,间接排放,通用","10.8","0.03","33.5","二氧化氯","2024-06-27","<0.09","mg/L","0.5","","是","否",""]
["2024","06","27","新余市","分宜县","江西恩达麻世纪科技股份有限公司","工业企业","1732|麻织造加工","水环境","车间排口(DW002)","国家标准","纺织染整工业水污染物排放标准(GB4287-2012)","（表1）现有企业水污染物排放浓度限值及单位产品基准排水量,车间或生产设施废水排放口","","","","六价铬","2024-06-27","0.094","mg/L","0.5","","是","否",""]
["2024","06","27","新余市","分宜县","江西恩达麻世纪科技股份有限公司","工业企业","1732|麻织造加工","水环境","废水总排口监测点(DW001)","国家标准","纺织染整工业水污染物排放标准(GB4287-2012)","（表2）新建企业水污染物排放浓度限值及单位产品基准排水量,企业废水总排放口,间接排放,非蜡染行业间接排放","10.8","0.03","33.5","总氮（以N计）","2024-06-27","12.0","mg/L","30","","是","否",""]
["2024","06","27","新余市","分宜县","江西恩达麻世纪科技股份有限公司","工业企业","1732|麻织造加工","水环境","废水总排口监测点(DW001)","国家标准","纺织染整工业水污染物排放标准(GB4287-2012)","（表2）新建企业水污染物排放浓度限值及单位产品基准排水量,企业废水总排放口,间接排放,通用","10.8","0.03","33.5","总锑","2024-06-27","0.00049","mg/L","0.10","","是","否",""]
["2024","06","27","新余市","分宜县","江西恩达麻世纪科技股份有限公司","工业企业","1732|麻织造加工","水环境","废水总排口监测点(DW001)","国家标准","纺织染整工业水污染物排放标准(GB4287-2012)","（表2）新建企业水污染物排放浓度限值及单位产品基准排水量,企业废水总排放口,间接排放,通用","10.8","0.03","33.5","五日生化需氧量（BOD5）","2024-06-27","4.8","mg/L","50","","是","否",""]
["2024","06","27","新余市","分宜县","江西恩达麻世纪科技股份有限公司","工业企业","1732|麻织造加工","水环境","废水总排口监测点(DW001)","国家标准","纺织染整工业水污染物排放标准(GB4287-2012)","（表2）新建企业水污染物排放浓度限值及单位产品基准排水量,企业废水总排放口,间接排放,通用","10.8","0.03","33.5","悬浮物","2024-06-27","14","mg/L","100","","是","否",""]
["2024","06","27","新余市","分宜县","江西恩达麻世纪科技股份有限公司","工业企业","1732|麻织造加工","水环境","废水总排口监测点(DW001)","国家标准","纺织染整工业水污染物排放标准(GB4287-2012)","（表2）新建企业水污染物排放浓度限值及单位产品基准排水量,企业废水总排放口,间接排放,通用","10.8","0.03","33.5","化学需氧量","2024-06-27","59","mg/L","200","","是","否",""]
["2024","06","27","新余市","分宜县","江西恩达麻世纪科技股份有限公司","工业企业","1732|麻织造加工","水环境","废水总排口监测点","国家标准","纺织染整工业水污染物排放标准(GB4287-2012)","（表3）水污染物特别排放限值,企业废水总排放口,间接排放","10.8","0.03","33.5","总磷（以P计）","2024-06-27","0.05","mg/L","0.5","","是","否",""]
["2024","06","27","新余市","分宜县","江西恩达麻世纪科技股份有限公司","工业企业","1732|麻织造加工","水环境","废水总排口监测点(DW001)","国家标准","纺织染整工业水污染物排放标准(GB4287-2012)","（表2）新建企业水污染物排放浓度限值及单位产品基准排水量,企业废水总排放口,间接排放,非蜡染行业间接排放","10.8","0.03","33.5","氨氮（NH3-N）","2024-06-27","2.68","mg/L","20","","是","否",""]
["2024","06","27","新余市","分宜县","江西恩达麻世纪科技股份有限公司","工业企业","1732|麻织造加工","水环境","废水总排口监测点","国家标准","麻纺工业水污染物排放标准(GB28938-2012)","（表1、表2）现有和新建企业水污染物排浓度放限值及单位产品基准排水量,企业废水总排放口,间接排放","10.8","0.03","33.5","可吸附有机卤素化合物（AOX）","2024-06-27","0.185","mg/L","10","","是","否",""]
["2024","06","27","新余市","分宜县","江西恩达麻世纪科技股份有限公司","工业企业","1732|麻织造加工","水环境","废水总排口监测点(DW001)","国家标准","纺织染整工业水污染物排放标准(GB4287-2012)","（表2）新建企业水污染物排放浓度限值及单位产品基准排水量,企业废水总排放口,间接排放,通用","10.8","0.03","33.5","pH值","2024-06-27","6.9","无量纲","9","6","是","否",""]
["2024","06","27","新余市","分宜县","江西恩达麻世纪科技股份有限公司","工业企业","1732|麻织造加工","水环境","废水总排口监测点(DW001)","国家标准","纺织染整工业水污染物排放标准(GB4287-2012)","（表2）新建企业水污染物排放浓度限值及单位产品基准排水量,企业废水总排放口,间接排放,通用","10.8","0.03","33.5","色度","2024-06-27","6","倍","80","","是","否",""]
["2024","06","27","新余市","分宜县","江西恩达麻世纪科技股份有限公司","工业企业","1732|麻织造加工","水环境","废水总排口监测点(DW001)","国家标准","纺织染整工业水污染物排放标准(GB4287-2012)","（表2）新建企业水污染物排放浓度限值及单位产品基准排水量,企业废水总排放口,间接排放,通用","10.8","0.03","33.5","硫化物","2024-06-27","<0.01","mg/L","0.5","","是","否",""]
["2024","06","27","新余市","分宜县","江西恩达麻世纪科技股份有限公司","工业企业","1732|麻织造加工","水环境","废水总排口监测点(DW001)","国家标准","纺织染整工业水污染物排放标准(GB4287-2012)","（表1）现有企业水污染物排放浓度限值及单位产品基准排水量,企业废水总排放口,间接排放,通用","10.8","0.03","33.5","苯胺类","2024-06-27","0.23","mg/L","1.0","","是","否",""]
["2024","06","26","新余市","","华腾地毯有限公司","工业企业","2437|地毯、挂毯制造","水环境","废水监测点1(DW001)","国家标准","纺织染整工业水污染物排放标准(GB4287-2012)","（表2）新建企业水污染物排放浓度限值及单位产品基准排水量,企业废水总排放口,间接排放,通用","7.5","","24.3","总磷（以P计）","2024-06-26","0.04","mg/L","1.5","","是","否",""]
["2024","06","26","新余市","","华腾地毯有限公司","工业企业","2437|地毯、挂毯制造","水环境","废水监测点1(DW001)","国家标准","纺织染整工业水污染物排放标准(GB4287-2012)","（表2）新建企业水污染物排放浓度限值及单位产品基准排水量,企业废水总排放口,间接排放,通用","7.5","","24.3","硫化物","2024-06-26","<0.01","mg/L","0.5","","是","否",""]
["2024","06","26","新余市","","华腾地毯有限公司","工业企业","2437|地毯、挂毯制造","水环境","废水监测点1(DW001)","国家标准","纺织染整工业水污染物排放标准(GB4287-2012)","（表1）现有企业水污染物排放浓度限值及单位产品基准排水量,企业废水总排放口,间接排放,通用","7.5","","24.3","苯胺类","2024-06-26","0.16","mg/L","1.0","","是","否",""]
["2024","06","26","新余市","","华腾地毯有限公司","工业企业","2437|地毯、挂毯制造","水环境","废水监测点1(DW001)","国家标准","纺织染整工业水污染物排放标准(GB4287-2012)","（表2）新建企业水污染物排放浓度限值及单位产品基准排水量,企业废水总排放口,间接排放,通用","7.5","","24.3","色度","2024-06-26","6","倍","80","","是","否",""]
["2024","06","26","新余市","","华腾地毯有限公司","工业企业","2437|地毯、挂毯制造","水环境","废水监测点1(DW001)","国家标准","纺织染整工业水污染物排放标准(GB4287-2012)","（表2）新建企业水污染物排放浓度限值及单位产品基准排水量,企业废水总排放口,间接排放,非蜡染行业间接排放","7.5","","24.3","总氮（以N计）","2024-06-26","1.59","mg/L","30","","是","否",""]
["2024","06","26","新余市","","华腾地毯有限公司","工业企业","2437|地毯、挂毯制造","水环境","废水监测点1(DW001)","国家标准","纺织染整工业水污染物排放标准(GB4287-2012)","（表2）新建企业水污染物排放浓度限值及单位产品基准排水量,企业废水总排放口,间接排放,通用","7.5","","24.3","二氧化氯","2024-06-26","<0.09","mg/L","0.5","","是","否",""]
["2024","06","26","新余市","","华腾地毯有限公司","工业企业","2437|地毯、挂毯制造","水环境","废水监测点1(DW001)","国家标准","纺织染整工业水污染物排放标准(GB4287-2012)","（表2）新建企业水污染物排放浓度限值及单位产品基准排水量,企业废水总排放口,间接排放,通用","7.5","","24.3","可吸附有机卤素化合物（AOX）","2024-06-26","0.204","mg/L","12","","是","否",""]
["2024","06","26","新余市","","华腾地毯有限公司","工业企业","2437|地毯、挂毯制造","水环境","废水监测点1(DW001)","国家标准","纺织染整工业水污染物排放标准(GB4287-2012)","（表2）新建企业水污染物排放浓度限值及单位产品基准排水量,企业废水总排放口,间接排放,通用","7.5","","24.3","五日生化需氧量（BOD5）","2024-06-26","0.9","mg/L","50","","是","否",""]
["2024","06","26","新余市","","华腾地毯有限公司","工业企业","2437|地毯、挂毯制造","水环境","废水监测点1(DW001)","国家标准","污水综合排放标准(GB8978-1996)","（表4）第二类污染物最高允许排放浓度（1998年1月1日后建的单位）,一切排污单位 ,三级标准","7.5","","24.3","石油类","2024-06-26","<0.06","mg/L","20","","是","否",""]
["2024","06","26","新余市","","华腾地毯有限公司","工业企业","2437|地毯、挂毯制造","水环境","废水监测点1(DW001)","国家标准","纺织染整工业水污染物排放标准(GB4287-2012)","（表2）新建企业水污染物排放浓度限值及单位产品基准排水量,企业废水总排放口,间接排放,通用","7.5","","24.3","总锑","2024-06-26","0.00494","mg/L","0.10","","是","否",""]
["2024","06","26","新余市","","华腾地毯有限公司","工业企业","2437|地毯、挂毯制造","水环境","废水监测点1(DW001)","国家标准","纺织染整工业水污染物排放标准(GB4287-2012)","（表2）新建企业水污染物排放浓度限值及单位产品基准排水量,企业废水总排放口,间接排放,非蜡染行业间接排放","7.5","","24.3","氨氮（NH3-N）","2024-06-26","0.228","mg/L","20","","是","否",""]
["2024","06","26","新余市","","华腾地毯有限公司","工业企业","2437|地毯、挂毯制造","水环境","车间排口","国家标准","纺织染整工业水污染物排放标准(GB4287-2012)","（表1）现有企业水污染物排放浓度限值及单位产品基准排水量,车间或生产设施废水排放口","","","","六价铬","2024-06-26","0.020","mg/L","0.5","","是","否",""]
["2024","06","26","新余市","","华腾地毯有限公司","工业企业","2437|地毯、挂毯制造","水环境","废水监测点1(DW001)","国家标准","纺织染整工业水污染物排放标准(GB4287-2012)","（表2）新建企业水污染物排放浓度限值及单位产品基准排水量,企业废水总排放口,间接排放,通用","7.5","","24.3","pH值","2024-06-26","7.7","无量纲","9","6","是","否",""]
["2024","06","26","新余市","","华腾地毯有限公司","工业企业","2437|地毯、挂毯制造","水环境","废水监测点1(DW001)","国家标准","纺织染整工业水污染物排放标准(GB4287-2012)","（表2）新建企业水污染物排放浓度限值及单位产品基准排水量,企业废水总排放口,间接排放,通用","7.5","","24.3","悬浮物","2024-06-26","9","mg/L","100","","是","否",""]
["2024","06","26","新余市","","华腾地毯有限公司","工业企业","2437|地毯、挂毯制造","水环境","废水监测点1(DW001)","国家标准","纺织染整工业水污染物排放标准(GB4287-2012)","（表2）新建企业水污染物排放浓度限值及单位产品基准排水量,企业废水总排放口,间接排放,通用","7.5","","24.3","化学需氧量","2024-06-26","19","mg/L","200","","是","否",""]
["2024","06","24","新余市","","江西澳力特缸套有限公司","工业企业","367|汽车零部件及配件制造","水环境,土壤污染监管","处理设施排口（总排口、车间排口）","国家标准","电镀污染物排放标准(GB21900-2008)","（表2）新建企业水污染物排放限值,企业废水总排放口","1","","22.8","总铁","2024-06-24","<0.03","mg/L","3.0","","是","否",""]
["2024","06","24","新余市","","江西澳力特缸套有限公司","工业企业","367|汽车零部件及配件制造","水环境,土壤污染监管","处理设施排口（总排口、车间排口）","国家标准","电镀污染物排放标准(GB21900-2008)","（表2）新建企业水污染物排放限值,企业废水总排放口","1","","22.8","悬浮物","2024-06-24","12","mg/L","50","","是","否",""]
["2024","06","24","新余市","","江西澳力特缸套有限公司","工业企业","367|汽车零部件及配件制造","水环境,土壤污染监管","处理设施排口（总排口、车间排口）","国家标准","电镀污染物排放标准(GB21900-2008)","（表2）新建企业水污染物排放限值,企业废水总排放口","1","","22.8","总铜","2024-06-24","0.457","mg/L","0.5","","是","否",""]
["2024","06","24","新余市","","江西澳力特缸套有限公司","工业企业","367|汽车零部件及配件制造","水环境,土壤污染监管","处理设施排口（总排口、车间排口）","国家标准","电镀污染物排放标准(GB21900-2008)","（表2）新建企业水污染物排放限值,企业废水总排放口","1","","22.8","总铝","2024-06-24","0.0927","mg/L","3.0","","是","否",""]
["2024","06","24","新余市","","江西澳力特缸套有限公司","工业企业","367|汽车零部件及配件制造","水环境,土壤污染监管","处理设施排口（总排口、车间排口）","国家标准","电镀污染物排放标准(GB21900-2008)","（表2）新建企业水污染物排放限值,企业废水总排放口","1","","22.8","总氮（以N计）","2024-06-24","8.78","mg/L","20","","是","否",""]
["2024","06","24","新余市","","江西澳力特缸套有限公司","工业企业","367|汽车零部件及配件制造","水环境,土壤污染监管","处理设施排口（总排口、车间排口）","国家标准","电镀污染物排放标准(GB21900-2008)","（表2）新建企业水污染物排放限值,企业废水总排放口","1","","22.8","石油类","2024-06-24","<0.06","mg/L","3.0","","是","否",""]
["2024","06","24","新余市","","江西澳力特缸套有限公司","工业企业","367|汽车零部件及配件制造","水环境,土壤污染监管","处理设施排口（总排口、车间排口）","国家标准","电镀污染物排放标准(GB21900-2008)","（表2）新建企业水污染物排放限值,企业废水总排放口","1","","22.8","氟化物","2024-06-24","3.45","mg/L","10","","是","否",""]
["2024","06","24","新余市","","江西澳力特缸套有限公司","工业企业","367|汽车零部件及配件制造","水环境,土壤污染监管","处理设施排口（总排口、车间排口）","国家标准","电镀污染物排放标准(GB21900-2008)","（表2）新建企业水污染物排放限值,企业废水总排放口","1","","22.8","化学需氧量","2024-06-24","18","mg/L","80","","是","否",""]
["2024","06","24","新余市","","江西澳力特缸套有限公司","工业企业","367|汽车零部件及配件制造","水环境,土壤污染监管","处理设施排口（总排口、车间排口）","国家标准","电镀污染物排放标准(GB21900-2008)","（表2）新建企业水污染物排放限值,企业废水总排放口","1","","22.8","总锌","2024-06-24","0.0220","mg/L","1.5","","是","否",""]
["2024","06","24","新余市","","江西澳力特缸套有限公司","工业企业","367|汽车零部件及配件制造","水环境,土壤污染监管","处理设施排口（总排口、车间排口）","国家标准","电镀污染物排放标准(GB21900-2008)","（表2）新建企业水污染物排放限值,车间或生产设施废水排放口","1","","22.8","总铬","2024-06-24","0.049","mg/L","1.0","","是","否",""]
["2024","06","24","新余市","","江西澳力特缸套有限公司","工业企业","367|汽车零部件及配件制造","水环境,土壤污染监管","处理设施排口（总排口、车间排口）","地方标准","江西省地方标准《工业废水铊污染物排放标准》[地标][地标](DB36/1149——2019)","工业废水铊污染物排放","1","","22.8","铊","2024-06-24","<0.00002","mg/L","0.005","","是","否",""]
["2024","06","24","新余市","","江西澳力特缸套有限公司","工业企业","367|汽车零部件及配件制造","水环境,土壤污染监管","处理设施排口（总排口、车间排口）","","","","1","","22.8","锑","2024-06-24","<0.00015","mg/L","","","否","",""]
["2024","06","24","新余市","","江西澳力特缸套有限公司","工业企业","367|汽车零部件及配件制造","水环境,土壤污染监管","处理设施排口（总排口、车间排口）","国家标准","电镀污染物排放标准(GB21900-2008)","（表2）新建企业水污染物排放限值,车间或生产设施废水排放口","1","","22.8","六价铬","2024-06-24","0.029","mg/L","0.2","","是","否",""]
["2024","06","24","新余市","","江西澳力特缸套有限公司","工业企业","367|汽车零部件及配件制造","水环境,土壤污染监管","处理设施排口（总排口、车间排口）","国家标准","电镀污染物排放标准(GB21900-2008)","（表2）新建企业水污染物排放限值,企业废水总排放口","1","","22.8","pH值","2024-06-24","8.8","无量纲","9","6","是","否",""]
["2024","06","24","新余市","","江西澳力特缸套有限公司","工业企业","367|汽车零部件及配件制造","水环境,土壤污染监管","处理设施排口（总排口、车间排口）","国家标准","电镀污染物排放标准(GB21900-2008)","（表2）新建企业水污染物排放限值,企业废水总排放口","1","","22.8","氨氮（NH3-N）","2024-06-24","6.78","mg/L","15","","是","否",""]
["2024","06","24","新余市","","江西澳力特缸套有限公司","工业企业","367|汽车零部件及配件制造","水环境,土壤污染监管","处理设施排口（总排口、车间排口）","国家标准","电镀污染物排放标准(GB21900-2008)","（表2）新建企业水污染物排放限值,企业废水总排放口","1","","22.8","总磷（以P计）","2024-06-24","0.04","mg/L","1.0","","是","否",""]
["2024","06","24","新余市","","江西澳力特缸套有限公司","工业企业","367|汽车零部件及配件制造","水环境,土壤污染监管","处理设施排口（总排口、车间排口）","国家标准","电镀污染物排放标准(GB21900-2008)","（表2）新建企业水污染物排放限值,企业废水总排放口","1","","22.8","氰化物（总氰化合物）","2024-06-24","<0.001","mg/L","0.3","","是","否",""]
["2024","06","21","新余市","","江西宏懋新材料科技有限公司","工业企业","1751|化纤织造加工","水环境","综合废水排放口001(DW001)","地方标准","新余高新区污水处理厂接管标准(001)","污水处理厂接管进水限值","45","0.0013","28","总磷（以P计）","2024-06-21","0.06","mg/L","7","","是","否",""]
["2024","06","21","新余市","","江西宏懋新材料科技有限公司","工业企业","1751|化纤织造加工","水环境","综合废水排放口001(DW001)","地方标准","新余高新区污水处理厂接管标准(001)","污水处理厂接管进水限值","45","0.0013","28","化学需氧量","2024-06-21","116","mg/L","500","","是","否",""]
["2024","06","21","新余市","","江西宏懋新材料科技有限公司","工业企业","1751|化纤织造加工","水环境","综合废水排放口001(DW001)","地方标准","新余高新区污水处理厂接管标准(001)","污水处理厂接管进水限值","45","0.0013","28","悬浮物","2024-06-21","8","mg/L","300","","是","否",""]
["2024","06","21","新余市","","江西宏懋新材料科技有限公司","工业企业","1751|化纤织造加工","水环境","综合废水排放口001(DW001)","地方标准","新余高新区污水处理厂接管标准(001)","污水处理厂接管进水限值","45","0.0013","28","五日生化需氧量（BOD5）","2024-06-21","36.7","mg/L","250","","是","否",""]
["2024","06","21","新余市","","江西宏懋新材料科技有限公司","工业企业","1751|化纤织造加工","水环境","综合废水排放口001(DW001)","地方标准","新余高新区污水处理厂接管标准(001)","污水处理厂接管进水限值","45","0.0013","28","氨氮（NH3-N）","2024-06-21","0.24","mg/L","35","","是","否",""]
["2024","06","21","新余市","","江西宏懋新材料科技有限公司","工业企业","1751|化纤织造加工","水环境","综合废水排放口001(DW001)","地方标准","新余高新区污水处理厂接管标准(001)","污水处理厂接管进水限值","45","0.0013","28","总氮（以N计）","2024-06-21","0.70","mg/L","50","","是","否",""]
["2024","06","21","新余市","","江西宏懋新材料科技有限公司","工业企业","1751|化纤织造加工","水环境","综合废水排放口001(DW001)","地方标准","新余高新区污水处理厂接管标准(001)","污水处理厂接管进水限值","45","0.0013","28","pH值","2024-06-21","7.3","无量纲","9","6","是","否",""]
["2024","06","21","新余市","","江西省金锂科技股份有限公司","工业企业","2614|有机化学原料制造","水环境","污水排放总口(DW001)","国家标准","无机化学工业污染物排放标准(GB31573-2015)"," （表1）水污染物排放限值,间接排放","77.8","0.00025","26.7","化学需氧量","2024-06-21","7","mg/L","200","","是","否",""]
["2024","06","21","新余市","","江西省金锂科技股份有限公司","工业企业","2614|有机化学原料制造","水环境","污水排放总口(DW001)","地方标准","新余高新区污水处理厂接管标准(001)","污水处理厂接管进水限值","77.8","0.00025","26.7","五日生化需氧量（BOD5）","2024-06-21","1.5","mg/L","250","","是","否",""]
["2024","06","21","新余市","","江西省金锂科技股份有限公司","工业企业","2614|有机化学原料制造","水环境","污水排放总口(DW001)","国家标准","无机化学工业污染物排放标准(GB31573-2015)"," （表1）水污染物排放限值,间接排放","77.8","0.00025","26.7","PH","2024-06-21","7.4","无量纲","9","6","是","否",""]
["2024","06","21","新余市","","江西省金锂科技股份有限公司","工业企业","2614|有机化学原料制造","水环境","污水排放总口(DW001)","国家标准","无机化学工业污染物排放标准(GB31573-2015)"," （表1）水污染物排放限值,直接排放","77.8","0.00025","26.7","总磷（以P计）","2024-06-21","0.08","mg/L","2","","是","否",""]
["2024","06","21","新余市","","江西省金锂科技股份有限公司","工业企业","2614|有机化学原料制造","水环境","污水排放总口(DW001)","地方标准","新余高新区污水处理厂接管标准(001)","污水处理厂接管进水限值","77.8","0.00025","26.7","氨氮（NH3-N）","2024-06-21","0.08","mg/L","35","","是","否",""]
["2024","06","21","新余市","","江西省金锂科技股份有限公司","工业企业","2614|有机化学原料制造","水环境","污水排放总口(DW001)","国家标准","无机化学工业污染物排放标准(GB31573-2015)"," （表1）水污染物排放限值,直接排放","77.8","0.00025","26.7","悬浮物","2024-06-21","8","mg/L","100","","是","否",""]
["2024","06","21","新余市","","江西省金锂科技股份有限公司","工业企业","2614|有机化学原料制造","水环境","污水排放总口(DW001)","地方标准","新余高新区污水处理厂接管标准(001)","污水处理厂接管进水限值","77.8","0.00025","26.7","总氮（以N计）","2024-06-21","1.53","mg/L","50","","是","否",""]
["2024","06","13","新余市","","新余新钢金属制品有限公司","工业企业","3340|金属丝绳及其制品制造","环境风险管控","钢丝厂废水总排放口(DW001)","国家标准","钢铁工业水污染物排放标准(GB13456-2012)","（表1、表2）现有和新建企业水污染物排放浓度限值及单位产品基准排水量,企业废水总排放口,间接排放限值","82.1","0.0021","27.4","总铜","2024-06-13","0.0104","mg/L","1.0","","是","否",""]
["2024","06","13","新余市","","新余新钢金属制品有限公司","工业企业","3340|金属丝绳及其制品制造","环境风险管控","钢丝厂车间废水排放口(DW002)","国家标准","钢铁工业水污染物排放标准(GB13456-2012)","（表1、表2）现有和新建企业水污染物排放浓度限值及单位产品基准排水量,车间或生产设施废水排放口,间接排放限值","82.1","","28.8","总砷","2024-06-13","0.0047","mg/L","0.5","","是","否",""]
["2024","06","13","新余市","","新余新钢金属制品有限公司","工业企业","3340|金属丝绳及其制品制造","环境风险管控","钢丝厂废水总排放口(DW001)","国家标准","钢铁工业水污染物排放标准(GB13456-2012)","（表1、表2）现有和新建企业水污染物排放浓度限值及单位产品基准排水量,企业废水总排放口,间接排放限值","82.1","0.0021","27.4","总铁","2024-06-13","0.0639","mg/L","10","","是","否",""]
["2024","06","13","新余市","","新余新钢金属制品有限公司","工业企业","3340|金属丝绳及其制品制造","环境风险管控","钢丝厂废水总排放口(DW001)","国家标准","钢铁工业水污染物排放标准(GB13456-2012)","（表1、表2）现有和新建企业水污染物排放浓度限值及单位产品基准排水量,企业废水总排放口,间接排放限值","82.1","0.0021","27.4","pH值","2024-06-13","7.4","无量纲","9","6","是","否",""]
["2024","06","13","新余市","","新余新钢金属制品有限公司","工业企业","3340|金属丝绳及其制品制造","环境风险管控","钢丝厂车间废水排放口(DW002)","国家标准","钢铁工业水污染物排放标准(GB13456-2012)","（表1、表2）现有和新建企业水污染物排放浓度限值及单位产品基准排水量,车间或生产设施废水排放口,间接排放限值","82.1","","28.8","总铬","2024-06-13","0.008","mg/L","1.5","","是","否",""]
["2024","06","13","新余市","","新余新钢金属制品有限公司","工业企业","3340|金属丝绳及其制品制造","环境风险管控","钢丝厂车间废水排放口(DW002)","国家标准","钢铁工业水污染物排放标准(GB13456-2012)","（表1、表2）现有和新建企业水污染物排放浓度限值及单位产品基准排水量,车间或生产设施废水排放口,间接排放限值","82.1","","28.8","总镍","2024-06-13","0.679","mg/L","1","","是","否",""]
["2024","06","13","新余市","","新余新钢金属制品有限公司","工业企业","3340|金属丝绳及其制品制造","环境风险管控","钢丝厂废水总排放口(DW001)","国家标准","钢铁工业水污染物排放标准(GB13456-2012)","（表1、表2）现有和新建企业水污染物排放浓度限值及单位产品基准排水量,企业废水总排放口,间接排放限值","82.1","0.0021","27.4","总氰化物","2024-06-13","<0.001","mg/L","0.5","","是","否",""]
["2024","06","13","新余市","","新余新钢金属制品有限公司","工业企业","3340|金属丝绳及其制品制造","环境风险管控","钢丝厂废水总排放口(DW001)","国家标准","钢铁工业水污染物排放标准(GB13456-2012)","（表1、表2）现有和新建企业水污染物排放浓度限值及单位产品基准排水量,企业废水总排放口,间接排放限值","82.1","0.0021","27.4","悬浮物","2024-06-13","8","mg/L","100","","是","否",""]
["2024","06","13","新余市","","新余新钢金属制品有限公司","工业企业","3340|金属丝绳及其制品制造","环境风险管控","钢丝厂废水总排放口(DW001)","国家标准","钢铁工业水污染物排放标准(GB13456-2012)","（表1、表2）现有和新建企业水污染物排放浓度限值及单位产品基准排水量,企业废水总排放口,间接排放限值","82.1","0.0021","27.4","化学需氧量","2024-06-13","10","mg/L","200","","是","否",""]
["2024","06","13","新余市","","新余新钢金属制品有限公司","工业企业","3340|金属丝绳及其制品制造","环境风险管控","钢丝厂废水总排放口(DW001)","国家标准","钢铁工业水污染物排放标准(GB13456-2012)","（表1、表2）现有和新建企业水污染物排放浓度限值及单位产品基准排水量,企业废水总排放口,间接排放限值","82.1","0.0021","27.4","总磷（以P计）","2024-06-13","0.04","mg/L","2.0","","是","否",""]
["2024","06","13","新余市","","新余新钢金属制品有限公司","工业企业","3340|金属丝绳及其制品制造","环境风险管控","钢丝厂车间废水排放口(DW002)","国家标准","钢铁工业水污染物排放标准(GB13456-2012)","（表1、表2）现有和新建企业水污染物排放浓度限值及单位产品基准排水量,车间或生产设施废水排放口,间接排放限值","82.1","","28.8","总汞","2024-06-13","0.00006","mg/L","0.05","","是","否",""]
["2024","06","13","新余市","","新余新钢金属制品有限公司","工业企业","3340|金属丝绳及其制品制造","环境风险管控","钢丝厂车间废水排放口(DW002)","国家标准","钢铁工业水污染物排放标准(GB13456-2012)","（表1、表2）现有和新建企业水污染物排放浓度限值及单位产品基准排水量,车间或生产设施废水排放口,间接排放限值","82.1","","28.8","六价铬","2024-06-13","<0.004","mg/L","0.5","","是","否",""]
["2024","06","13","新余市","","新余新钢金属制品有限公司","工业企业","3340|金属丝绳及其制品制造","环境风险管控","钢丝厂废水总排放口(DW001)","国家标准","钢铁工业水污染物排放标准(GB13456-2012)","（表1、表2）现有和新建企业水污染物排放浓度限值及单位产品基准排水量,企业废水总排放口,间接排放限值","82.1","0.0021","27.4","氨氮（NH3-N）","2024-06-13","0.64","mg/L","15","","是","否",""]
["2024","06","13","新余市","","新余新钢金属制品有限公司","工业企业","3340|金属丝绳及其制品制造","环境风险管控","钢丝厂废水总排放口(DW001)","国家标准","钢铁工业水污染物排放标准(GB13456-2012)","（表1、表2）现有和新建企业水污染物排放浓度限值及单位产品基准排水量,企业废水总排放口,间接排放限值","82.1","0.0021","27.4","石油类","2024-06-13","0.10","mg/L","10","","是","否",""]
["2024","06","13","新余市","","新余新钢金属制品有限公司","工业企业","3340|金属丝绳及其制品制造","环境风险管控","钢丝厂废水总排放口(DW001)","国家标准","钢铁工业水污染物排放标准(GB13456-2012)","（表1、表2）现有和新建企业水污染物排放浓度限值及单位产品基准排水量,企业废水总排放口,间接排放限值","82.1","0.0021","27.4","总锌","2024-06-13","0.902","mg/L","4.0","","是","否",""]
["2024","06","13","新余市","","新余新钢金属制品有限公司","工业企业","3340|金属丝绳及其制品制造","环境风险管控","钢丝厂废水总排放口(DW001)","国家标准","钢铁工业水污染物排放标准(GB13456-2012)","（表1、表2）现有和新建企业水污染物排放浓度限值及单位产品基准排水量,企业废水总排放口,间接排放限值","82.1","0.0021","27.4","总氮（以N计）","2024-06-13","34.5","mg/L","35","","是","否",""]
["2024","06","13","新余市","","新余新钢金属制品有限公司","工业企业","3340|金属丝绳及其制品制造","环境风险管控","钢丝厂车间废水排放口(DW002)","国家标准","钢铁工业水污染物排放标准(GB13456-2012)","（表1、表2）现有和新建企业水污染物排放浓度限值及单位产品基准排水量,车间或生产设施废水排放口,间接排放限值","82.1","","28.8","总镉","2024-06-13","0.00042","mg/L","0.1","","是","否",""]
["2024","06","13","新余市","","新余新钢金属制品有限公司","工业企业","3340|金属丝绳及其制品制造","环境风险管控","钢丝厂废水总排放口(DW001)","国家标准","钢铁工业水污染物排放标准(GB13456-2012)","（表1、表2）现有和新建企业水污染物排放浓度限值及单位产品基准排水量,企业废水总排放口,间接排放限值","82.1","0.0021","27.4","氟化物","2024-06-13","0.27","mg/L","20","","是","否",""]

{"sheet":"周边环境","index":2,"n_rows":156,"n_cols":41,"rows_kept":156,"merged":[[0,0,0,40]],"flags":["formulas_cached_only"]}
["执法监测周边环境数据",null,"","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","",""]
["监测年","监测月","监测日","市","县","企业名称","企业类别","行业类别","名录类别","监测点名称","排放标准类型","排放标准名称","标准条目","监测项目","项目监测日期","环境空气湿度","环境空气气温","环境空气气压","环境空气风速","环境空气风向","地表水流量","地表水感官描述","地表水有无漂浮物","地表水有无油","地下水井深","地下水水位","土壤采样深度","土壤pH值","土壤颜色","土壤水分","土壤利用情况","环境监测结果/周边环境噪声监测结果(昼间)","周边环境噪声监测结果(夜间)","周边环境噪声声源","周边环境噪声风速","取值单位","排放上限","排放下限","是否有评价限值","是否超标","超标倍数"]
["2024","06","04","新余市","渝水区","奉先德业(新余）医废处置有限公司","固废处置厂","7724|危险废物治理","土壤环境,其他","土壤","","","","锌","2024-06-04","","","","","","","","","","","","0.5","","黄棕","2.8","工业用地","56","","","","mg/KG","","","0","否",""]
["2024","06","04","新余市","渝水区","奉先德业(新余）医废处置有限公司","固废处置厂","7724|危险废物治理","土壤环境,其他","地下水井","国家标准","地下水质量标准(GB/T 14848-2017)","（表2）地下水质量非常规指标及限值,Ⅲ类","镍 ","2024-06-04","","","","","","","","","","8","2.7","","","","","","<0.005","","","","mg/L","0.02","","1","否",""]
["2024","06","04","新余市","渝水区","奉先德业(新余）医废处置有限公司","固废处置厂","7724|危险废物治理","土壤环境,其他","土壤","国家标准","土壤环境质量建设用地土壤污染风险管控标准标准(试行)(GB36600-2018)","表1 建设用地土壤污染风险筛选值与管制值（基本项目）,第二类用地-筛选值","铅","2024-06-04","","","","","","","","","","","","0.5","","黄棕","2.8","工业用地","17.4","","","","mg/KG","800","","1","否",""]
["2024","06","04","新余市","渝水区","奉先德业(新余）医废处置有限公司","固废处置厂","7724|危险废物治理","土壤环境,其他","地下水井","国家标准","地下水质量标准(GB/T 14848-2017)","（表1）地下水质量常规指标及限值,Ⅲ类","汞","2024-06-04","","","","","","","","","","8","2.7","","","","","","0.00009","","","","mg/L","0.001","","1","否",""]
["2024","06","04","新余市","渝水区","奉先德业(新余）医废处置有限公司","固废处置厂","7724|危险废物治理","土壤环境,其他","土壤","国家标准","土壤环境质量建设用地土壤污染风险管控标准标准(试行)(GB36600-2018)","表1 建设用地土壤污染风险筛选值与管制值（基本项目）,第二类用地-筛选值","铬（六价）","2024-06-04","","","","","","","","","","","","0.5","","黄棕","2.8","工业用地","<0.5","","","","mg/KG","5.7","","1","否",""]
["2024","06","04","新余市","渝水区","奉先德业(新余）医废处置有限公司","固废处置厂","7724|危险废物治理","土壤环境,其他","土壤","国家标准","土壤环境质量建设用地土壤污染风险管控标准标准(试行)(GB36600-2018)","表1 建设用地土壤污染风险筛选值与管制值（基本项目）,第二类用地-筛选值","砷","2024-06-04","","","","","","","","","","","","0.5","","黄棕","2.8","工业用地","7.52","","","","mg/KG","60","","1","否",""]
["2024","06","04","新余市","渝水区","奉先德业(新余）医废处置有限公司","固废处置厂","7724|危险废物治理","土壤环境,其他","土壤","国家标准","土壤环境质量建设用地土壤污染风险管控标准标准(试行)(GB36600-2018)","表1 建设用地土壤污染风险筛选值与管制值（基本项目）,第二类用地-筛选值","汞","2024-06-04","","","","","","","","","","","","0.5","","黄棕","2.8","工业用地","0.77","","","","mg/KG","38","","1","否",""]
["2024","06","04","新余市","渝水区","奉先德业(新余）医废处置有限公司","固废处置厂","7724|危险废物治理","土壤环境,其他","地下水井","国家标准","地下水质量标准(GB/T 14848-2017)","（表1）地下水质量常规指标及限值,Ⅲ类","铅","2024-06-04","","","","","","","","","","8","2.7","","","","","","<0.0025","","","","mg/L","0.01","","1","否",""]
["2024","06","04","新余市","渝水区","奉先德业(新余）医废处置有限公司","固废处置厂","7724|危险废物治理","土壤环境,其他","地下水井","国家标准","地下水质量标准(GB/T 14848-2017)","（表1）地下水质量常规指标及限值,Ⅱ类","pH","2024-06-04","","","","","","","","","","8","2.7","","","","","","6.9","","","","无量纲","8.5","6.5","1","否",""]
["2024","06","04","新余市","渝水区","奉先德业(新余）医废处置有限公司","固废处置厂","7724|危险废物治理","土壤环境,其他","土壤","国家标准","土壤环境质量建设用地土壤污染风险管控标准标准(试行)(GB36600-2018)","表1 建设用地土壤污染风险筛选值与管制值（基本项目）,第二类用地-筛选值","铜","2024-06-04","","","","","","","","","","","","0.5","","黄棕","2.8","工业用地","22","","","","mg/KG","18000","","1","否",""]
["2024","06","04","新余市","渝水区","奉先德业(新余）医废处置有限公司","固废处置厂","7724|危险废物治理","土壤环境,其他","土壤","","","","pH","2024-06-04","","","","","","","","","","","","0.5","","黄棕","2.8","工业用地","7.61","","","","无量纲","","","0","否",""]
["2024","06","04","新余市","渝水区","奉先德业(新余）医废处置有限公司","固废处置厂","7724|危险废物治理","土壤环境,其他","地下水井","国家标准","地下水质量标准(GB/T 14848-2017)","（表1）地下水质量常规指标及限值,Ⅲ类","铬（六价）","2024-06-04","","","","","","","","","","8","2.7","","","","","","<0.004","","","","mg/L","0.05","","1","否",""]
["2024","06","04","新余市","渝水区","奉先德业(新余）医废处置有限公司","固废处置厂","7724|危险废物治理","土壤环境,其他","地下水井","国家标准","地下水质量标准(GB/T 14848-2017)","（表1）地下水质量常规指标及限值,Ⅲ类","镉","2024-06-04","","","","","","","","","","8","2.7","","","","","","<0.0005","","","","mg/L","0.005","","1","否",""]
["2024","06","04","新余市","渝水区","奉先德业(新余）医废处置有限公司","固废处置厂","7724|危险废物治理","土壤环境,其他","地下水井","国家标准","地下水质量标准(GB/T 14848-2017)","（表1）地下水质量常规指标及限值,Ⅲ类","锌","2024-06-04","","","","","","","","","","8","2.7","","","","","","<0.05","","","","mg/L","1.0","","1","否",""]
["2024","06","04","新余市","渝水区","奉先德业(新余）医废处置有限公司","固废处置厂","7724|危险废物治理","土壤环境,其他","土壤","国家标准","土壤环境质量建设用地土壤污染风险管控标准标准(试行)(GB36600-2018)","表1 建设用地土壤污染风险筛选值与管制值（基本项目）,第二类用地-筛选值","镍 ","2024-06-04","","","","","","","","","","","","0.5","","黄棕","2.8","工业用地","28","","","","mg/KG","900","","1","否",""]
["2024","06","04","新余市","渝水区","奉先德业(新余）医废处置有限公司","固废处置厂","7724|危险废物治理","土壤环境,其他","地下水井","国家标准","地下水质量标准(GB/T 14848-2017)","（表1）地下水质量常规指标及限值,Ⅲ类","铜","2024-06-04","","","","","","","","","","8","2.7","","","","","","<0.05","","","","mg/L","1.00","","1","否",""]
["2024","06","04","新余市","渝水区","奉先德业(新余）医废处置有限公司","固废处置厂","7724|危险废物治理","土壤环境,其他","土壤","国家标准","土壤环境质量建设用地土壤污染风险管控标准标准(试行)(GB36600-2018)","表1 建设用地土壤污染风险筛选值与管制值（基本项目）,第二类用地-筛选值","镉","2024-06-04","","","","","","","","","","","","0.5","","黄棕","2.8","工业用地","0.14","","","","mg/KG","65","","1","否",""]
["2024","06","04","新余市","渝水区","奉先德业(新余）医废处置有限公司","固废处置厂","7724|危险废物治理","土壤环境,其他","地下水井","国家标准","地下水质量标准(GB/T 14848-2017)","（表1）地下水质量常规指标及限值,Ⅲ类","砷","2024-06-04","","","","","","","","","","8","2.7","","","","","","0.0006","","","","mg/L","0.01","","1","否",""]
["2024","06","04","新余市","渝水区","新余超能通新能源有限公司","工业企业","3841|锂离子电池制造","环境风险管控","土壤","国家标准","土壤环境质量建设用地土壤污染风险管控标准标准(试行)(GB36600-2018)","表1 建设用地土壤污染风险筛选值与管制值（基本项目）,第二类用地-筛选值","镉","2024-06-04","","","","","","","","","","","","0.5","","黄棕","3.5","工业用地","0.13","","","","mg/KG","65","","1","否",""]
["2024","06","04","新余市","渝水区","新余超能通新能源有限公司","工业企业","3841|锂离子电池制造","环境风险管控","土壤","国家标准","土壤环境质量建设用地土壤污染风险管控标准标准(试行)(GB36600-2018)","表1 建设用地土壤污染风险筛选值与管制值（基本项目）,第二类用地-筛选值","铬（六价）","2024-06-04","","","","","","","","","","","","0.5","","黄棕","3.5","工业用地","<0.5","","","","mg/KG","5.7","","1","否",""]
["2024","06","04","新余市","渝水区","新余超能通新能源有限公司","工业企业","3841|锂离子电池制造","环境风险管控","土壤","","","","锌","2024-06-04","","","","","","","","","","","","0.5","","黄棕","3.5","工业用地","78","","","","mg/KG","","","0","否",""]
["2024","06","04","新余市","渝水区","新余超能通新能源有限公司","工业企业","3841|锂离子电池制造","环境风险管控","土壤","国家标准","土壤环境质量建设用地土壤污染风险管控标准标准(试行)(GB36600-2018)","表1 建设用地土壤污染风险筛选值与管制值（基本项目）,第二类用地-筛选值","汞","2024-06-04","","","","","","","","","","","","0.5","","黄棕","3.5","工业用地","2.66","","","","mg/KG","38","","1","否",""]
["2024","06","04","新余市","渝水区","新余超能通新能源有限公司","工业企业","3841|锂离子电池制造","环境风险管控","土壤","国家标准","土壤环境质量建设用地土壤污染风险管控标准标准(试行)(GB36600-2018)","表1 建设用地土壤污染风险筛选值与管制值（基本项目）,第二类用地-筛选值","砷","2024-06-04","","","","","","","","","","","","0.5","","黄棕","3.5","工业用地","9.96","","","","mg/KG","60","","1","否",""]
["2024","06","04","新余市","渝水区","新余超能通新能源有限公司","工业企业","3841|锂离子电池制造","环境风险管控","土壤","国家标准","土壤环境质量建设用地土壤污染风险管控标准标准(试行)(GB36600-2018)","表1 建设用地土壤污染风险筛选值与管制值（基本项目）,第二类用地-筛选值","铅","2024-06-04","","","","","","","","","","","","0.5","","黄棕","3.5","工业用地","32.4","","","","mg/KG","800","","1","否",""]
["2024","06","04","新余市","渝水区","新余超能通新能源有限公司","工业企业","3841|锂离子电池制造","环境风险管控","土壤","","","","pH","2024-06-04","","","","","","","","","","","","0.5","","黄棕","3.5","工业用地","7.67","","","","无量纲","","","0","否",""]
["2024","06","04","新余市","渝水区","新余超能通新能源有限公司","工业企业","3841|锂离子电池制造","环境风险管控","土壤","国家标准","土壤环境质量建设用地土壤污染风险管控标准标准(试行)(GB36600-2018)","表1 建设用地土壤污染风险筛选值与管制值（基本项目）,第二类用地-筛选值","镍 ","2024-06-04","","","","","","","","","","","","0.5","","黄棕","3.5","工业用地","27","","","","mg/KG","900","","1","否",""]
["2024","06","04","新余市","渝水区","新余超能通新能源有限公司","工业企业","3841|锂离子电池制造","环境风险管控","土壤","国家标准","土壤环境质量建设用地土壤污染风险管控标准标准(试行)(GB36600-2018)","表1 建设用地土壤污染风险筛选值与管制值（基本项目）,第二类用地-筛选值","铜","2024-06-04","","","","","","","","","","","","0.5","","黄棕","3.5","工业用地","26","","","","mg/KG","18000","","1","否",""]
["2024","06","03","新余市","渝水区","新余闽鑫资源综合利用科技有限公司","工业企业","7724|危险废物治理","大气环境,土壤污染监管","厂区地下水","国家标准","地下水质量标准(GB/T 14848-2017)","（表1）地下水质量常规指标及限值,Ⅲ类","汞","2024-06-03","","","","","","","","","","8","3.4","","","","","","<0.00004","","","","mg/L","0.001","","1","否",""]
["2024","06","03","新余市","渝水区","新余闽鑫资源综合利用科技有限公司","工业企业","7724|危险废物治理","大气环境,土壤污染监管","厂区地下水","国家标准","地下水质量标准(GB/T 14848-2017)","（表1）地下水质量常规指标及限值,Ⅲ类","砷","2024-06-03","","","","","","","","","","8","3.4","","","","","","0.0006","","","","mg/L","0.01","","1","否",""]
["2024","06","03","新余市","渝水区","新余闽鑫资源综合利用科技有限公司","工业企业","7724|危险废物治理","大气环境,土壤污染监管","厂区地下水","国家标准","地下水质量标准(GB/T 14848-2017)","（表1）地下水质量常规指标及限值,Ⅲ类","铜","2024-06-03","","","","","","","","","","8","3.4","","","","","","<0.05","","","","mg/L","1.00","","1","否",""]
["2024","06","03","新余市","渝水区","新余闽鑫资源综合利用科技有限公司","工业企业","7724|危险废物治理","大气环境,土壤污染监管","厂区地下水","国家标准","地下水质量标准(GB/T 14848-2017)","（表2）地下水质量非常规指标及限值,Ⅲ类","镍 ","2024-06-03","","","","","","","","","","8","3.4","","","","","","<0.005","","","","mg/L","0.02","","1","否",""]
["2024","06","03","新余市","渝水区","新余闽鑫资源综合利用科技有限公司","工业企业","7724|危险废物治理","大气环境,土壤污染监管","厂区地下水","国家标准","地下水质量标准(GB/T 14848-2017)","（表1）地下水质量常规指标及限值,Ⅲ类","镉","2024-06-03","","","","","","","","","","8","3.4","","","","","","<0.0005","","","","mg/L","0.005","","1","否",""]
["2024","06","03","新余市","渝水区","新余闽鑫资源综合利用科技有限公司","工业企业","7724|危险废物治理","大气环境,土壤污染监管","厂区地下水","国家标准","地下水质量标准(GB/T14848-93)","表1地下水质量分类指标,Ⅲ类","高锰酸盐指数","2024-06-03","","","","","","","","","","8","3.4","","","","","","1.0","","","","mg/L","3.0","","1","否",""]
["2024","06","03","新余市","渝水区","新余闽鑫资源综合利用科技有限公司","工业企业","7724|危险废物治理","大气环境,土壤污染监管","厂区地下水","国家标准","地下水质量标准(GB/T 14848-2017)","（表1）地下水质量常规指标及限值,Ⅲ类","铁","2024-06-03","","","","","","","","","","8","3.4","","","","","","<0.03","","","","mg/L","0.3","","1","否",""]
["2024","06","03","新余市","渝水区","新余闽鑫资源综合利用科技有限公司","工业企业","7724|危险废物治理","大气环境,土壤污染监管","厂区土壤","","","","pH值","2024-06-03","","","","","","","","","","","","0.5","","黄棕","4.3","工业用地","7.52","","","","无量纲","8.5","6.5","1","否",""]
["2024","06","03","新余市","渝水区","新余闽鑫资源综合利用科技有限公司","工业企业","7724|危险废物治理","大气环境,土壤污染监管","厂区土壤","国家标准","土壤环境质量建设用地土壤污染风险管控标准标准(试行)(GB36600-2018)","表1 建设用地土壤污染风险筛选值与管制值（基本项目）,第二类用地-筛选值","镉","2024-06-03","","","","","","","","","","","","0.5","","黄棕","4.3","工业用地","0.14","","","","mg/KG","65","","1","否",""]
["2024","06","03","新余市","渝水区","新余闽鑫资源综合利用科技有限公司","工业企业","7724|危险废物治理","大气环境,土壤污染监管","厂区土壤","国家标准","土壤环境质量建设用地土壤污染风险管控标准标准(试行)(GB36600-2018)","表1 建设用地土壤污染风险筛选值与管制值（基本项目）,第二类用地-筛选值","铅","2024-06-03","","","","","","","","","","","","0.5","","黄棕","4.3","工业用地","23.6","","","","mg/KG","800","","1","否",""]
["2024","06","03","新余市","渝水区","新余闽鑫资源综合利用科技有限公司","工业企业","7724|危险废物治理","大气环境,土壤污染监管","厂区土壤","","","","锌","2024-06-03","","","","","","","","","","","","0.5","","黄棕","4.3","工业用地","57","","","","mg/KG","","","0","否",""]
["2024","06","03","新余市","渝水区","新余闽鑫资源综合利用科技有限公司","工业企业","7724|危险废物治理","大气环境,土壤污染监管","厂区地下水","国家标准","地下水质量标准(GB/T 14848-2017)","（表1）地下水质量常规指标及限值,Ⅲ类","铅","2024-06-03","","","","","","","","","","8","3.4","","","","","","0.0048","","","","mg/L","0.01","","1","否",""]
["2024","06","03","新余市","渝水区","新余闽鑫资源综合利用科技有限公司","工业企业","7724|危险废物治理","大气环境,土壤污染监管","厂区地下水","国家标准","地下水质量标准(GB/T 14848-2017)","（表1）地下水质量常规指标及限值,Ⅲ类","总锌","2024-06-03","","","","","","","","","","8","3.4","","","","","","<0.05","","","","mg/L","1.0","","1","否",""]
["2024","06","03","新余市","渝水区","新余闽鑫资源综合利用科技有限公司","工业企业","7724|危险废物治理","大气环境,土壤污染监管","厂区土壤","国家标准","土壤环境质量建设用地土壤污染风险管控标准标准(试行)(GB36600-2018)","表1 建设用地土壤污染风险筛选值与管制值（基本项目）,第二类用地-筛选值","镍 ","2024-06-03","","","","","","","","","","","","0.5","","黄棕","4.3","工业用地","38","","","","mg/KG","900","","1","否",""]
["2024","06","03","新余市","渝水区","新余闽鑫资源综合利用科技有限公司","工业企业","7724|危险废物治理","大气环境,土壤污染监管","厂区土壤","国家标准","土壤环境质量建设用地土壤污染风险管控标准标准(试行)(GB36600-2018)","表1 建设用地土壤污染风险筛选值与管制值（基本项目）,第二类用地-筛选值","砷","2024-06-03","","","","","","","","","","","","0.5","","黄棕","4.3","工业用地","6.66","","","","mg/KG","60","","1","否",""]
["2024","06","03","新余市","渝水区","新余闽鑫资源综合利用科技有限公司","工业企业","7724|危险废物治理","大气环境,土壤污染监管","厂区土壤","国家标准","土壤环境质量建设用地土壤污染风险管控标准标准(试行)(GB36600-2018)","表1 建设用地土壤污染风险筛选值与管制值（基本项目）,第二类用地-筛选值","铜","2024-06-03","","","","","","","","","","","","0.5","","黄棕","4.3","工业用地","20","","","","mg/KG","18000","","1","否",""]
["2024","06","03","新余市","渝水区","新余闽鑫资源综合利用科技有限公司","工业企业","7724|危险废物治理","大气环境,土壤污染监管","厂区地下水","国家标准","地下水质量标准(GB/T 14848-2017)","（表1）地下水质量常规指标及限值,Ⅲ类","氨氮","2024-06-03","","","","","","","","","","8","3.4","","","","","","0.044","","","","mg/L","0.5","","1","否",""]
["2024","06","03","新余市","渝水区","新余闽鑫资源综合利用科技有限公司","工业企业","7724|危险废物治理","大气环境,土壤污染监管","厂区地下水","国家标准","地下水质量标准(GB/T 14848-2017)","（表1）地下水质量常规指标及限值,Ⅲ类","锰","2024-06-03","","","","","","","","","","8","3.4","","","","","","<0.01","","","","mg/L","0.10","","1","否",""]
["2024","06","03","新余市","渝水区","新余闽鑫资源综合利用科技有限公司","工业企业","7724|危险废物治理","大气环境,土壤污染监管","厂区地下水","国家标准","地下水质量标准(GB/T 14848-2017)","（表1）地下水质量常规指标及限值,Ⅲ类","六价铬","2024-06-03","","","","","","","","","","8","3.4","","","","","","<0.004","","","","mg/L","0.05","","1","否",""]
["2024","06","03","新余市","渝水区","新余闽鑫资源综合利用科技有限公司","工业企业","7724|危险废物治理","大气环境,土壤污染监管","厂区土壤","国家标准","土壤环境质量建设用地土壤污染风险管控标准标准(试行)(GB36600-2018)","表1 建设用地土壤污染风险筛选值与管制值（基本项目）,第二类用地-筛选值","铬（六价）","2024-06-03","","","","","","","","","","","","0.5","","黄棕","4.3","工业用地","<0.5","","","","mg/KG","5.7","","1","否",""]
["2024","06","03","新余市","渝水区","新余闽鑫资源综合利用科技有限公司","工业企业","7724|危险废物治理","大气环境,土壤污染监管","厂区地下水","国家标准","地下水质量标准(GB/T 14848-2017)","（表1）地下水质量常规指标及限值,Ⅲ类","总硬度","2024-06-03","","","","","","","","","","8","3.4","","","","","","354","","","","mg/L","450","","1","否",""]
["2024","06","03","新余市","渝水区","新余闽鑫资源综合利用科技有限公司","工业企业","7724|危险废物治理","大气环境,土壤污染监管","厂区地下水","国家标准","地下水质量标准(GB/T 14848-2017)","（表1）地下水质量常规指标及限值,Ⅲ类","硒","2024-06-03","","","","","","","","","","8","3.4","","","","","","0.0004","","","","mg/L","0.01","","1","否",""]
["2024","06","03","新余市","渝水区","新余闽鑫资源综合利用科技有限公司","工业企业","7724|危险废物治理","大气环境,土壤污染监管","厂区土壤","国家标准","土壤环境质量建设用地土壤污染风险管控标准标准(试行)(GB36600-2018)","表1 建设用地土壤污染风险筛选值与管制值（基本项目）,第二类用地-筛选值","汞","2024-06-03","","","","","","","","","","","","0.5","","黄棕","4.3","工业用地","1.70","","","","mg/KG","38","","1","否",""]
["2024","06","03","新余市","渝水区","新余市环境卫生管理处（生活垃圾卫生填埋场）","固废处置厂","7820|环境卫生管理","水环境,地下水,环境风险管控","土壤","国家标准","土壤环境质量建设用地土壤污染风险管控标准标准(试行)(GB36600-2018)","表1 建设用地土壤污染风险筛选值与管制值（基本项目）,第二类用地-筛选值","镉","2024-06-03","","","","","","","","","","","","0.5","","黄棕","3.8","工业用地","0.20","","","","mg/KG","65","","1","否",""]
["2024","06","03","新余市","渝水区","新余市环境卫生管理处（生活垃圾卫生填埋场）","固废处置厂","7820|环境卫生管理","水环境,地下水,环境风险管控","1#井","国家标准","地下水质量标准(GB/T 14848-2017)","（表1）地下水质量常规指标及限值,Ⅲ类","硫酸盐","2024-06-03","","","","","","","","","","25","3.8","","","","","","21.6","","","","mg/L","250","","1","否",""]
["2024","06","03","新余市","渝水区","新余市环境卫生管理处（生活垃圾卫生填埋场）","固废处置厂","7820|环境卫生管理","水环境,地下水,环境风险管控","1#井","国家标准","地下水质量标准(GB/T 14848-2017)","（表1）地下水质量常规指标及限值,Ⅲ类","总硬度","2024-06-03","","","","","","","","","","25","3.8","","","","","","149","","","","mg/L","450","","1","否",""]
["2024","06","03","新余市","渝水区","新余市环境卫生管理处（生活垃圾卫生填埋场）","固废处置厂","7820|环境卫生管理","水环境,地下水,环境风险管控","1#井","国家标准","地下水质量标准(GB/T 14848-2017)","（表1）地下水质量常规指标及限值,Ⅲ类","铅","2024-06-03","","","","","","","","","","25","3.8","","","","","","0.0090","","","","mg/L","0.01","","1","否",""]
["2024","06","03","新余市","渝水区","新余市环境卫生管理处（生活垃圾卫生填埋场）","固废处置厂","7820|环境卫生管理","水环境,地下水,环境风险管控","1#井","国家标准","地下水质量标准(GB/T 14848-2017)","（表1）地下水质量常规指标及限值,Ⅲ类","氨氮","2024-06-03","","","","","","","","","","25","3.8","","","","","","0.102","","","","mg/L","0.5","","1","否",""]
["2024","06","03","新余市","渝水区","新余市环境卫生管理处（生活垃圾卫生填埋场）","固废处置厂","7820|环境卫生管理","水环境,地下水,环境风险管控","1#井","国家标准","地下水质量标准(GB/T 14848-2017)","（表1）地下水质量常规指标及限值,Ⅱ类","pH值","2024-06-03","","","","","","","","","","25","3.8","","","","","","6.9","","","","无量纲","8.5","6.5","1","否",""]
["2024","06","03","新余市","渝水区","新余市环境卫生管理处（生活垃圾卫生填埋场）","固废处置厂","7820|环境卫生管理","水环境,地下水,环境风险管控","土壤","国家标准","土壤环境质量建设用地土壤污染风险管控标准标准(试行)(GB36600-2018)","表1 建设用地土壤污染风险筛选值与管制值（基本项目）,第二类用地-筛选值","砷","2024-06-03","","","","","","","","","","","","0.5","","黄棕","3.8","工业用地","10.5","","","","mg/KG","60","","1","否",""]
["2024","06","03","新余市","渝水区","新余市环境卫生管理处（生活垃圾卫生填埋场）","固废处置厂","7820|环境卫生管理","水环境,地下水,环境风险管控","1#井","国家标准","地下水质量标准(GB/T 14848-2017)","（表1）地下水质量常规指标及限值,Ⅲ类","总大肠菌群","2024-06-03","","","","","","","","","","25","3.8","","","","","","<2","","","","MPN/100mL","3.0","","1","否",""]
["2024","06","03","新余市","渝水区","新余市环境卫生管理处（生活垃圾卫生填埋场）","固废处置厂","7820|环境卫生管理","水环境,地下水,环境风险管控","1#井","国家标准","地下水质量标准(GB/T 14848-2017)","（表1）地下水质量常规指标及限值,Ⅲ类","镉","2024-06-03","","","","","","","","","","25","3.8","","","","","","0.0018","","","","mg/L","0.005","","1","否",""]
["2024","06","03","新余市","渝水区","新余市环境卫生管理处（生活垃圾卫生填埋场）","固废处置厂","7820|环境卫生管理","水环境,地下水,环境风险管控","1#井","国家标准","地下水质量标准(GB/T 14848-2017)","（表1）地下水质量常规指标及限值,Ⅲ类","砷","2024-06-03","","","","","","","","","","25","3.8","","","","","","0.0006","","","","mg/L","0.01","","1","否",""]
["2024","06","03","新余市","渝水区","新余市环境卫生管理处（生活垃圾卫生填埋场）","固废处置厂","7820|环境卫生管理","水环境,地下水,环境风险管控","土壤","国家标准","土壤环境质量建设用地土壤污染风险管控标准标准(试行)(GB36600-2018)","表1 建设用地土壤污染风险筛选值与管制值（基本项目）,第二类用地-筛选值","汞","2024-06-03","","","","","","","","","","","","0.5","","黄棕","3.8","工业用地","1.02","","","","mg/KG","38","","1","否",""]
["2024","06","03","新余市","渝水区","新余市环境卫生管理处（生活垃圾卫生填埋场）","固废处置厂","7820|环境卫生管理","水环境,地下水,环境风险管控","土壤","","","","pH","2024-06-03","","","","","","","","","","","","0.5","","黄棕","3.8","工业用地","6.61","","","","无量纲","","","0","否",""]
["2024","06","03","新余市","渝水区","新余市环境卫生管理处（生活垃圾卫生填埋场）","固废处置厂","7820|环境卫生管理","水环境,地下水,环境风险管控","土壤","国家标准","土壤环境质量建设用地土壤污染风险管控标准标准(试行)(GB36600-2018)","表1 建设用地土壤污染风险筛选值与管制值（基本项目）,第二类用地-筛选值","铬（六价）","2024-06-03","","","","","","","","","","","","0.5","","黄棕","3.8","工业用地","<0.5","","","","mg/KG","5.7","","1","否",""]
["2024","06","03","新余市","渝水区","新余市环境卫生管理处（生活垃圾卫生填埋场）","固废处置厂","7820|环境卫生管理","水环境,地下水,环境风险管控","土壤","","","","锌","2024-06-03","","","","","","","","","","","","0.5","","黄棕","3.8","工业用地","141","","","","mg/KG","","","0","否",""]
["2024","06","03","新余市","渝水区","新余市环境卫生管理处（生活垃圾卫生填埋场）","固废处置厂","7820|环境卫生管理","水环境,地下水,环境风险管控","1#井","国家标准","地下水质量标准(GB/T 14848-2017)","（表1）地下水质量常规指标及限值,Ⅲ类","总锌","2024-06-03","","","","","","","","","","25","3.8","","","","","","<0.05","","","","mg/L","1.0","","1","否",""]
["2024","06","03","新余市","渝水区","新余市环境卫生管理处（生活垃圾卫生填埋场）","固废处置厂","7820|环境卫生管理","水环境,地下水,环境风险管控","1#井","国家标准","地下水质量标准(GB/T 14848-2017)","（表1）地下水质量常规指标及限值,Ⅲ类","耗氧量（COD法，以O2计）","2024-06-03","","","","","","","","","","25","3.8","","","","","","1.2","","","","mg/L","3.0","","1","否",""]
["2024","06","03","新余市","渝水区","新余市环境卫生管理处（生活垃圾卫生填埋场）","固废处置厂","7820|环境卫生管理","水环境,地下水,环境风险管控","1#井","国家标准","地下水质量标准(GB/T 14848-2017)","（表1）地下水质量常规指标及限值,Ⅲ类","铁","2024-06-03","","","","","","","","","","25","3.8","","","","","","<0.03","","","","mg/L","0.3","","1","否",""]
["2024","06","03","新余市","渝水区","新余市环境卫生管理处（生活垃圾卫生填埋场）","固废处置厂","7820|环境卫生管理","水环境,地下水,环境风险管控","1#井","国家标准","地下水质量标准(GB/T 14848-2017)","（表1）地下水质量常规指标及限值,Ⅲ类","硝酸盐","2024-06-03","","","","","","","","","","25","3.8","","","","","","2.53","","","","mg/L","20.0","","1","否",""]
["2024","06","03","新余市","渝水区","新余市环境卫生管理处（生活垃圾卫生填埋场）","固废处置厂","7820|环境卫生管理","水环境,地下水,环境风险管控","土壤","国家标准","土壤环境质量建设用地土壤污染风险管控标准标准(试行)(GB36600-2018)","表1 建设用地土壤污染风险筛选值与管制值（基本项目）,第二类用地-筛选值","镍 ","2024-06-03","","","","","","","","","","","","0.5","","黄棕","3.8","工业用地","48","","","","mg/KG","900","","1","否",""]
["2024","06","03","新余市","渝水区","新余市环境卫生管理处（生活垃圾卫生填埋场）","固废处置厂","7820|环境卫生管理","水环境,地下水,环境风险管控","1#井","","","","溶解性总固体","2024-06-03","","","","","","","","","","25","3.8","","","","","","311","","","","mg/L","1000","","1","否",""]
["2024","06","03","新余市","渝水区","新余市环境卫生管理处（生活垃圾卫生填埋场）","固废处置厂","7820|环境卫生管理","水环境,地下水,环境风险管控","1#井","国家标准","地下水质量标准(GB/T 14848-2017)","（表1）地下水质量常规指标及限值,Ⅲ类","铜","2024-06-03","","","","","","","","","","25","3.8","","","","","","<0.05","","","","mg/L","1.00","","1","否",""]
["2024","06","03","新余市","渝水区","新余市环境卫生管理处（生活垃圾卫生填埋场）","固废处置厂","7820|环境卫生管理","水环境,地下水,环境风险管控","1#井","国家标准","地下水质量标准(GB/T 14848-2017)","（表1）地下水质量常规指标及限值,Ⅲ类","汞","2024-06-03","","","","","","","","","","25","3.8","","","","","","<0.00004","","","","mg/L","0.001","","1","否",""]
["2024","06","03","新余市","渝水区","新余市环境卫生管理处（生活垃圾卫生填埋场）","固废处置厂","7820|环境卫生管理","水环境,地下水,环境风险管控","土壤","国家标准","土壤环境质量建设用地土壤污染风险管控标准标准(试行)(GB36600-2018)","表1 建设用地土壤污染风险筛选值与管制值（基本项目）,第二类用地-筛选值","铅","2024-06-03","","","","","","","","","","","","0.5","","黄棕","3.8","工业用地","61.5","","","","mg/KG","800","","1","否",""]
["2024","06","03","新余市","渝水区","新余市环境卫生管理处（生活垃圾卫生填埋场）","固废处置厂","7820|环境卫生管理","水环境,地下水,环境风险管控","1#井","国家标准","地下水质量标准(GB/T 14848-2017)","（表1）地下水质量常规指标及限值,Ⅲ类","氰化物","2024-06-03","","","","","","","","","","25","3.8","","","","","","<0.001","","","","mg/L","0.05","","1","否",""]
["2024","06","03","新余市","渝水区","新余市环境卫生管理处（生活垃圾卫生填埋场）","固废处置厂","7820|环境卫生管理","水环境,地下水,环境风险管控","1#井","国家标准","地下水质量标准(GB/T 14848-2017)","（表1）地下水质量常规指标及限值,Ⅲ类","六价铬","2024-06-03","","","","","","","","","","25","3.8","","","","","","<0.004","","","","mg/L","0.05","","1","否",""]
["2024","06","03","新余市","渝水区","新余市环境卫生管理处（生活垃圾卫生填埋场）","固废处置厂","7820|环境卫生管理","水环境,地下水,环境风险管控","1#井","国家标准","地下水质量标准(GB/T 14848-2017)","（表1）地下水质量常规指标及限值,Ⅲ类","挥发性酚类（以苯酚计）","2024-06-03","","","","","","","","","","25","3.8","","","","","","0.00195","","","","mg/L","0.002","","1","否",""]
["2024","06","03","新余市","渝水区","新余市环境卫生管理处（生活垃圾卫生填埋场）","固废处置厂","7820|环境卫生管理","水环境,地下水,环境风险管控","1#井","国家标准","地下水质量标准(GB/T 14848-2017)","（表1）地下水质量常规指标及限值,Ⅲ类","氯化物","2024-06-03","","","","","","","","","","25","3.8","","","","","","173","","","","mg/L","250","","1","否",""]
["2024","06","03","新余市","渝水区","新余市环境卫生管理处（生活垃圾卫生填埋场）","固废处置厂","7820|环境卫生管理","水环境,地下水,环境风险管控","土壤","国家标准","土壤环境质量建设用地土壤污染风险管控标准标准(试行)(GB36600-2018)","表1 建设用地土壤污染风险筛选值与管制值（基本项目）,第二类用地-筛选值","铜","2024-06-03","","","","","","","","","","","","0.5","","黄棕","3.8","工业用地","87","","","","mg/KG","18000","","1","否",""]
["2024","06","03","新余市","渝水区","新余市环境卫生管理处（生活垃圾卫生填埋场）","固废处置厂","7820|环境卫生管理","水环境,地下水,环境风险管控","1#井","国家标准","地下水质量标准(GB/T 14848-2017)","（表1）地下水质量常规指标及限值,Ⅲ类","锰","2024-06-03","","","","","","","","","","25","3.8","","","","","","<0.01","","","","mg/L","0.10","","1","否",""]
["2024","06","03","新余市","渝水区","新余市环境卫生管理处（生活垃圾卫生填埋场）","固废处置厂","7820|环境卫生管理","水环境,地下水,环境风险管控","1#井","国家标准","地下水质量标准(GB/T 14848-2017)","（表1）地下水质量常规指标及限值,Ⅲ类","氟化物","2024-06-03","","","","","","","","","","25","3.8","","","","","","0.465","","","","mg/L","1.0","","1","否",""]
["2024","06","03","新余市","渝水区","新余市环境卫生管理处（生活垃圾卫生填埋场）","固废处置厂","7820|环境卫生管理","水环境,地下水,环境风险管控","1#井","国家标准","地下水质量标准(GB/T 14848-2017)","（表1）地下水质量常规指标及限值,Ⅲ类","亚硝酸盐","2024-06-03","","","","","","","","","","25","3.8","","","","","","0.064","","","","mg/L","1.00","","1","否",""]
["2024","06","04","新余市","渝水区","新余市伟成金属制品有限公司","工业企业","3340|金属丝绳及其制品制造","水环境","土壤","国家标准","土壤环境质量建设用地土壤污染风险管控标准标准(试行)(GB36600-2018)","表1 建设用地土壤污染风险筛选值与管制值（基本项目）,第二类用地-筛选值","铜","2024-06-04","","","","","","","","","","","","0.5","","黄棕","3.9","工业用地","21","","","","mg/KG","18000","","1","否",""]
["2024","06","04","新余市","渝水区","新余市伟成金属制品有限公司","工业企业","3340|金属丝绳及其制品制造","水环境","土壤","国家标准","土壤环境质量建设用地土壤污染风险管控标准标准(试行)(GB36600-2018)","表1 建设用地土壤污染风险筛选值与管制值（基本项目）,第二类用地-筛选值","砷","2024-06-04","","","","","","","","","","","","0.5","","黄棕","3.9","工业用地","9.40","","","","mg/KG","60","","1","否",""]
["2024","06","04","新余市","渝水区","新余市伟成金属制品有限公司","工业企业","3340|金属丝绳及其制品制造","水环境","土壤","","","","pH","2024-06-04","","","","","","","","","","","","0.5","","黄棕","3.9","工业用地","5.60","","","","无量纲","","","0","否",""]
["2024","06","04","新余市","渝水区","新余市伟成金属制品有限公司","工业企业","3340|金属丝绳及其制品制造","水环境","土壤","国家标准","土壤环境质量建设用地土壤污染风险管控标准标准(试行)(GB36600-2018)","表1 建设用地土壤污染风险筛选值与管制值（基本项目）,第二类用地-筛选值","镉","2024-06-04","","","","","","","","","","","","0.5","","黄棕","3.9","工业用地","0.09","","","","mg/KG","65","","1","否",""]
["2024","06","04","新余市","渝水区","新余市伟成金属制品有限公司","工业企业","3340|金属丝绳及其制品制造","水环境","土壤","国家标准","土壤环境质量建设用地土壤污染风险管控标准标准(试行)(GB36600-2018)","表1 建设用地土壤污染风险筛选值与管制值（基本项目）,第二类用地-筛选值","铅","2024-06-04","","","","","","","","","","","","0.5","","黄棕","3.9","工业用地","12.4","","","","mg/KG","800","","1","否",""]
["2024","06","04","新余市","渝水区","新余市伟成金属制品有限公司","工业企业","3340|金属丝绳及其制品制造","水环境","土壤","国家标准","土壤环境质量建设用地土壤污染风险管控标准标准(试行)(GB36600-2018)","表1 建设用地土壤污染风险筛选值与管制值（基本项目）,第二类用地-筛选值","铬（六价）","2024-06-04","","","","","","","","","","","","0.5","","黄棕","3.9","工业用地","<0.5","","","","mg/KG","5.7","","1","否",""]
["2024","06","04","新余市","渝水区","新余市伟成金属制品有限公司","工业企业","3340|金属丝绳及其制品制造","水环境","土壤","国家标准","土壤环境质量建设用地土壤污染风险管控标准标准(试行)(GB36600-2018)","表1 建设用地土壤污染风险筛选值与管制值（基本项目）,第二类用地-筛选值","汞","2024-06-04","","","","","","","","","","","","0.5","","黄棕","3.9","工业用地","1.49","","","","mg/KG","38","","1","否",""]
["2024","06","04","新余市","渝水区","新余市伟成金属制品有限公司","工业企业","3340|金属丝绳及其制品制造","水环境","土壤","","","","锌","2024-06-04","","","","","","","","","","","","0.5","","黄棕","3.9","工业用地","58","","","","mg/KG","","","0","否",""]
["2024","06","04","新余市","渝水区","新余市伟成金属制品有限公司","工业企业","3340|金属丝绳及其制品制造","水环境","土壤","国家标准","土壤环境质量建设用地土壤污染风险管控标准标准(试行)(GB36600-2018)","表1 建设用地土壤污染风险筛选值与管制值（基本项目）,第二类用地-筛选值","镍 ","2024-06-04","","","","","","","","","","","","0.5","","黄棕","3.9","工业用地","28","","","","mg/KG","900","","1","否",""]
["2024","06","04","新余市","渝水区","新余市星泰新材料有限公司","工业企业","2614|有机化学原料制造","环境风险管控","地下水井","国家标准","地下水质量标准(GB/T 14848-2017)","（表2）地下水质量非常规指标及限值,Ⅲ类","镍 ","2024-06-04","","","","","","","","","","8","2.6","","","","","","<0.005","","","","mg/L","0.02","","1","否",""]
["2024","06","04","新余市","渝水区","新余市星泰新材料有限公司","工业企业","2614|有机化学原料制造","环境风险管控","土壤","国家标准","土壤环境质量建设用地土壤污染风险管控标准标准(试行)(GB36600-2018)","表1 建设用地土壤污染风险筛选值与管制值（基本项目）,第二类用地-筛选值","汞","2024-06-04","","","","","","","","","","","","0.5","","黄棕","3.9","工业用地","1.33","","","","mg/KG","38","","1","否",""]
["2024","06","04","新余市","渝水区","新余市星泰新材料有限公司","工业企业","2614|有机化学原料制造","环境风险管控","土壤","国家标准","土壤环境质量建设用地土壤污染风险管控标准标准(试行)(GB36600-2018)","表1 建设用地土壤污染风险筛选值与管制值（基本项目）,第二类用地-筛选值","铜","2024-06-04","","","","","","","","","","","","0.5","","黄棕","3.9","工业用地","24","","","","mg/KG","18000","","1","否",""]
["2024","06","04","新余市","渝水区","新余市星泰新材料有限公司","工业企业","2614|有机化学原料制造","环境风险管控","土壤","国家标准","土壤环境质量建设用地土壤污染风险管控标准标准(试行)(GB36600-2018)","表1 建设用地土壤污染风险筛选值与管制值（基本项目）,第二类用地-筛选值","铅","2024-06-04","","","","","","","","","","","","0.5","","黄棕","3.9","工业用地","13.0","","","","mg/KG","800","","1","否",""]
["2024","06","04","新余市","渝水区","新余市星泰新材料有限公司","工业企业","2614|有机化学原料制造","环境风险管控","地下水井","国家标准","地下水质量标准(GB/T 14848-2017)","（表1）地下水质量常规指标及限值,Ⅲ类","铜","2024-06-04","","","","","","","","","","8","2.6","","","","","","<0.05","","","","mg/L","1.00","","1","否",""]
["2024","06","04","新余市","渝水区","新余市星泰新材料有限公司","工业企业","2614|有机化学原料制造","环境风险管控","地下水井","国家标准","地下水质量标准(GB/T 14848-2017)","（表1）地下水质量常规指标及限值,Ⅲ类","镉","2024-06-04","","","","","","","","","","8","2.6","","","","","","<0.0005","","","","mg/L","0.005","","1","否",""]
["2024","06","04","新余市","渝水区","新余市星泰新材料有限公司","工业企业","2614|有机化学原料制造","环境风险管控","地下水井","国家标准","地下水质量标准(GB/T 14848-2017)","（表1）地下水质量常规指标及限值,Ⅲ类","pH","2024-06-04","","","","","","","","","","8","2.6","","","","","","7.1","","","","无量纲","8.5","6.5","1","否",""]
["2024","06","04","新余市","渝水区","新余市星泰新材料有限公司","工业企业","2614|有机化学原料制造","环境风险管控","地下水井","国家标准","地下水质量标准(GB/T 14848-2017)","（表1）地下水质量常规指标及限值,Ⅲ类","铅","2024-06-04","","","","","","","","","","8","2.6","","","","","","<0.0025","","","","mg/L","0.01","","1","否",""]
["2024","06","04","新余市","渝水区","新余市星泰新材料有限公司","工业企业","2614|有机化学原料制造","环境风险管控","土壤","","","","锌","2024-06-04","","","","","","","","","","","","0.5","","黄棕","3.9","工业用地","128","","","","mg/KG","","","0","否",""]
["2024","06","04","新余市","渝水区","新余市星泰新材料有限公司","工业企业","2614|有机化学原料制造","环境风险管控","土壤","国家标准","土壤环境质量建设用地土壤污染风险管控标准标准(试行)(GB36600-2018)","表1 建设用地土壤污染风险筛选值与管制值（基本项目）,第二类用地-筛选值","砷","2024-06-04","","","","","","","","","","","","0.5","","黄棕","3.9","工业用地","15.7","","","","mg/KG","60","","1","否",""]
["2024","06","04","新余市","渝水区","新余市星泰新材料有限公司","工业企业","2614|有机化学原料制造","环境风险管控","地下水井","国家标准","地下水质量标准(GB/T 14848-2017)","（表1）地下水质量常规指标及限值,Ⅲ类","铬（六价）","2024-06-04","","","","","","","","","","8","2.6","","","","","","0.008","","","","mg/L","0.05","","1","否",""]
["2024","06","04","新余市","渝水区","新余市星泰新材料有限公司","工业企业","2614|有机化学原料制造","环境风险管控","土壤","国家标准","土壤环境质量建设用地土壤污染风险管控标准标准(试行)(GB36600-2018)","表1 建设用地土壤污染风险筛选值与管制值（基本项目）,第二类用地-筛选值","镍 ","2024-06-04","","","","","","","","","","","","0.5","","黄棕","3.9","工业用地","54","","","","mg/KG","900","","1","否",""]
["2024","06","04","新余市","渝水区","新余市星泰新材料有限公司","工业企业","2614|有机化学原料制造","环境风险管控","土壤","国家标准","土壤环境质量建设用地土壤污染风险管控标准标准(试行)(GB36600-2018)","表1 建设用地土壤污染风险筛选值与管制值（基本项目）,第二类用地-筛选值","铬（六价）","2024-06-04","","","","","","","","","","","","0.5","","黄棕","3.9","工业用地","<0.5","","","","mg/KG","5.7","","1","否",""]
["2024","06","04","新余市","渝水区","新余市星泰新材料有限公司","工业企业","2614|有机化学原料制造","环境风险管控","地下水井","国家标准","地下水质量标准(GB/T 14848-2017)","（表1）地下水质量常规指标及限值,Ⅲ类","锌","2024-06-04","","","","","","","","","","8","2.6","","","","","","<0.05","","","","mg/L","1.0","","1","否",""]
["2024","06","04","新余市","渝水区","新余市星泰新材料有限公司","工业企业","2614|有机化学原料制造","环境风险管控","土壤","国家标准","土壤环境质量建设用地土壤污染风险管控标准标准(试行)(GB36600-2018)","表1 建设用地土壤污染风险筛选值与管制值（基本项目）,第二类用地-筛选值","镉","2024-06-04","","","","","","","","","","","","0.5","","黄棕","3.9","工业用地","0.10","","","","mg/KG","65","","1","否",""]
["2024","06","04","新余市","渝水区","新余市星泰新材料有限公司","工业企业","2614|有机化学原料制造","环境风险管控","土壤","","","","pH","2024-06-04","","","","","","","","","","","","0.5","","黄棕","3.9","工业用地","5.28","","","","无量纲","","","0","否",""]
["2024","06","04","新余市","渝水区","新余市星泰新材料有限公司","工业企业","2614|有机化学原料制造","环境风险管控","地下水井","国家标准","地下水质量标准(GB/T 14848-2017)","（表1）地下水质量常规指标及限值,Ⅲ类","汞","2024-06-04","","","","","","","","","","8","2.6","","","","","","<0.00004","","","","mg/L","0.001","","1","否",""]
["2024","06","04","新余市","渝水区","新余市星泰新材料有限公司","工业企业","2614|有机化学原料制造","环境风险管控","地下水井","国家标准","地下水质量标准(GB/T 14848-2017)","（表1）地下水质量常规指标及限值,Ⅲ类","砷","2024-06-04","","","","","","","","","","8","2.6","","","","","","0.0006","","","","mg/L","0.01","","1","否",""]
["2024","06","19","新余市","渝水区","新余益欣金属材料有限公司","工业企业","3360|金属表面处理及热处理加工","环境风险管控","项目地","地方标准","江西省地方标准《建设用地土壤污染风险管控标准》(DB36/1282-2020)","第二类用地筛选值","镍 ","2024-06-19","","","","","","","","","","","","0.2","","红褐色","","","24","","","","mg/KG","900","","1","否",""]
["2024","06","19","新余市","渝水区","新余益欣金属材料有限公司","工业企业","3360|金属表面处理及热处理加工","环境风险管控","项目地","地方标准","江西省地方标准《建设用地土壤污染风险管控标准》(DB36/1282-2020)","第二类用地筛选值","镉","2024-06-19","","","","","","","","","","","","0.2","","红褐色","","","<0.07","","","","mg/KG","65","","1","否",""]
["2024","06","19","新余市","渝水区","新余益欣金属材料有限公司","工业企业","3360|金属表面处理及热处理加工","环境风险管控","项目所在地","国家标准","地下水质量标准(GB/T 14848-2017)","（表1）地下水质量常规指标及限值,Ⅲ类","氨氮","2024-06-19","","","","","","","","","","6","58.2","","","","","","0.18","","","","mg/L","0.5","","1","否",""]
["2024","06","19","新余市","渝水区","新余益欣金属材料有限公司","工业企业","3360|金属表面处理及热处理加工","环境风险管控","项目地","地方标准","江西省地方标准《建设用地土壤污染风险管控标准》(DB36/1282-2020)","第二类用地筛选值","汞","2024-06-19","","","","","","","","","","","","0.2","","红褐色","","","0.020","","","","mg/KG","38","","1","否",""]
["2024","06","19","新余市","渝水区","新余益欣金属材料有限公司","工业企业","3360|金属表面处理及热处理加工","环境风险管控","项目地","地方标准","江西省地方标准《建设用地土壤污染风险管控标准》(DB36/1282-2020)","第二类用地筛选值","铬（六价）","2024-06-19","","","","","","","","","","","","0.2","","","","","<0.5","","","","mg/KG","5.7","","1","否",""]
["2024","06","19","新余市","渝水区","新余益欣金属材料有限公司","工业企业","3360|金属表面处理及热处理加工","环境风险管控","项目所在地","国家标准","地下水质量标准(GB/T 14848-2017)","（表1）地下水质量常规指标及限值,Ⅲ类","pH值","2024-06-19","","","","","","","","","","6","58.2","","","","","","7.8","","","","无量纲","8.5","6.5","1","否",""]
["2024","06","19","新余市","渝水区","新余益欣金属材料有限公司","工业企业","3360|金属表面处理及热处理加工","环境风险管控","项目地","地方标准","江西省地方标准《建设用地土壤污染风险管控标准》(DB36/1282-2020)","第二类用地筛选值","铜","2024-06-19","","","","","","","","","","","","0.2","","红褐色","","","25.1","","","","mg/KG","18000","","1","否",""]
["2024","06","19","新余市","渝水区","新余益欣金属材料有限公司","工业企业","3360|金属表面处理及热处理加工","环境风险管控","项目地","地方标准","江西省地方标准《建设用地土壤污染风险管控标准》(DB36/1282-2020)","第二类用地筛选值","铅","2024-06-19","","","","","","","","","","","","0.2","","红褐色","","","28","","","","mg/KG","800","","1","否",""]
["2024","06","19","新余市","渝水区","新余益欣金属材料有限公司","工业企业","3360|金属表面处理及热处理加工","环境风险管控","项目地","地方标准","江西省地方标准《建设用地土壤污染风险管控标准》(DB36/1282-2020)","第二类用地筛选值","砷","2024-06-19","","","","","","","","","","","","0.2","","红褐色","","","12.6","","","","mg/KG","60","","1","否",""]
["2024","06","19","新余市","渝水区","新余益欣金属材料有限公司","工业企业","3360|金属表面处理及热处理加工","环境风险管控","项目所在地","国家标准","地下水质量标准(GB/T 14848-2017)","（表1）地下水质量常规指标及限值,Ⅲ类","氯化物","2024-06-19","","","","","","","","","","6","58.2","","","","","","18.5","","","","mg/L","250","","1","否",""]
["2024","06","19","新余市","渝水区","新余益欣金属材料有限公司","工业企业","3360|金属表面处理及热处理加工","环境风险管控","项目所在地","国家标准","地下水质量标准(GB/T 14848-2017)","（表1）地下水质量常规指标及限值,Ⅱ类","总锌","2024-06-19","","","","","","","","","","6","58.2","","","","","","0.0148","","","","mg/L","1.0","","1","否",""]
["2024","06","19","新余市","渝水区","新余益欣金属材料有限公司","工业企业","3360|金属表面处理及热处理加工","环境风险管控","项目所在地","国家标准","地下水质量标准(GB/T 14848-2017)","（表1）地下水质量常规指标及限值,Ⅲ类","耗氧量（COD法，以O2计）","2024-06-19","","","","","","","","","","6","58.2","","","","","","2.6","","","","mg/L","3.0","","1","否",""]
["2024","06","03","新余市","渝水区","新余永清环保能源有限公司","固废处置厂","4417-1|生物质能发电-生活垃圾焚烧发电","水环境,土壤污染监管","地下水井","国家标准","地下水质量标准(GB/T 14848-2017)","（表1）地下水质量常规指标及限值,Ⅲ类","氯化物","2024-06-03","","","","","","","","","","30","5.6","","","","","","4.17","","","","mg/L","250","","1","否",""]
["2024","06","03","新余市","渝水区","新余永清环保能源有限公司","固废处置厂","4417-1|生物质能发电-生活垃圾焚烧发电","水环境,土壤污染监管","土壤","国家标准","土壤环境质量建设用地土壤污染风险管控标准标准(试行)(GB36600-2018)","表1 建设用地土壤污染风险筛选值与管制值（基本项目）,第二类用地-筛选值","镍 ","2024-06-03","","","","","","","","","","","","0.5","","黄棕","2.2","工业用地","48","","","","mg/KG","900","","1","否",""]
["2024","06","03","新余市","渝水区","新余永清环保能源有限公司","固废处置厂","4417-1|生物质能发电-生活垃圾焚烧发电","水环境,土壤污染监管","地下水井","国家标准","地下水质量标准(GB/T 14848-2017)","（表1）地下水质量常规指标及限值,Ⅲ类","亚硝酸盐","2024-06-03","","","","","","","","","","30","5.6","","","","","","<0.016","","","","mg/L","1.00","","1","否",""]
["2024","06","03","新余市","渝水区","新余永清环保能源有限公司","固废处置厂","4417-1|生物质能发电-生活垃圾焚烧发电","水环境,土壤污染监管","土壤","国家标准","土壤环境质量建设用地土壤污染风险管控标准标准(试行)(GB36600-2018)","表2 建设用地土壤污染风险筛选值与管制值（基本项目）,第二类用地-筛选值","二噁英类（总毒性当量）","2024-06-03","","","","","","","","","","","","0.5","","黄棕","2.2","工业用地","2.4","","","","ngTEQ/kg","40","","1","否",""]
["2024","06","03","新余市","渝水区","新余永清环保能源有限公司","固废处置厂","4417-1|生物质能发电-生活垃圾焚烧发电","水环境,土壤污染监管","土壤","国家标准","土壤环境质量建设用地土壤污染风险管控标准标准(试行)(GB36600-2018)","表1 建设用地土壤污染风险筛选值与管制值（基本项目）,第二类用地-筛选值","铜","2024-06-03","","","","","","","","","","","","0.5","","黄棕","2.2","工业用地","43","","","","mg/KG","18000","","1","否",""]
["2024","06","03","新余市","渝水区","新余永清环保能源有限公司","固废处置厂","4417-1|生物质能发电-生活垃圾焚烧发电","水环境,土壤污染监管","地下水井","国家标准","地下水质量标准(GB/T 14848-2017)","（表1）地下水质量常规指标及限值,Ⅲ类","pH","2024-06-03","","","","","","","","","","30","5.6","","","","","","7.0","","","","无量纲","8.5","6.5","1","否",""]
["2024","06","03","新余市","渝水区","新余永清环保能源有限公司","固废处置厂","4417-1|生物质能发电-生活垃圾焚烧发电","水环境,土壤污染监管","土壤","国家标准","土壤环境质量建设用地土壤污染风险管控标准标准(试行)(GB36600-2018)","表1 建设用地土壤污染风险筛选值与管制值（基本项目）,第二类用地-筛选值","镉","2024-06-03","","","","","","","","","","","","0.5","","黄棕","2.2","工业用地","0.10","","","","mg/KG","65","","1","否",""]
["2024","06","03","新余市","渝水区","新余永清环保能源有限公司","固废处置厂","4417-1|生物质能发电-生活垃圾焚烧发电","水环境,土壤污染监管","土壤","国家标准","土壤环境质量建设用地土壤污染风险管控标准标准(试行)(GB36600-2018)","表1 建设用地土壤污染风险筛选值与管制值（基本项目）,第二类用地-筛选值","砷","2024-06-03","","","","","","","","","","","","0.5","","黄棕","2.2","工业用地","11.8","","","","mg/KG","60","","1","否",""]
["2024","06","03","新余市","渝水区","新余永清环保能源有限公司","固废处置厂","4417-1|生物质能发电-生活垃圾焚烧发电","水环境,土壤污染监管","地下水井","国家标准","地下水质量标准(GB/T 14848-2017)","（表1）地下水质量常规指标及限值,Ⅲ类","耗氧量（COD法，以O2计）","2024-06-03","","","","","","","","","","30","5.6","","","","","","1.6","","","","mg/L","3.0","","1","否",""]
["2024","06","03","新余市","渝水区","新余永清环保能源有限公司","固废处置厂","4417-1|生物质能发电-生活垃圾焚烧发电","水环境,土壤污染监管","土壤","","","","铬","2024-06-03","","","","","","","","","","","","0.5","","黄棕","2.2","工业用地","37","","","","mg/KG","","","0","否",""]
["2024","06","03","新余市","渝水区","新余永清环保能源有限公司","固废处置厂","4417-1|生物质能发电-生活垃圾焚烧发电","水环境,土壤污染监管","地下水井","国家标准","地下水质量标准(GB/T 14848-2017)","（表1）地下水质量常规指标及限值,Ⅲ类","汞","2024-06-03","","","","","","","","","","30","5.6","","","","","","<0.00004","","","","mg/L","0.001","","1","否",""]
["2024","06","03","新余市","渝水区","新余永清环保能源有限公司","固废处置厂","4417-1|生物质能发电-生活垃圾焚烧发电","水环境,土壤污染监管","地下水井","国家标准","地下水质量标准(GB/T 14848-2017)","（表1）地下水质量常规指标及限值,Ⅲ类","氨氮","2024-06-03","","","","","","","","","","30","5.6","","","","","","0.104","","","","mg/L","0.5","","1","否",""]
["2024","06","03","新余市","渝水区","新余永清环保能源有限公司","固废处置厂","4417-1|生物质能发电-生活垃圾焚烧发电","水环境,土壤污染监管","土壤","国家标准","土壤环境质量建设用地土壤污染风险管控标准标准(试行)(GB36600-2018)","表1 建设用地土壤污染风险筛选值与管制值（基本项目）,第二类用地-筛选值","汞","2024-06-03","","","","","","","","","","","","0.5","","黄棕","2.2","工业用地","0.58","","","","mg/KG","38","","1","否",""]
["2024","06","03","新余市","渝水区","新余永清环保能源有限公司","固废处置厂","4417-1|生物质能发电-生活垃圾焚烧发电","水环境,土壤污染监管","土壤","国家标准","土壤环境质量建设用地土壤污染风险管控标准标准(试行)(GB36600-2018)","表1 建设用地土壤污染风险筛选值与管制值（基本项目）,第二类用地-筛选值","铅","2024-06-03","","","","","","","","","","","","0.5","","黄棕","2.2","工业用地","14.1","","","","mg/KG","800","","1","否",""]
["2024","06","03","新余市","渝水区","新余永清环保能源有限公司","固废处置厂","4417-1|生物质能发电-生活垃圾焚烧发电","水环境,土壤污染监管","地下水井","国家标准","地下水质量标准(GB/T 14848-2017)","（表1）地下水质量常规指标及限值,Ⅲ类","硝酸盐（以N计）","2024-06-03","","","","","","","","","","30","5.6","","","","","","2.06","","","","mg/L","20.0","","1","否",""]
["2024","06","03","新余市","渝水区","新余永清环保能源有限公司","固废处置厂","4417-1|生物质能发电-生活垃圾焚烧发电","水环境,土壤污染监管","地下水井","国家标准","地下水质量标准(GB/T 14848-2017)","（表1）地下水质量常规指标及限值,Ⅲ类","砷","2024-06-03","","","","","","","","","","30","5.6","","","","","","0.0006","","","","mg/L","0.01","","1","否",""]
["2024","06","03","新余市","渝水区","新余永清环保能源有限公司","固废处置厂","4417-1|生物质能发电-生活垃圾焚烧发电","水环境,土壤污染监管","地下水井","国家标准","地下水质量标准(GB/T 14848-2017)","（表1）地下水质量常规指标及限值,Ⅲ类","镉","2024-06-03","","","","","","","","","","30","5.6","","","","","","<0.0005","","","","mg/L","0.005","","1","否",""]
["2024","06","03","新余市","渝水区","新余永清环保能源有限公司","固废处置厂","4417-1|生物质能发电-生活垃圾焚烧发电","水环境,土壤污染监管","地下水井","国家标准","地下水质量标准(GB/T 14848-2017)","（表1）地下水质量常规指标及限值,Ⅲ类","铅","2024-06-03","","","","","","","","","","30","5.6","","","","","","<0.0025","","","","mg/L","0.01","","1","否",""]
["2024","06","23","新余市","","新余海顺环保科技有限公司","工业企业","4190|其他未列明制造业","环境风险管控","棱里 安置 小区3 #监测 井","国家标准","地下水质量标准(GB/T 14848-2017)","（表1）地下水质量常规指标及限值,Ⅲ类","总硬度","2024-06-23","","","","","","","","","","","","","","","","","38","","","","mg/L","450","","1","否",""]
["2024","06","23","新余市","","新余海顺环保科技有限公司","工业企业","4190|其他未列明制造业","环境风险管控","棱里 安置 小区3 #监测 井","国家标准","地下水质量标准(GB/T 14848-2017)","（表1）地下水质量常规指标及限值,Ⅲ类","氨氮","2024-06-23","","","","","","","","","","","","","","","","","0.04","","","","mg/L","0.5","","1","否",""]
["2024","06","23","新余市","","新余海顺环保科技有限公司","工业企业","4190|其他未列明制造业","环境风险管控","棱里 安置 小区3 #监测 井","国家标准","地下水质量标准(GB/T 14848-2017)","（表1）地下水质量常规指标及限值,Ⅲ类","苯","2024-06-23","","","","","","","","","","","","","","","","","<0.0014","","","","mg/L","0.01","","1","否",""]
["2024","06","23","新余市","","新余海顺环保科技有限公司","工业企业","4190|其他未列明制造业","环境风险管控","棱里 安置 小区3 #监测 井","国家标准","地下水质量标准(GB/T 14848-2017)","（表1）地下水质量常规指标及限值,Ⅱ类","pH值","2024-06-23","","","","","","","","","","","","","","","","","7.8","","","","无量纲","8.5","6.5","1","否",""]
["2024","06","23","新余市","","新余海顺环保科技有限公司","工业企业","4190|其他未列明制造业","环境风险管控","棱里 安置 小区3 #监测 井","国家标准","地下水质量标准(GB/T 14848-2017)","（表1）地下水质量常规指标及限值,Ⅲ类","溶解性总固体","2024-06-23","","","","","","","","","","","","","","","","","151","","","","mg/L","1000","","1","否",""]
["2024","06","23","新余市","","新余海顺环保科技有限公司","工业企业","4190|其他未列明制造业","环境风险管控","棱里 安置 小区3 #监测 井","国家标准","地下水质量标准(GB/T 14848-2017)","（表1）地下水质量常规指标及限值,Ⅲ类","氯化物","2024-06-23","","","","","","","","","","","","","","","","","3.02","","","","mg/L","250","","1","否",""]
["2024","06","23","新余市","","新余海顺环保科技有限公司","工业企业","4190|其他未列明制造业","环境风险管控","棱里 安置 小区3 #监测 井","国家标准","地下水质量标准(GB/T 14848-2017)","（表1）地下水质量常规指标及限值,Ⅲ类","甲苯","2024-06-23","","","","","","","","","","","","","","","","","<0.0014","","","","mg/L","0.7","","1","否",""]
["2024","06","23","新余市","","新余海顺环保科技有限公司","工业企业","4190|其他未列明制造业","环境风险管控","棱里 安置 小区3 #监测 井","国家标准","地下水质量标准(GB/T 14848-2017)","（表1）地下水质量常规指标及限值,Ⅲ类","硫酸盐","2024-06-23","","","","","","","","","","","","","","","","","1.40","","","","mg/L","250","","1","否",""]
["2024","06","23","新余市","","新余海顺环保科技有限公司","工业企业","4190|其他未列明制造业","环境风险管控","棱里 安置 小区3 #监测 井","","","","石油类","2024-06-23","","","","","","","","","","","","","","","","","<0.01","","","","mg/L","","","0","否",""]
["2024","06","23","新余市","","新余海顺环保科技有限公司","工业企业","4190|其他未列明制造业","环境风险管控","棱里 安置 小区3 #监测 井","国家标准","地下水质量标准(GB/T 14848-2017)","（表1）地下水质量常规指标及限值,Ⅲ类","耗氧量（COD法，以O2计）","2024-06-23","","","","","","","","","","","","","","","","","<0.5","","","","mg/L","3.0","","1","否",""]
["2024","06","21","新余市","","新余市郁海环保科技有限公司","工业企业","7724|危险废物治理","环境风险管控","地下水监测井（厂区）","国家标准","地下水质量标准(GB/T 14848-2017)","（表1）地下水质量常规指标及限值,Ⅲ类","氨氮","2024-06-21","","","","","","","","","","5.48","58.17","","","","","","0.16","","","","mg/L","0.5","","1","否",""]
["2024","06","21","新余市","","新余市郁海环保科技有限公司","工业企业","7724|危险废物治理","环境风险管控","地下水监测井（厂区）","国家标准","地下水质量标准(GB/T 14848-2017)","（表1）地下水质量常规指标及限值,Ⅲ类","耗氧量（COD法，以O2计）","2024-06-21","","","","","","","","","","5.48","58.17","","","","","","1.2","","","","mg/L","3.0","","1","否",""]
["2024","06","21","新余市","","新余市郁海环保科技有限公司","工业企业","7724|危险废物治理","环境风险管控","地下水监测井（厂区）","国家标准","地下水质量标准(GB/T 14848-2017)","（表1）地下水质量常规指标及限值,Ⅲ类","pH值","2024-06-21","","","","","","","","","","5.48","58.17","","","","","","7.3","","","","无量纲","8.5","6.5","1","否",""]
["2024","06","21","新余市","","新余市郁海环保科技有限公司","工业企业","7724|危险废物治理","环境风险管控","地下水监测井（厂区）","国家标准","地下水质量标准(GB/T 14848-2017)","（表1）地下水质量常规指标及限值,Ⅲ类","硫酸盐","2024-06-21","","","","","","","","","","5.48","58.17","","","","","","17.4","","","","mg/L","250","","1","否",""]
["2024","06","21","新余市","","新余市郁海环保科技有限公司","工业企业","7724|危险废物治理","环境风险管控","地下水监测井（厂区）","国家标准","地下水质量标准(GB/T 14848-2017)","（表1）地下水质量常规指标及限值,Ⅲ类","铅","2024-06-21","","","","","","","","","","5.48","58.17","","","","","","<0.00009","","","","mg/L","0.01","","1","否",""]
["2024","06","21","新余市","","新余市郁海环保科技有限公司","工业企业","7724|危险废物治理","环境风险管控","项目地\t","地方标准","江西省地方标准《建设用地土壤污染风险管控标准》(DB36/1282-2020)","第二类用地筛选值","铅","2024-06-21","","","","","","","","","","","","0.2","","红褐色","","","26","","","","mg/KG","800","","1","否",""]

{"sheet":"噪声","index":3,"n_rows":66,"n_cols":24,"rows_kept":66,"merged":[[0,0,0,23]],"flags":["formulas_cached_only"]}
["执法监测厂界噪声数据",null,"","","","","","","","","","","","","","","","","","","","","",""]
["监测年","监测月","监测日","市","县","企业名称","企业类别","行业类别","名录类别","监测点名称","排放标准类型","排放标准名称","标准条目","噪声声源","噪声风速","监测项目","项目监测日期","噪声监测结果","噪声监测结果(夜间)","取值单位","排放上限","排放下限","是否超标","超标倍数"]
["2024","06","04","新余市","渝水区","奉先德业(新余）医废处置有限公司","固废处置厂","7724|危险废物治理","土壤环境,其他","厂界噪声南","国家标准","工业企业厂界环境噪声排放标准(GB12348-2008)","（表1）工业企业厂界环境噪声排放限值,厂界与噪声敏感建筑物距离不小于1m,2类厂界外声环境功能区,昼间/夜间","生产噪声","2","工业企业厂界环境噪声","2024-06-04","53.6","42.9","dB","60;50","","否",""]
["2024","06","04","新余市","渝水区","奉先德业(新余）医废处置有限公司","固废处置厂","7724|危险废物治理","土壤环境,其他","厂界噪声西","国家标准","工业企业厂界环境噪声排放标准(GB12348-2008)","（表1）工业企业厂界环境噪声排放限值,厂界与噪声敏感建筑物距离不小于1m,2类厂界外声环境功能区,昼间/夜间","生产噪声","2","工业企业厂界环境噪声","2024-06-04","52.2","47","dB","60;50","","否",""]
["2024","06","04","新余市","渝水区","奉先德业(新余）医废处置有限公司","固废处置厂","7724|危险废物治理","土壤环境,其他","厂界噪声北","国家标准","工业企业厂界环境噪声排放标准(GB12348-2008)","（表1）工业企业厂界环境噪声排放限值,厂界与噪声敏感建筑物距离不小于1m,2类厂界外声环境功能区,昼间/夜间","生产噪声","2","工业企业厂界环境噪声","2024-06-04","53.4","47.8","dB","60;50","","否",""]
["2024","06","04","新余市","渝水区","奉先德业(新余）医废处置有限公司","固废处置厂","7724|危险废物治理","土壤环境,其他","厂界噪声东","国家标准","工业企业厂界环境噪声排放标准(GB12348-2008)","（表1）工业企业厂界环境噪声排放限值,厂界与噪声敏感建筑物距离不小于1m,2类厂界外声环境功能区,昼间/夜间","生产噪声","2","工业企业厂界环境噪声","2024-06-04","52.1","42.5","dB","60;50","","否",""]
["2024","06","04","新余市","渝水区","新余超能通新能源有限公司","工业企业","3841|锂离子电池制造","环境风险管控","厂界北","国家标准","工业企业厂界环境噪声排放标准(GB12348-2008)","（表1）工业企业厂界环境噪声排放限值,厂界与噪声敏感建筑物距离不小于1m,2类厂界外声环境功能区,昼间/夜间","生产噪声","2.1","工业企业厂界环境噪声","2024-06-04","53.6","48.2","dB","60;50","","否",""]
["2024","06","04","新余市","渝水区","新余超能通新能源有限公司","工业企业","3841|锂离子电池制造","环境风险管控","厂界东","国家标准","工业企业厂界环境噪声排放标准(GB12348-2008)","（表1）工业企业厂界环境噪声排放限值,厂界与噪声敏感建筑物距离不小于1m,2类厂界外声环境功能区,昼间/夜间","生产噪声","2.1","工业企业厂界环境噪声","2024-06-04","56.9","43.9","dB","60;50","","否",""]
["2024","06","04","新余市","渝水区","新余超能通新能源有限公司","工业企业","3841|锂离子电池制造","环境风险管控","厂界西","国家标准","工业企业厂界环境噪声排放标准(GB12348-2008)","（表1）工业企业厂界环境噪声排放限值,厂界与噪声敏感建筑物距离不小于1m,2类厂界外声环境功能区,昼间/夜间","生产噪声","2.1","工业企业厂界环境噪声","2024-06-04","53.3","47.8","dB","60;50","","否",""]
["2024","06","04","新余市","渝水区","新余超能通新能源有限公司","工业企业","3841|锂离子电池制造","环境风险管控","厂界南","国家标准","工业企业厂界环境噪声排放标准(GB12348-2008)","（表1）工业企业厂界环境噪声排放限值,厂界与噪声敏感建筑物距离不小于1m,2类厂界外声环境功能区,昼间/夜间","生产噪声","2.1","工业企业厂界环境噪声","2024-06-04","53.8","47.9","dB","60;50","","否",""]
["2024","06","03","新余市","渝水区","新余闽鑫资源综合利用科技有限公司","工业企业","7724|危险废物治理","大气环境,土壤污染监管","厂界南","国家标准","工业企业厂界环境噪声排放标准(GB12348-2008)","（表1）工业企业厂界环境噪声排放限值,厂界与噪声敏感建筑物距离不小于1m,3类厂界外声环境功能区,昼间/夜间","生产噪声","2.1","工业企业厂界环境噪声","2024-06-03","52.6","47.9","dB","65;55","","否",""]
["2024","06","03","新余市","渝水区","新余闽鑫资源综合利用科技有限公司","工业企业","7724|危险废物治理","大气环境,土壤污染监管","厂界东","国家标准","工业企业厂界环境噪声排放标准(GB12348-2008)","（表1）工业企业厂界环境噪声排放限值,厂界与噪声敏感建筑物距离不小于1m,3类厂界外声环境功能区,昼间/夜间","生产噪声","2.1","工业企业厂界环境噪声","2024-06-03","56.3","47.9","dB","65;55","","否",""]
["2024","06","03","新余市","渝水区","新余闽鑫资源综合利用科技有限公司","工业企业","7724|危险废物治理","大气环境,土壤污染监管","厂界北","国家标准","工业企业厂界环境噪声排放标准(GB12348-2008)","（表1）工业企业厂界环境噪声排放限值,厂界与噪声敏感建筑物距离不小于1m,3类厂界外声环境功能区,昼间/夜间","生产噪声","2.1","工业企业厂界环境噪声","2024-06-03","55.3","47.7","dB","65;55","","否",""]
["2024","06","03","新余市","渝水区","新余闽鑫资源综合利用科技有限公司","工业企业","7724|危险废物治理","大气环境,土壤污染监管","厂界西","国家标准","工业企业厂界环境噪声排放标准(GB12348-2008)","（表1）工业企业厂界环境噪声排放限值,厂界与噪声敏感建筑物距离不小于1m,3类厂界外声环境功能区,昼间/夜间","生产噪声","2.1","工业企业厂界环境噪声","2024-06-03","51.6","47.8","dB","65;55","","否",""]
["2024","06","20","新余市","渝水区","新余市钢城实业有限公司","工业企业","3340|金属丝绳及其制品制造","环境风险管控","厂界噪声北面","国家标准","工业企业厂界环境噪声排放标准(GB12348-2008)","（表1）工业企业厂界环境噪声排放限值,厂界与噪声敏感建筑物距离不小于1m,3类厂界外声环境功能区,昼间/夜间","厂区设备","3.1","工业企业厂界环境噪声","2024-06-20","56.6","48.8","dB","65;55","","否",""]
["2024","06","20","新余市","渝水区","新余市钢城实业有限公司","工业企业","3340|金属丝绳及其制品制造","环境风险管控","厂界噪声西面","国家标准","工业企业厂界环境噪声排放标准(GB12348-2008)","（表1）工业企业厂界环境噪声排放限值,厂界与噪声敏感建筑物距离不小于1m,3类厂界外声环境功能区,昼间/夜间","厂区设备","3.1","工业企业厂界环境噪声","2024-06-20","58.5","47.4","dB","65;55","","否",""]
["2024","06","20","新余市","渝水区","新余市钢城实业有限公司","工业企业","3340|金属丝绳及其制品制造","环境风险管控","厂界噪声南面","国家标准","工业企业厂界环境噪声排放标准(GB12348-2008)","（表1）工业企业厂界环境噪声排放限值,厂界与噪声敏感建筑物距离不小于1m,3类厂界外声环境功能区,昼间/夜间","厂区设备","3.1","工业企业厂界环境噪声","2024-06-20","59","48","dB","65;55","","否",""]
["2024","06","20","新余市","渝水区","新余市钢城实业有限公司","工业企业","3340|金属丝绳及其制品制造","环境风险管控","厂界噪声东面","国家标准","工业企业厂界环境噪声排放标准(GB12348-2008)","（表1）工业企业厂界环境噪声排放限值,厂界与噪声敏感建筑物距离不小于1m,3类厂界外声环境功能区,昼间/夜间","厂区设备","3.1","工业企业厂界环境噪声","2024-06-20","57.7","48.1","dB","65;55","","否",""]
["2024","06","03","新余市","渝水区","新余市环境卫生管理处（生活垃圾卫生填埋场）","固废处置厂","7820|环境卫生管理","水环境,地下水,环境风险管控","厂界噪声南","国家标准","工业企业厂界环境噪声排放标准(GB12348-2008)","（表1）工业企业厂界环境噪声排放限值,厂界与噪声敏感建筑物距离不小于1m,2类厂界外声环境功能区,昼间/夜间","生产噪声","2.2","工业企业厂界环境噪声","2024-06-03","52.1","47.1","dB","60;50","","否",""]
["2024","06","03","新余市","渝水区","新余市环境卫生管理处（生活垃圾卫生填埋场）","固废处置厂","7820|环境卫生管理","水环境,地下水,环境风险管控","厂界噪声东","国家标准","工业企业厂界环境噪声排放标准(GB12348-2008)","（表1）工业企业厂界环境噪声排放限值,厂界与噪声敏感建筑物距离不小于1m,2类厂界外声环境功能区,昼间/夜间","生产噪声","2.2","工业企业厂界环境噪声","2024-06-03","52","47.4","dB","60;50","","否",""]
["2024","06","03","新余市","渝水区","新余市环境卫生管理处（生活垃圾卫生填埋场）","固废处置厂","7820|环境卫生管理","水环境,地下水,环境风险管控","厂界噪声北","国家标准","工业企业厂界环境噪声排放标准(GB12348-2008)","（表1）工业企业厂界环境噪声排放限值,厂界与噪声敏感建筑物距离不小于1m,2类厂界外声环境功能区,昼间/夜间","生产噪声","2.2","工业企业厂界环境噪声","2024-06-03","56.5","47.7","dB","60;50","","否",""]
["2024","06","03","新余市","渝水区","新余市环境卫生管理处（生活垃圾卫生填埋场）","固废处置厂","7820|环境卫生管理","水环境,地下水,环境风险管控","厂界噪声西","国家标准","工业企业厂界环境噪声排放标准(GB12348-2008)","（表1）工业企业厂界环境噪声排放限值,厂界与噪声敏感建筑物距离不小于1m,2类厂界外声环境功能区,昼间/夜间","生产噪声","2.2","工业企业厂界环境噪声","2024-06-03","53.4","47.9","dB","60;50","","否",""]
["2024","06","04","新余市","渝水区","新余市伟成金属制品有限公司","工业企业","3340|金属丝绳及其制品制造","水环境","厂界噪声东","国家标准","工业企业厂界环境噪声排放标准(GB12348-2008)","（表1）工业企业厂界环境噪声排放限值,厂界与噪声敏感建筑物距离不小于1m,2类厂界外声环境功能区,昼间/夜间","生产噪声","2.1","工业企业厂界环境噪声","2024-06-04","54.5","44","dB","60;50","","否",""]
["2024","06","04","新余市","渝水区","新余市伟成金属制品有限公司","工业企业","3340|金属丝绳及其制品制造","水环境","厂界噪声南","国家标准","工业企业厂界环境噪声排放标准(GB12348-2008)","（表1）工业企业厂界环境噪声排放限值,厂界与噪声敏感建筑物距离不小于1m,2类厂界外声环境功能区,昼间/夜间","生产噪声","2.1","工业企业厂界环境噪声","2024-06-04","59.5","46.9","dB","60;50","","否",""]
["2024","06","04","新余市","渝水区","新余市伟成金属制品有限公司","工业企业","3340|金属丝绳及其制品制造","水环境","厂界噪声北","国家标准","工业企业厂界环境噪声排放标准(GB12348-2008)","（表1）工业企业厂界环境噪声排放限值,厂界与噪声敏感建筑物距离不小于1m,2类厂界外声环境功能区,昼间/夜间","生产噪声","2.1","工业企业厂界环境噪声","2024-06-04","54.6","45.3","dB","60;50","","否",""]
["2024","06","04","新余市","渝水区","新余市伟成金属制品有限公司","工业企业","3340|金属丝绳及其制品制造","水环境","厂界噪声西","国家标准","工业企业厂界环境噪声排放标准(GB12348-2008)","（表1）工业企业厂界环境噪声排放限值,厂界与噪声敏感建筑物距离不小于1m,2类厂界外声环境功能区,昼间/夜间","生产噪声","2.1","工业企业厂界环境噪声","2024-06-04","55.1","43.4","dB","60;50","","否",""]
["2024","06","04","新余市","渝水区","新余市星泰新材料有限公司","工业企业","2614|有机化学原料制造","环境风险管控","厂界噪声南","国家标准","工业企业厂界环境噪声排放标准(GB12348-2008)","（表1）工业企业厂界环境噪声排放限值,厂界与噪声敏感建筑物距离不小于1m,2类厂界外声环境功能区,昼间/夜间","生产噪声","2.1","工业企业厂界环境噪声","2024-06-04","52.1","43.2","dB","60;50","","否",""]
["2024","06","04","新余市","渝水区","新余市星泰新材料有限公司","工业企业","2614|有机化学原料制造","环境风险管控","厂界噪声北","国家标准","工业企业厂界环境噪声排放标准(GB12348-2008)","（表1）工业企业厂界环境噪声排放限值,厂界与噪声敏感建筑物距离不小于1m,2类厂界外声环境功能区,昼间/夜间","生产噪声","2.1","工业企业厂界环境噪声","2024-06-04","53.3","43.8","dB","60;50","","否",""]
["2024","06","04","新余市","渝水区","新余市星泰新材料有限公司","工业企业","2614|有机化学原料制造","环境风险管控","厂界噪声西","国家标准","工业企业厂界环境噪声排放标准(GB12348-2008)","（表1）工业企业厂界环境噪声排放限值,厂界与噪声敏感建筑物距离不小于1m,2类厂界外声环境功能区,昼间/夜间","生产噪声","2.1","工业企业厂界环境噪声","2024-06-04","55.4","46.4","dB","60;50","","否",""]
["2024","06","04","新余市","渝水区","新余市星泰新材料有限公司","工业企业","2614|有机化学原料制造","环境风险管控","厂界噪声东","国家标准","工业企业厂界环境噪声排放标准(GB12348-2008)","（表1）工业企业厂界环境噪声排放限值,厂界与噪声敏感建筑物距离不小于1m,2类厂界外声环境功能区,昼间/夜间","生产噪声","2.1","工业企业厂界环境噪声","2024-06-04","55.4","43.7","dB","60;50","","否",""]
["2024","06","20","新余市","渝水区","新余市裕富金属制品有限公司","工业企业","3130|钢压延加工","环境风险管控","北","国家标准","工业企业厂界环境噪声排放标准(GB12348-2008)","（表1）工业企业厂界环境噪声排放限值,厂界与噪声敏感建筑物距离不小于1m,3类厂界外声环境功能区,昼间/夜间","企业生产","2.7","工业企业厂界环境噪声","2024-06-20","57.6","","dB","65;55","","否",""]
["2024","06","20","新余市","渝水区","新余市裕富金属制品有限公司","工业企业","3130|钢压延加工","环境风险管控","西","国家标准","工业企业厂界环境噪声排放标准(GB12348-2008)","（表1）工业企业厂界环境噪声排放限值,厂界与噪声敏感建筑物距离不小于1m,3类厂界外声环境功能区,昼间/夜间","企业生产","2.7","工业企业厂界环境噪声","2024-06-20","56.1","","dB","65;55","","否",""]
["2024","06","20","新余市","渝水区","新余市裕富金属制品有限公司","工业企业","3130|钢压延加工","环境风险管控","南","国家标准","工业企业厂界环境噪声排放标准(GB12348-2008)","（表1）工业企业厂界环境噪声排放限值,厂界与噪声敏感建筑物距离不小于1m,3类厂界外声环境功能区,昼间/夜间","企业生产","2.7","工业企业厂界环境噪声","2024-06-20","58.8","","dB","65;55","","否",""]
["2024","06","20","新余市","渝水区","新余市裕富金属制品有限公司","工业企业","3130|钢压延加工","环境风险管控","东","国家标准","工业企业厂界环境噪声排放标准(GB12348-2008)","（表1）工业企业厂界环境噪声排放限值,厂界与噪声敏感建筑物距离不小于1m,3类厂界外声环境功能区,昼间/夜间","企业生产","2.7","工业企业厂界环境噪声","2024-06-20","58.7","","dB","65;55","","否",""]
["2024","06","19","新余市","渝水区","新余益欣金属材料有限公司","工业企业","3360|金属表面处理及热处理加工","环境风险管控","厂界北","国家标准","工业企业厂界环境噪声排放标准(GB12348-2008)","（表1）工业企业厂界环境噪声排放限值,厂界与噪声敏感建筑物距离不小于1m,3类厂界外声环境功能区,昼间/夜间","厂区设备","2.9","工业企业厂界环境噪声","2024-06-19","56.9","","dB","65;55","","否",""]
["2024","06","19","新余市","渝水区","新余益欣金属材料有限公司","工业企业","3360|金属表面处理及热处理加工","环境风险管控","厂界南","国家标准","工业企业厂界环境噪声排放标准(GB12348-2008)","（表1）工业企业厂界环境噪声排放限值,厂界与噪声敏感建筑物距离不小于1m,3类厂界外声环境功能区,昼间/夜间","厂区设备","2.9","工业企业厂界环境噪声","2024-06-19","57.3","","dB","65;55","","否",""]
["2024","06","19","新余市","渝水区","新余益欣金属材料有限公司","工业企业","3360|金属表面处理及热处理加工","环境风险管控","厂界东","国家标准","工业企业厂界环境噪声排放标准(GB12348-2008)","（表1）工业企业厂界环境噪声排放限值,厂界与噪声敏感建筑物距离不小于1m,3类厂界外声环境功能区,昼间/夜间","厂区设备","2.9","工业企业厂界环境噪声","2024-06-19","57.4","","dB","65;55","","否",""]
["2024","06","19","新余市","渝水区","新余益欣金属材料有限公司","工业企业","3360|金属表面处理及热处理加工","环境风险管控","厂界西","国家标准","工业企业厂界环境噪声排放标准(GB12348-2008)","（表1）工业企业厂界环境噪声排放限值,厂界与噪声敏感建筑物距离不小于1m,3类厂界外声环境功能区,昼间/夜间","厂区设备","2.9","工业企业厂界环境噪声","2024-06-19","57.2","","dB","65;55","","否",""]
["2024","06","03","新余市","渝水区","新余永清环保能源有限公司","固废处置厂","4417-1|生物质能发电-生活垃圾焚烧发电","水环境,土壤污染监管","厂界噪声北","国家标准","工业企业厂界环境噪声排放标准(GB12348-2008)","（表1）工业企业厂界环境噪声排放限值,厂界与噪声敏感建筑物距离不小于1m,2类厂界外声环境功能区,昼间/夜间","生产噪声","1.8","工业企业厂界环境噪声","2024-06-03","59.6","48.4","dB","60;50","","否",""]
["2024","06","03","新余市","渝水区","新余永清环保能源有限公司","固废处置厂","4417-1|生物质能发电-生活垃圾焚烧发电","水环境,土壤污染监管","厂界噪声东","国家标准","工业企业厂界环境噪声排放标准(GB12348-2008)","（表1）工业企业厂界环境噪声排放限值,厂界与噪声敏感建筑物距离不小于1m,2类厂界外声环境功能区,昼间/夜间","生产噪声","1.8","工业企业厂界环境噪声","2024-06-03","55.3","48.2","dB","60;50","","否",""]
["2024","06","03","新余市","渝水区","新余永清环保能源有限公司","固废处置厂","4417-1|生物质能发电-生活垃圾焚烧发电","水环境,土壤污染监管","厂界噪声西","国家标准","工业企业厂界环境噪声排放标准(GB12348-2008)","（表1）工业企业厂界环境噪声排放限值,厂界与噪声敏感建筑物距离不小于1m,2类厂界外声环境功能区,昼间/夜间","生产噪声","1.8","工业企业厂界环境噪声","2024-06-03","55","48.1","dB","60;50","","否",""]
["2024","06","03","新余市","渝水区","新余永清环保能源有限公司","固废处置厂","4417-1|生物质能发电-生活垃圾焚烧发电","水环境,土壤污染监管","厂界噪声南","国家标准","工业企业厂界环境噪声排放标准(GB12348-2008)","（表1）工业企业厂界环境噪声排放限值,厂界与噪声敏感建筑物距离不小于1m,2类厂界外声环境功能区,昼间/夜间","生产噪声","1.8","工业企业厂界环境噪声","2024-06-03","58.4","48.5","dB","60;50","","否",""]
["2024","06","20","新余市","","江西新华新材料科技股份有限公司","工业企业","3340|金属丝绳及其制品制造","环境风险管控","厂界噪声西面","国家标准","工业企业厂界环境噪声排放标准(GB12348-2008)","（表1）工业企业厂界环境噪声排放限值,厂界与噪声敏感建筑物距离不小于1m,2类厂界外声环境功能区,昼间/夜间","厂区设备","3.1","工业企业厂界环境噪声","2024-06-20","56.6","45.9","dB","60;50","","否",""]
["2024","06","20","新余市","","江西新华新材料科技股份有限公司","工业企业","3340|金属丝绳及其制品制造","环境风险管控","厂界噪声东面","国家标准","工业企业厂界环境噪声排放标准(GB12348-2008)","（表1）工业企业厂界环境噪声排放限值,厂界与噪声敏感建筑物距离不小于1m,2类厂界外声环境功能区,昼间/夜间","厂区设备","3.1","工业企业厂界环境噪声","2024-06-20","56.1","48.4","dB","60;50","","否",""]
["2024","06","20","新余市","","江西新华新材料科技股份有限公司","工业企业","3340|金属丝绳及其制品制造","环境风险管控","厂界噪声南面","国家标准","工业企业厂界环境噪声排放标准(GB12348-2008)","（表1）工业企业厂界环境噪声排放限值,厂界与噪声敏感建筑物距离不小于1m,2类厂界外声环境功能区,昼间/夜间","厂区设备","3.1","工业企业厂界环境噪声","2024-06-20","59.1","48.5","dB","60;50","","否",""]
["2024","06","20","新余市","","江西新华新材料科技股份有限公司","工业企业","3340|金属丝绳及其制品制造","环境风险管控","厂界噪声北面","国家标准","工业企业厂界环境噪声排放标准(GB12348-2008)","（表1）工业企业厂界环境噪声排放限值,厂界与噪声敏感建筑物距离不小于1m,2类厂界外声环境功能区,昼间/夜间","厂区设备","3.1","工业企业厂界环境噪声","2024-06-20","56.8","46.9","dB","60;50","","否",""]
["2024","06","22","新余市","","江西增鑫科技股份有限公司","工业企业","3574|畜牧机械制造","环境风险管控","东界","国家标准","工业企业厂界环境噪声排放标准(GB12348-2008)","（表1）工业企业厂界环境噪声排放限值,厂界与噪声敏感建筑物距离不小于1m,2类厂界外声环境功能区,昼间/夜间","厂区设备","2.5","工业企业厂界环境噪声","2024-06-22","57.7","49.4","dB","60;50","","否",""]
["2024","06","22","新余市","","江西增鑫科技股份有限公司","工业企业","3574|畜牧机械制造","环境风险管控","西界","国家标准","工业企业厂界环境噪声排放标准(GB12348-2008)","（表1）工业企业厂界环境噪声排放限值,厂界与噪声敏感建筑物距离不小于1m,2类厂界外声环境功能区,昼间/夜间","厂区设备","2.5","工业企业厂界环境噪声","2024-06-22","55.9","49.1","dB","60;50","","否",""]
["2024","06","22","新余市","","江西增鑫科技股份有限公司","工业企业","3574|畜牧机械制造","环境风险管控","北界","国家标准","工业企业厂界环境噪声排放标准(GB12348-2008)","（表1）工业企业厂界环境噪声排放限值,厂界与噪声敏感建筑物距离不小于1m,2类厂界外声环境功能区,昼间/夜间","厂区设备","2.5","工业企业厂界环境噪声","2024-06-22","56.7","47.9","dB","60;50","","否",""]
["2024","06","22","新余市","","江西增鑫科技股份有限公司","工业企业","3574|畜牧机械制造","环境风险管控","南界","国家标准","工业企业厂界环境噪声排放标准(GB12348-2008)","（表1）工业企业厂界环境噪声排放限值,厂界与噪声敏感建筑物距离不小于1m,2类厂界外声环境功能区,昼间/夜间","厂区设备","2.5","工业企业厂界环境噪声","2024-06-22","59.5","47.2","dB","60;50","","否",""]
["2024","06","23","新余市","","新余海顺环保科技有限公司","工业企业","4190|其他未列明制造业","环境风险管控","厂界西","国家标准","工业企业厂界环境噪声排放标准(GB12348-2008)","（表1）工业企业厂界环境噪声排放限值,厂界与噪声敏感建筑物距离不小于1m,3类厂界外声环境功能区,昼间/夜间","厂区设备","2.1","工业企业厂界环境噪声","2024-06-23","56.1","","dB","65;55","","否",""]
["2024","06","23","新余市","","新余海顺环保科技有限公司","工业企业","4190|其他未列明制造业","环境风险管控","厂界南","国家标准","工业企业厂界环境噪声排放标准(GB12348-2008)","（表1）工业企业厂界环境噪声排放限值,厂界与噪声敏感建筑物距离不小于1m,3类厂界外声环境功能区,昼间/夜间","厂区设备","2.1","工业企业厂界环境噪声","2024-06-23","58.3","","dB","65;55","","否",""]
["2024","06","23","新余市","","新余海顺环保科技有限公司","工业企业","4190|其他未列明制造业","环境风险管控","厂界东","国家标准","工业企业厂界环境噪声排放标准(GB12348-2008)","（表1）工业企业厂界环境噪声排放限值,厂界与噪声敏感建筑物距离不小于1m,3类厂界外声环境功能区,昼间/夜间","厂区设备","2.1","工业企业厂界环境噪声","2024-06-23","58.2","","dB","65;55","","否",""]
["2024","06","23","新余市","","新余海顺环保科技有限公司","工业企业","4190|其他未列明制造业","环境风险管控","厂界北","国家标准","工业企业厂界环境噪声排放标准(GB12348-2008)","（表1）工业企业厂界环境噪声排放限值,厂界与噪声敏感建筑物距离不小于1m,3类厂界外声环境功能区,昼间/夜间","厂区设备","2.1","工业企业厂界环境噪声","2024-06-23","58.1","","dB","65;55","","否",""]
["2024","06","21","新余市","","新余市郁海环保科技有限公司","工业企业","7724|危险废物治理","环境风险管控","厂界南","国家标准","工业企业厂界环境噪声排放标准(GB12348-2008)","（表1）工业企业厂界环境噪声排放限值,厂界与噪声敏感建筑物距离不小于1m,3类厂界外声环境功能区,昼间/夜间","厂区设备","1.9","工业企业厂界环境噪声","2024-06-21","58.8","","dB","65;55","","否",""]
["2024","06","21","新余市","","新余市郁海环保科技有限公司","工业企业","7724|危险废物治理","环境风险管控","厂界西","国家标准","工业企业厂界环境噪声排放标准(GB12348-2008)","（表1）工业企业厂界环境噪声排放限值,厂界与噪声敏感建筑物距离不小于1m,3类厂界外声环境功能区,昼间/夜间","厂区设备","1.9","工业企业厂界环境噪声","2024-06-21","56.6","","dB","65;55","","否",""]
["2024","06","21","新余市","","新余市郁海环保科技有限公司","工业企业","7724|危险废物治理","环境风险管控","厂界东","国家标准","工业企业厂界环境噪声排放标准(GB12348-2008)","（表1）工业企业厂界环境噪声排放限值,厂界与噪声敏感建筑物距离不小于1m,3类厂界外声环境功能区,昼间/夜间","厂区设备","1.9","工业企业厂界环境噪声","2024-06-21","58.7","","dB","65;55","","否",""]
["2024","06","21","新余市","","新余市郁海环保科技有限公司","工业企业","7724|危险废物治理","环境风险管控","厂界北","国家标准","工业企业厂界环境噪声排放标准(GB12348-2008)","（表1）工业企业厂界环境噪声排放限值,厂界与噪声敏感建筑物距离不小于1m,3类厂界外声环境功能区,昼间/夜间","厂区设备","1.9","工业企业厂界环境噪声","2024-06-21","55.6","","dB","65;55","","否",""]
["2024","06","20","新余市","","新余新钢金属制品有限公司","工业企业","3340|金属丝绳及其制品制造","环境风险管控","铝包生产区厂界噪声东面","国家标准","工业企业厂界环境噪声排放标准(GB12348-2008)","（表1）工业企业厂界环境噪声排放限值,厂界与噪声敏感建筑物距离不小于1m,2类厂界外声环境功能区,昼间/夜间","厂区设备","2.7","工业企业厂界环境噪声","2024-06-20","57.4","","dB","60;50","","否",""]
["2024","06","20","新余市","","新余新钢金属制品有限公司","工业企业","3340|金属丝绳及其制品制造","环境风险管控","钢丝生产区厂界噪声南面","国家标准","工业企业厂界环境噪声排放标准(GB12348-2008)","（表1）工业企业厂界环境噪声排放限值,厂界与噪声敏感建筑物距离不小于1m,2类厂界外声环境功能区,昼间/夜间","厂区设备","3.2","工业企业厂界环境噪声","2024-06-20","58.6","48","dB","60;50","","否",""]
["2024","06","20","新余市","","新余新钢金属制品有限公司","工业企业","3340|金属丝绳及其制品制造","环境风险管控","铝包生产区厂界噪声南面","国家标准","工业企业厂界环境噪声排放标准(GB12348-2008)","（表1）工业企业厂界环境噪声排放限值,厂界与噪声敏感建筑物距离不小于1m,2类厂界外声环境功能区,昼间/夜间","厂区设备","2.7","工业企业厂界环境噪声","2024-06-20","55.6","","dB","60;50","","否",""]
["2024","06","20","新余市","","新余新钢金属制品有限公司","工业企业","3340|金属丝绳及其制品制造","环境风险管控","钢丝生产区厂界噪声北面","国家标准","工业企业厂界环境噪声排放标准(GB12348-2008)","（表1）工业企业厂界环境噪声排放限值,厂界与噪声敏感建筑物距离不小于1m,2类厂界外声环境功能区,昼间/夜间","厂区设备","3.2","工业企业厂界环境噪声","2024-06-20","56.3","47.5","dB","60;50","","否",""]
["2024","06","20","新余市","","新余新钢金属制品有限公司","工业企业","3340|金属丝绳及其制品制造","环境风险管控","钢丝生产区厂界噪声西面","国家标准","工业企业厂界环境噪声排放标准(GB12348-2008)","（表1）工业企业厂界环境噪声排放限值,厂界与噪声敏感建筑物距离不小于1m,2类厂界外声环境功能区,昼间/夜间","厂区设备","3.2","工业企业厂界环境噪声","2024-06-20","55.3","47","dB","60;50","","否",""]
["2024","06","20","新余市","","新余新钢金属制品有限公司","工业企业","3340|金属丝绳及其制品制造","环境风险管控","铝包生产区厂界噪声北面","国家标准","工业企业厂界环境噪声排放标准(GB12348-2008)","（表1）工业企业厂界环境噪声排放限值,厂界与噪声敏感建筑物距离不小于1m,2类厂界外声环境功能区,昼间/夜间","厂区设备","2.7","工业企业厂界环境噪声","2024-06-20","57.6","","dB","60;50","","否",""]
["2024","06","20","新余市","","新余新钢金属制品有限公司","工业企业","3340|金属丝绳及其制品制造","环境风险管控","钢丝生产区厂界噪声东面","国家标准","工业企业厂界环境噪声排放标准(GB12348-2008)","（表1）工业企业厂界环境噪声排放限值,厂界与噪声敏感建筑物距离不小于1m,2类厂界外声环境功能区,昼间/夜间","厂区设备","3.2","工业企业厂界环境噪声","2024-06-20","56.7","47.5","dB","60;50","","否",""]
["2024","06","20","新余市","","新余新钢金属制品有限公司","工业企业","3340|金属丝绳及其制品制造","环境风险管控","铝包生产区厂界噪声西面","国家标准","工业企业厂界环境噪声排放标准(GB12348-2008)","（表1）工业企业厂界环境噪声排放限值,厂界与噪声敏感建筑物距离不小于1m,2类厂界外声环境功能区,昼间/夜间","厂区设备","2.7","工业企业厂界环境噪声","2024-06-20","56.5","","dB","60;50","","否",""]

{"sheet":"无组织","index":4,"n_rows":26,"n_cols":25,"rows_kept":26,"merged":[[0,0,0,24]],"flags":["formulas_cached_only"]}
["执法监测无组织数据",null,"","","","","","","","","","","","","","","","","","","","","","",""]
["监测年","监测月","监测日","市","县","企业名称","企业类别","行业类别","名录类别","监测点名称","排放标准类型","排放标准名称","标准条目","无组织风向","无组织风速(m/s)","无组织温度(℃)","无组织压力(kPa)","监测项目","项目监测日期","监测结果","取值单位","排放上限","排放下限","是否超标","超标倍数"]
["2024","06","22","新余市","","江西鸿强科技有限公司","工业企业","2613|无机盐制造","大气环境","上风向","国家标准","无机化学工业污染物排放标准(GB31573-2015)","（表5）企业边界大气污染物排放限值,除硫化合物及硫酸盐工业、无机氰化合物工业外","西南风","2.1","29.3","100.1","氯气","2024-06-22","<0.03","mg/m3","0.1","","否",""]
["2024","06","22","新余市","","江西鸿强科技有限公司","工业企业","2613|无机盐制造","大气环境","上风向","国家标准","大气污染物综合排放标准(GB16297-1996)","（表2）新污染源大气污染物排放限值（1997年1月1日起）,无组织排放监控浓度限值,除玻璃棉尘、石英粉尘、矿渣棉尘外其他","西南风","2.1","29.3","100.1","颗粒物","2024-06-22","0.211","mg/m3","1.0","","否",""]
["2024","06","22","新余市","","江西鸿强科技有限公司","工业企业","2613|无机盐制造","大气环境","下风向2","国家标准","无机化学工业污染物排放标准(GB31573-2015)","（表5）企业边界大气污染物排放限值,除硫化合物及硫酸盐工业、无机氰化合物工业外","西南风","2.1","29.3","100.1","氯化氢","2024-06-22","<0.02","mg/m3","0.05","","否",""]
["2024","06","22","新余市","","江西鸿强科技有限公司","工业企业","2613|无机盐制造","大气环境","上风向","国家标准","无机化学工业污染物排放标准(GB31573-2015)","（表5）企业边界大气污染物排放限值,除硫化合物及硫酸盐工业、无机氰化合物工业外","西南风","2.1","29.3","100.1","氯化氢","2024-06-22","<0.02","mg/Nm3","0.05","","否",""]
["2024","06","22","新余市","","江西鸿强科技有限公司","工业企业","2613|无机盐制造","大气环境","下风向1","国家标准","大气污染物综合排放标准(GB16297-1996)","（表2）新污染源大气污染物排放限值（1997年1月1日起）,无组织排放监控浓度限值,除玻璃棉尘、石英粉尘、矿渣棉尘外其他","西南风","2.1","29.3","100.1","颗粒物","2024-06-22","0.295","mg/m3","1.0","","否",""]
["2024","06","22","新余市","","江西鸿强科技有限公司","工业企业","2613|无机盐制造","大气环境","下风向3","国家标准","无机化学工业污染物排放标准(GB31573-2015)","（表5）企业边界大气污染物排放限值,除硫化合物及硫酸盐工业、无机氰化合物工业外","西南风","2.1","29.3","100.1","氯气","2024-06-22","<0.03","mg/m3","0.1","","否",""]
["2024","06","22","新余市","","江西鸿强科技有限公司","工业企业","2613|无机盐制造","大气环境","下风向1","国家标准","无机化学工业污染物排放标准(GB31573-2015)","（表5）企业边界大气污染物排放限值,除硫化合物及硫酸盐工业、无机氰化合物工业外","西南风","2.1","29.3","100.1","氯化氢","2024-06-22","<0.02","mg/m3","0.05","","否",""]
["2024","06","22","新余市","","江西鸿强科技有限公司","工业企业","2613|无机盐制造","大气环境","下风向1","国家标准","无机化学工业污染物排放标准(GB31573-2015)","（表5）企业边界大气污染物排放限值,除硫化合物及硫酸盐工业、无机氰化合物工业外","西南风","2.1","29.3","100.1","氯气","2024-06-22","0.03","mg/m3","0.1","","否",""]
["2024","06","22","新余市","","江西鸿强科技有限公司","工业企业","2613|无机盐制造","大气环境","下风向2","国家标准","无机化学工业污染物排放标准(GB31573-2015)","（表5）企业边界大气污染物排放限值,除硫化合物及硫酸盐工业、无机氰化合物工业外","西南风","2.1","29.3","100.1","氯气","2024-06-22","0.06","mg/m3","0.1","","否",""]
["2024","06","22","新余市","","江西鸿强科技有限公司","工业企业","2613|无机盐制造","大气环境","下风向3","国家标准","无机化学工业污染物排放标准(GB31573-2015)","（表5）企业边界大气污染物排放限值,除硫化合物及硫酸盐工业、无机氰化合物工业外","西南风","2.1","29.3","100.1","氯化氢","2024-06-22","<0.02","mg/m3","0.05","","否",""]
["2024","06","22","新余市","","江西鸿强科技有限公司","工业企业","2613|无机盐制造","大气环境","下风向3","国家标准","大气污染物综合排放标准(GB16297-1996)","（表2）新污染源大气污染物排放限值（1997年1月1日起）,无组织排放监控浓度限值,除玻璃棉尘、石英粉尘、矿渣棉尘外其他","西南风","2.1","29.3","100.1","颗粒物","2024-06-22","0.286","mg/m3","1.0","","否",""]
["2024","06","22","新余市","","江西鸿强科技有限公司","工业企业","2613|无机盐制造","大气环境","下风向2","国家标准","大气污染物综合排放标准(GB16297-1996)","（表2）新污染源大气污染物排放限值（1997年1月1日起）,无组织排放监控浓度限值,除玻璃棉尘、石英粉尘、矿渣棉尘外其他","西南风","2.1","29.3","100.1","颗粒物","2024-06-22","0.303","mg/m3","1.0","","否",""]
["2024","06","19","新余市","","江西新华新材料科技股份有限公司","工业企业","3340|金属丝绳及其制品制造","环境风险管控","厂界无组织","国家标准","大气污染物综合排放标准(GB16297-1996)","（表2）新污染源大气污染物排放限值（1997年1月1日起）,无组织排放监控浓度限值,通用","西南风","3.0","27.8","100.6","二氧化硫","2024-06-19","0.020","mg/m3","0.40","","否",""]
["2024","06","19","新余市","","江西新华新材料科技股份有限公司","工业企业","3340|金属丝绳及其制品制造","环境风险管控","厂界无组织","国家标准","大气污染物综合排放标准(GB16297-1996)","（表2）新污染源大气污染物排放限值（1997年1月1日起）,无组织排放监控浓度限值,通用","西南风","3.0","27.8","100.6","氯化氢","2024-06-19","0.144","mg/m3","0.20","","否",""]
["2024","06","19","新余市","","江西新华新材料科技股份有限公司","工业企业","3340|金属丝绳及其制品制造","环境风险管控","厂界无组织","国家标准","大气污染物综合排放标准(GB16297-1996)","（表2）新污染源大气污染物排放限值（1997年1月1日起）,无组织排放监控浓度限值,除玻璃棉尘、石英粉尘、矿渣棉尘外其他","西南风","3.0","27.8","100.6","颗粒物","2024-06-19","0.296","mg/m3","1.0","","否",""]
["2024","06","19","新余市","","江西新华新材料科技股份有限公司","工业企业","3340|金属丝绳及其制品制造","环境风险管控","厂界无组织","国家标准","大气污染物综合排放标准(GB16297-1996)","（表2）新污染源大气污染物排放限值（1997年1月1日起）,无组织排放监控浓度限值,通用","西南风","3.0","27.8","100.6","氮氧化物","2024-06-19","0.026","mg/m3","0.12","","否",""]
["2024","06","19","新余市","","江西新华新材料科技股份有限公司","工业企业","3340|金属丝绳及其制品制造","环境风险管控","厂界无组织","国家标准","恶臭污染物排放标准(GB14554-93)","（表1）恶臭污染物厂界标准值,二级,新扩改建","西南风","3.0","27.8","100.6","氨（氨气）","2024-06-19","0.14","mg/m3","1.5","","否",""]
["2024","06","23","新余市","","新余海顺环保科技有限公司","工业企业","4190|其他未列明制造业","环境风险管控","厂界","国家标准","大气污染物综合排放标准(GB16297-1996)","（表2）新污染源大气污染物排放限值（1997年1月1日起）,无组织排放监控浓度限值,通用","西南风","1.8","28.5","100.2","非甲烷总烃","2024-06-23","1.09","mg/m3","4.0","","否",""]
["2024","06","23","新余市","","新余海顺环保科技有限公司","工业企业","4190|其他未列明制造业","环境风险管控","储油罐周边","国家标准","挥发性有机物无组织排放控制标准(GB 37822—2019)","表A.1 厂内VOCs无组织排放限值,监测点处1h平均浓度值,排放限值","西南风","1.8","28.5","100.2","NMHC","2024-06-23","1.04","mg/m3","10","","否",""]
["2024","06","20","新余市","","新余新钢金属制品有限公司","工业企业","3340|金属丝绳及其制品制造","环境风险管控","厂界","国家标准","大气污染物综合排放标准(GB16297-1996)","（表2）新污染源大气污染物排放限值（1997年1月1日起）,无组织排放监控浓度限值,通用","西南风","3.1","27.6","100.6","二氧化硫","2024-06-20","0.020","mg/m3","0.40","","否",""]
["2024","06","20","新余市","","新余新钢金属制品有限公司","工业企业","3340|金属丝绳及其制品制造","环境风险管控","厂界","国家标准","大气污染物综合排放标准(GB16297-1996)","（表2）新污染源大气污染物排放限值（1997年1月1日起）,无组织排放监控浓度限值,通用","西南风","3.1","27.6","100.6","氯化氢","2024-06-20","0.133","mg/m3","0.20","","否",""]
["2024","06","20","新余市","","新余新钢金属制品有限公司","工业企业","3340|金属丝绳及其制品制造","环境风险管控","热处理车间无组织","国家标准","大气污染物综合排放标准(GB16297-1996)","（表2）新污染源大气污染物排放限值（1997年1月1日起）,无组织排放监控浓度限值,通用","西南风","3.1","27.6","100.6","铅及其化合物","2024-06-20","0.000655","mg/m3","0.006","","否",""]
["2024","06","20","新余市","","新余新钢金属制品有限公司","工业企业","3340|金属丝绳及其制品制造","环境风险管控","厂界","国家标准","大气污染物综合排放标准(GB16297-1996)","（表2）新污染源大气污染物排放限值（1997年1月1日起）,无组织排放监控浓度限值,通用","西南风","3.1","27.6","100.6","氮氧化物","2024-06-20","0.024","mg/m3","0.12","","否",""]
["2024","06","20","新余市","","新余新钢金属制品有限公司","工业企业","3340|金属丝绳及其制品制造","环境风险管控","厂界","国家标准","大气污染物综合排放标准(GB16297-1996)","（表2）新污染源大气污染物排放限值（1997年1月1日起）,无组织排放监控浓度限值,除玻璃棉尘、石英粉尘、矿渣棉尘外其他","西南风","3.1","27.6","100.6","颗粒物","2024-06-20","0.292","mg/m3","1.0","","否",""]