{"text_format":"3","workbook":"xls","n_sheets":2,"sheets":["废气排放","废水排放"],"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"废气排放","index":0,"n_rows":83,"n_cols":29,"rows_kept":83,"merged":[[0,0,0,28]],"flags":["formulas_cached_only"]}
["执法监测废气排放数据","","","","","","","","","","","","","","","","","","","","","","","","","","","",""]
["监测年","监测月","监测日","市","县","企业名称","企业类别","行业类别","名录类别","监测点名称","排放标准类型","排放标准名称","标准条目","废气生产负荷","废气流量","废气温度","废气湿度","废气含氧量","废气流速","监测项目名称","项目监测日期","废气实测结果","废气折算结果","取值单位","排放上限","排放下限","是否有评价限值","是否超标","超标倍数"]
["2024","09","18","新余市","渝水区","新余新钢优特钢带有限公司","工业企业","3130|钢压延加工","大气环境","酸洗废气排放口","国家标准","轧钢工业大气污染物排放标准(GB28665-2012)","（表1、表2）现有和新建企业有组织大气污染物排放浓度限值,酸洗机组","100","6122","48.6","11.52","","5.9","氯化氢","2024-09-18","<0.2","<0.2","mg/m3","20","","是","否",""]
["2024","09","18","新余市","渝水区","新余新钢优特钢带有限公司","工业企业","3130|钢压延加工","大气环境","二期退火炉","国家标准","轧钢工业大气污染物排放标准(GB28665-2012)","（修改单）新建企业有组织大气污染物排放浓度限值,热处理炉,其他热处理炉","100","41268","133","3.5","17.93","10","二氧化硫","2024-09-18","<3","<3","mg/m3","100","","是","否",""]
["2024","09","18","新余市","渝水区","新余新钢优特钢带有限公司","工业企业","3130|钢压延加工","大气环境","二期退火炉","国家标准","轧钢工业大气污染物排放标准(GB28665-2012)","（表1、表2）现有和新建企业有组织大气污染物排放浓度限值,热处理炉","100","43988","133","3.5","17.97","10.7","颗粒物","2024-09-18","2.4","4.8","mg/m3","20","","是","否",""]
["2024","09","18","新余市","渝水区","新余新钢优特钢带有限公司","工业企业","3130|钢压延加工","大气环境","二期退火炉","国家标准","轧钢工业大气污染物排放标准(GB28665-2012)","（修改单）新建企业有组织大气污染物排放浓度限值,热处理炉,其他热处理炉","100","41268","133","3.5","17.93","10","氮氧化物","2024-09-18","47","91","mg/m3","200","","是","否",""]
["2024","09","29","新余市","分宜县","江西电力有限公司分宜发电厂（双林厂区）","工业企业","4411|火力发电","大气环境","#1机组烟囱001(DA001)","国家标准","火电厂大气污染物排放标准(GB13223-2011)","（表1）火力发电锅炉及燃汽轮机组大气污染物排放浓度限值,烟囱或烟道,燃煤锅炉,全部,通用","100","1813400","48.2","13.5","6.9","15.9","烟尘","2024-09-29","3.1","3.3","mg/m3","30","","是","否",""]
["2024","09","29","新余市","分宜县","江西电力有限公司分宜发电厂（双林厂区）","工业企业","4411|火力发电","大气环境","#1机组烟囱001(DA001)","国家标准","火电厂大气污染物排放标准(GB13223-2011)","（表1）火力发电锅炉及燃汽轮机组大气污染物排放浓度限值,烟囱排放口,燃煤锅炉，以油、气体为燃料的锅炉或燃汽轮机组","100","","","","","","林格曼黑度","2024-09-29","<1","<1","级","1","","是","否",""]
["2024","09","29","新余市","分宜县","江西电力有限公司分宜发电厂（双林厂区）","工业企业","4411|火力发电","大气环境","#2机组烟囱002（DA002）(DA002)","国家标准","火电厂大气污染物排放标准(GB13223-2011)","（表1）火力发电锅炉及燃汽轮机组大气污染物排放浓度限值,烟囱排放口,燃煤锅炉，以油、气体为燃料的锅炉或燃汽轮机组","100","","","","","","林格曼黑度","2024-09-29","<1","<1","级","1","","是","否",""]
["2024","09","29","新余市","分宜县","江西电力有限公司分宜发电厂（双林厂区）","工业企业","4411|火力发电","大气环境","#2机组烟囱002（DA002）(DA002)","国家标准","火电厂大气污染物排放标准(GB13223-2011)","（表1）火力发电锅炉及燃汽轮机组大气污染物排放浓度限值,烟囱或烟道,燃煤锅炉,全部,除（采用W型火焰炉膛的发电锅炉，现有循环流化床火力发电锅炉以及2003年12月31日前建成或通过建设项目环境影响报告书审批的火力发电锅）之外","100","1246908","51","14.9","7.5","11.3","氮氧化物","2024-09-29","30","33","mg/m3","100","","是","否",""]
["2024","09","29","新余市","分宜县","江西电力有限公司分宜发电厂（双林厂区）","工业企业","4411|火力发电","大气环境","#1机组烟囱001(DA001)","国家标准","火电厂大气污染物排放标准(GB13223-2011)","（表1）火力发电锅炉及燃汽轮机组大气污染物排放浓度限值,烟囱或烟道,燃煤锅炉,全部,通用","100","171610","47.9","15.3","6.91","15.1","汞及其化合物","2024-09-29","0.00202","0.00214","mg/m3","0.03","","是","否",""]
["2024","09","29","新余市","分宜县","江西电力有限公司分宜发电厂（双林厂区）","工业企业","4411|火力发电","大气环境","#2机组烟囱002（DA002）(DA002)","国家标准","火电厂大气污染物排放标准(GB13223-2011)","（表1）火力发电锅炉及燃汽轮机组大气污染物排放浓度限值,烟囱或烟道,燃煤锅炉,新建锅炉,其他新建锅炉（除位于广西壮族自治区、重庆市、四川省和贵州省之外）","100","1246908","51","14.9","7.5","11.3","二氧化硫","2024-09-29","19","21","mg/m3","100","","是","否",""]
["2024","09","29","新余市","分宜县","江西电力有限公司分宜发电厂（双林厂区）","工业企业","4411|火力发电","大气环境","#1机组烟囱001(DA001)","国家标准","火电厂大气污染物排放标准(GB13223-2011)","（表1）火力发电锅炉及燃汽轮机组大气污染物排放浓度限值,烟囱或烟道,燃煤锅炉,全部,除（采用W型火焰炉膛的发电锅炉，现有循环流化床火力发电锅炉以及2003年12月31日前建成或通过建设项目环境影响报告书审批的火力发电锅）之外","100","171610","47.9","15.3","6.91","15.1","氮氧化物","2024-09-29","42","44","mg/m3","100","","是","否",""]
["2024","09","29","新余市","分宜县","江西电力有限公司分宜发电厂（双林厂区）","工业企业","4411|火力发电","大气环境","#1机组烟囱001(DA001)","国家标准","火电厂大气污染物排放标准(GB13223-2011)","（表1）火力发电锅炉及燃汽轮机组大气污染物排放浓度限值,烟囱或烟道,燃煤锅炉,新建锅炉,其他新建锅炉（除位于广西壮族自治区、重庆市、四川省和贵州省之外）","100","171610","47.9","15.3","6.91","15.1","二氧化硫","2024-09-29","24","26","mg/m3","100","","是","否",""]
["2024","09","29","新余市","分宜县","江西电力有限公司分宜发电厂（双林厂区）","工业企业","4411|火力发电","大气环境","#2机组烟囱002（DA002）(DA002)","国家标准","火电厂大气污染物排放标准(GB13223-2011)","（表1）火力发电锅炉及燃汽轮机组大气污染物排放浓度限值,烟囱或烟道,燃煤锅炉,全部,通用","100","1204073","51","13.6","7.59","10.9","烟尘","2024-09-29","3.0","3.4","mg/m3","30","","是","否",""]
["2024","09","29","新余市","分宜县","江西电力有限公司分宜发电厂（双林厂区）","工业企业","4411|火力发电","大气环境","#2机组烟囱002（DA002）(DA002)","国家标准","火电厂大气污染物排放标准(GB13223-2011)","（表1）火力发电锅炉及燃汽轮机组大气污染物排放浓度限值,烟囱或烟道,燃煤锅炉,全部,通用","100","1246908","51","14.9","7.5","11.3","汞及其化合物","2024-09-29","0.00468","0.00521","mg/m3","0.03","","是","否",""]
["2024","09","19","新余市","高新区","江西东鹏新材料有限责任公司阳光大道厂","工业企业","2613|无机盐制造","水环境,大气环境,土壤污染监管","4#排气筒005(DA005)","国家标准","无机化学工业污染物排放标准(GB31573-2015)","（表3）大气污染排放限值,涉铊、锌、铜、铅重金属无机化合物工业","100","38843","242","15.4","","7","铊及其化合物（以铊计）","2024-09-19","0.0000274","0.0000274","mg/m3","0.05","","是","否",""]
["2024","09","19","新余市","高新区","江西东鹏新材料有限责任公司阳光大道厂","工业企业","2613|无机盐制造","水环境,大气环境,土壤污染监管","4#排气筒005(DA005)","国家标准","无机化学工业污染物排放标准(GB31573-2015)","（表3）大气污染排放限值,硫化合物及硫酸盐工业,涉钡、锶重金属无机化合物工业","100","30690","242","15.4","","5.5","硫酸雾","2024-09-19","6.63","6.63","mg/m3","20","","是","否",""]
["2024","09","19","新余市","高新区","江西东鹏新材料有限责任公司阳光大道厂","工业企业","2613|无机盐制造","水环境,大气环境,土壤污染监管","4#排气筒005(DA005)","国家标准","无机化学工业污染物排放标准(GB31573-2015)","（表3）大气污染排放限值,所有","100","32716","242","15.4","","5.9","颗粒物","2024-09-19","3.7","3.7","mg/m3","30","","是","否",""]
["2024","09","19","新余市","高新区","江西东鹏新材料有限责任公司阳光大道厂","工业企业","2613|无机盐制造","水环境,大气环境,土壤污染监管","2#排气筒003(DA003)","国家标准","无机化学工业污染物排放标准(GB31573-2015)","（表3）大气污染排放限值,所有","100","59482","123","3.5","11.51","5.1","氮氧化物","2024-09-19","64","87","mg/m3","200","","是","否",""]
["2024","09","19","新余市","高新区","江西东鹏新材料有限责任公司阳光大道厂","工业企业","2613|无机盐制造","水环境,大气环境,土壤污染监管","2#排气筒003(DA003)","国家标准","无机化学工业污染物排放标准(GB31573-2015)","（表3）大气污染排放限值,所有","100","52266","123","3.5","10.97","4.4","颗粒物","2024-09-19","12.6","16.3","mg/m3","30","","是","否",""]
["2024","09","19","新余市","高新区","江西东鹏新材料有限责任公司阳光大道厂","工业企业","2613|无机盐制造","水环境,大气环境,土壤污染监管","2#排气筒003(DA003)","国家标准","无机化学工业污染物排放标准(GB31573-2015)","（表3）大气污染排放限值,所有","100","59482","123","3.5","11.51","5.1","二氧化硫","2024-09-19","61","83","mg/m3","100","","是","否",""]
["2024","09","19","新余市","高新区","江西东鹏新材料有限责任公司阳光大道厂","工业企业","2613|无机盐制造","水环境,大气环境,土壤污染监管","2#排气筒003(DA003)","国家标准","无机化学工业污染物排放标准(GB31573-2015)","（表3）大气污染排放限值,涉铊、锌、铜、铅重金属无机化合物工业","100","62564","123","3.5","11.51","5.3","铊及其化合物（以铊计）","2024-09-19","0.000176","0.000245","mg/m3","0.05","","是","否",""]
["2024","09","04","新余市","高新区","江西鸿强科技有限公司","工业企业","2613|无机盐制造","大气环境","喷淋废气排放口(DA001)","国家标准","无机化学工业污染物排放标准(GB31573-2015)","（表3）大气污染排放限值,无机氯化合物及氯酸盐工业","100","192","44.8","4","20.8","2.1","氯气","2024-09-04","1.20","1.20","mg/m3","8","","是","否",""]
["2024","09","04","新余市","高新区","江西鸿强科技有限公司","工业企业","2613|无机盐制造","大气环境","喷淋废气排放口(DA001)","国家标准","无机化学工业污染物排放标准(GB31573-2015)","（表3）大气污染排放限值,无机氯化合物及氯酸盐工业","100","192","44.8","4","20.8","2.1","氯化氢","2024-09-04","6.37","6.37","mg/m3","20","","是","否",""]
["2024","09","04","新余市","高新区","江西鸿强科技有限公司","工业企业","2613|无机盐制造","大气环境","喷淋废气排放口(DA001)","国家标准","无机化学工业污染物排放标准(GB31573-2015)","（表3）大气污染排放限值,所有","100","192","44.8","4","20.8","2.1","颗粒物","2024-09-04","<20","<20","mg/m3","30","","是","否",""]
["2024","09","24","新余市","高新区","江西怡顺环保新材料有限公司","工业企业","2661|化学试剂和助剂制造","水环境,大气环境","锅炉排气口(DA001)","国家标准","锅炉大气污染物排放标准(GB13271-2014)","（表2）新建锅炉大气污染物排放浓度限值（2014年7月1日起新建锅炉）,烟囱或烟道,燃煤锅炉","100","7738","240","2.5","9.05","9.5","汞及其化合物","2024-09-24","0.00685","0.00687","mg/m3","0.05","","是","否",""]
["2024","09","24","新余市","高新区","江西怡顺环保新材料有限公司","工业企业","2661|化学试剂和助剂制造","水环境,大气环境","锅炉排气口(DA001)","国家标准","锅炉大气污染物排放标准(GB13271-2014)","（表2）新建锅炉大气污染物排放浓度限值（2014年7月1日起新建锅炉）,烟囱或烟道,燃煤锅炉","100","7738","240","2.5","9.05","9.5","氮氧化物","2024-09-24","167.4","168","mg/m3","300","","是","否",""]
["2024","09","24","新余市","高新区","江西怡顺环保新材料有限公司","工业企业","2661|化学试剂和助剂制造","水环境,大气环境","锅炉排气口(DA001)","国家标准","锅炉大气污染物排放标准(GB13271-2014)","（表2）新建锅炉大气污染物排放浓度限值（2014年7月1日起新建锅炉）,烟囱或烟道,燃煤锅炉","100","7738","240","2.5","9.05","9.5","颗粒物","2024-09-24","<20","<20","mg/m3","50","","是","否",""]
["2024","09","24","新余市","高新区","江西怡顺环保新材料有限公司","工业企业","2661|化学试剂和助剂制造","水环境,大气环境","对苯二甲酸烘干尾气排气口(DA001)","国家标准","大气污染物综合排放标准(GB16297-1996)","（表2）新污染源大气污染物排放限值（1997年1月1日起）,最高允许排放浓度,使用溶剂汽油或其他混合烃类物质,排气筒15m,二级,10","100","15839","76.9","3.6","","20.9","非甲烷总烃","2024-09-24","1.23","1.23","mg/m3","120","","是","否",""]
["2024","09","24","新余市","高新区","江西怡顺环保新材料有限公司","工业企业","2661|化学试剂和助剂制造","水环境,大气环境","对苯二甲酸烘干尾气排气口(DA001)","国家标准","大气污染物综合排放标准(GB16297-1996)","（表2）新污染源大气污染物排放限值（1997年1月1日起）,最高允许排放浓度,除碳黑尘、燃料尘、玻璃棉尘、石英粉尘、矿渣棉尘外其他,排气筒15m,二级,3.5","100","15839","76.9","3.6","","20.9","颗粒物","2024-09-24","<20","<20","mg/m3","120","","是","否",""]
["2024","09","24","新余市","高新区","江西怡顺环保新材料有限公司","工业企业","2661|化学试剂和助剂制造","水环境,大气环境","锅炉排气口(DA001)","国家标准","锅炉大气污染物排放标准(GB13271-2014)","（表2）新建锅炉大气污染物排放浓度限值（2014年7月1日起新建锅炉）,烟囱排放口,燃煤锅炉","100","","","","","","烟气黑度（林格曼黑度，级）","2024-09-24","<1","<1","级","1","","是","否",""]
["2024","09","24","新余市","高新区","江西怡顺环保新材料有限公司","工业企业","2661|化学试剂和助剂制造","水环境,大气环境","锅炉排气口(DA001)","国家标准","锅炉大气污染物排放标准(GB13271-2014)","（表2）新建锅炉大气污染物排放浓度限值（2014年7月1日起新建锅炉）,烟囱或烟道,燃煤锅炉","100","7738","240","2.5","9.05","9.5","二氧化硫","2024-09-24","45.6","46","mg/m3","300","","是","否",""]
["2024","09","27","新余市","仙女湖区","新余市永基新型环保建材有限责任公司","工业企业","303|砖瓦、石材等建筑材料制造","大气环境","焙烧废气处理设施（脱硫塔）排放口(DA001)","国家标准","砖瓦工业大气污染物排放标准(GB29620-2013)","（表1、表2）现有和新建企业大气污染物排放浓度限值,人工干燥及焙烧","100","40765","45","11.9","19.43","6","氮氧化物","2024-09-27","33.1","63","mg/m3","200","","是","否",""]
["2024","09","27","新余市","仙女湖区","新余市永基新型环保建材有限责任公司","工业企业","303|砖瓦、石材等建筑材料制造","大气环境","焙烧废气处理设施（脱硫塔）排放口(DA001)","国家标准","砖瓦工业大气污染物排放标准(GB29620-2013)","（修改单）新建企业大气污染物排放浓度限值,人工干燥及焙烧","100","40765","45","11.9","19.43","6","二氧化硫","2024-09-27","70.6","135","mg/m3","150","","是","否",""]
["2024","09","27","新余市","仙女湖区","新余市永基新型环保建材有限责任公司","工业企业","303|砖瓦、石材等建筑材料制造","大气环境","焙烧废气处理设施（脱硫塔）排放口(DA001)","国家标准","砖瓦工业大气污染物排放标准(GB29620-2013)","（表1、表2）现有和新建企业大气污染物排放浓度限值,人工干燥及焙烧","100","40765","45","11.9","19.43","6","氟化物","2024-09-27","1.03","1.97","mg/m3","3","","是","否",""]
["2024","09","27","新余市","仙女湖区","新余市永基新型环保建材有限责任公司","工业企业","303|砖瓦、石材等建筑材料制造","大气环境","焙烧废气处理设施（脱硫塔）排放口(DA001)","国家标准","砖瓦工业大气污染物排放标准(GB29620-2013)","（表1、表2）现有和新建企业大气污染物排放浓度限值,原料燃烧破碎及制备成型","100","40632","45","11.8","19.43","6","颗粒物","2024-09-27","4.0","7.6","mg/m3","30","","是","否",""]
["2024","09","12","新余市","","江西明迪科技有限公司","工业企业","2641|涂料制造","大气环境","合成树脂生产车间工艺废气排口(DA001)","国家标准","合成树脂工业污染物排放标准(GB31572-2015)","（表4）大气污染物排放限值,非焚烧类有机废气排放口,丙烯酸树脂","75","4086","27","3.9","","5.5","丙烯酸甲酯","2024-09-12","<1","<1","mg/m3","50","","是","否",""]
["2024","09","12","新余市","","江西明迪科技有限公司","工业企业","2641|涂料制造","大气环境","油性涂料生产车间工艺废气排口(DA004)","国家标准","涂料、油墨及胶粘剂工业大气污染物排放标准(GB37824—2019)","（表1）大气污染物排放限值,车间或生产设施排气筒,涂料制造、油墨及类似产品制造","75","6613","31","3.8","","8.9","苯系物","2024-09-12","1.109","1.109","mg/m3","60","","是","否",""]
["2024","09","12","新余市","","江西明迪科技有限公司","工业企业","2641|涂料制造","大气环境","油性涂料生产车间工艺废气排口(DA004)","地方标准","挥发性有机物排放标准  第2部分：有机化工行业[地标](DB36/1101.2-2019)","表1  有组织挥发性有机物排放限值","75","6613","31","3.8","","8.9","非甲烷总烃","2024-09-12","5.25","5.25","mg/m3","80","","是","否",""]
["2024","09","12","新余市","","江西明迪科技有限公司","工业企业","2641|涂料制造","大气环境","合成树脂生产车间工艺废气排口(DA001)","国家标准","合成树脂工业污染物排放标准(GB31572-2015)","（表4）大气污染物排放限值,非焚烧类有机废气排放口,丙烯酸树脂","75","4086","27","3.9","","5.5","甲基丙烯酸甲酯","2024-09-12","<1","<1","mg/m3","100","","是","否",""]
["2024","09","12","新余市","","江西明迪科技有限公司","工业企业","2641|涂料制造","大气环境","合成树脂生产车间工艺废气排口(DA001)","国家标准","合成树脂工业污染物排放标准(GB31572-2015)","（表4）大气污染物排放限值,非焚烧类有机废气排放口,聚苯乙烯树脂","75","4086","27","3.9","","5.5","苯乙烯","2024-09-12","<0.004","<0.004","mg/m3","50","","是","否",""]
["2024","09","12","新余市","","江西明迪科技有限公司","工业企业","2641|涂料制造","大气环境","合成树脂生产车间工艺废气排口(DA001)","国家标准","合成树脂工业污染物排放标准(GB31572-2015)","（表4）大气污染物排放限值,非焚烧类有机废气排放口,丙烯酸树脂","75","4086","27","3.9","","5.5","丙烯酸丁酯","2024-09-12","<1","<1","mg/m3","50","","是","否",""]
["2024","09","12","新余市","","江西明迪科技有限公司","工业企业","2641|涂料制造","大气环境","油性涂料生产车间工艺废气排口(DA004)","国家标准","恶臭污染物排放标准(GB14554-93)","（表2）恶臭污染物排放标准值,排气筒高度15m","75","6613","31","3.8","","8.9","臭气浓度","2024-09-12","98","98","无量纲","2000","","是","否",""]
["2024","09","12","新余市","","江西明迪科技有限公司","工业企业","2641|涂料制造","大气环境","油性涂料生产车间工艺废气排口(DA004)","地方标准","挥发性有机物排放标准 第2部分(有机化工行业DB36 1101.2-2019DB36 1101.2-2019)","挥发性有机物排放标准 第2部分：有机化工行业DB36 1101.2-2019DB36 1101.2-2019\t","75","6613","31","3.8","","8.9","二甲苯","2024-09-12","0.794","0.794","mg/m3","15","","是","否",""]
["2024","09","12","新余市","","江西明迪科技有限公司","工业企业","2641|涂料制造","大气环境","合成树脂生产车间工艺废气排口(DA001)","国家标准","恶臭污染物排放标准(GB14554-93)","（表2）恶臭污染物排放标准值,排气筒高度15m","75","4086","27","3.9","","5.5","臭气浓度","2024-09-12","41","41","无量纲","2000","","是","否",""]
["2024","09","12","新余市","","江西明迪科技有限公司","工业企业","2641|涂料制造","大气环境","油性涂料生产车间工艺废气排口(DA004)","国家标准","涂料、油墨及胶粘剂工业大气污染物排放标准(GB37824—2019)","（表1）大气污染物排放限值,车间或生产设施排气筒,涂料制造、油墨及类似产品制造","75","6613","31","3.8","","8.9","颗粒物","2024-09-12","<20","<20","mg/m3","30","","是","否",""]
["2024","09","12","新余市","","江西明迪科技有限公司","工业企业","2641|涂料制造","大气环境","油性涂料生产车间工艺废气排口(DA004)","国家标准","涂料、油墨及胶粘剂工业大气污染物排放标准(GB37824—2019)","（表1）大气污染物排放限值,车间或生产设施排气筒,涂料制造、油墨及类似产品制造","75","6613","31","3.8","","8.9","总挥发性有机物","2024-09-12","1.148","1.148","mg/m3","120","","是","否",""]
["2024","09","12","新余市","","江西明迪科技有限公司","工业企业","2641|涂料制造","大气环境","合成树脂生产车间工艺废气排口(DA001)","国家标准","合成树脂工业污染物排放标准(GB31572-2015)","（表4）大气污染物排放限值,非焚烧类有机废气排放口,所有合成树脂","75","4086","27","3.9","","5.5","颗粒物","2024-09-12","<20","<20","mg/m3","30","","是","否",""]
["2024","09","12","新余市","","江西明迪科技有限公司","工业企业","2641|涂料制造","大气环境","合成树脂生产车间工艺废气排口(DA001)","地方标准","挥发性有机物排放标准　第2部分有机化工行业(ＤＢ36/1101.2-2019)","挥发性有机物排放标准,挥发性有机物排放标准第2部分有机化工行业","75","4086","27","3.9","","5.5","非甲烷总烃","2024-09-12","1.74","1.74","mg/m3","80","","是","否",""]
["2024","09","12","新余市","","江西明迪科技有限公司","工业企业","2641|涂料制造","大气环境","油性涂料生产车间工艺废气排口(DA004)","国家标准","涂料、油墨及胶粘剂工业大气污染物排放标准(GB37824—2019)","（表1）大气污染物排放限值,车间或生产设施排气筒,涂料制造、油墨及类似产品制造","75","6613","31","3.8","","8.9","苯","2024-09-12","<0.004","<0.004","mg/m3","1","","是","否",""]
["2024","09","23","新余市","","江西新钢环保科技有限公司","工业企业","42|废弃资源综合利用业","大气环境,土壤污染监管","5#排放口004(DA004)","国家标准","钢铁烧结、球团工业大气污染物排放标准(GB28662-2012)","（表2）新建企业大气污染物排放浓度限值,烧结机球团焙烧设备","100","51845","136","2.5","12.16","2.8","氮氧化物","2024-09-23","51","17","mg/m3","300","","是","否",""]
["2024","09","23","新余市","","江西新钢环保科技有限公司","工业企业","42|废弃资源综合利用业","大气环境,土壤污染监管","5#排放口004(DA004)","国家标准","钢铁烧结、球团工业大气污染物排放标准(GB28662-2012)","（表2）新建企业大气污染物排放浓度限值,烧结机球团焙烧设备","100","51845","136","2.5","12.16","2.8","氟化物","2024-09-23","1.70","0.577","mg/m3","4.0","","是","否",""]
["2024","09","23","新余市","","江西新钢环保科技有限公司","工业企业","42|废弃资源综合利用业","大气环境,土壤污染监管","5#排放口004(DA004)","国家标准","钢铁烧结、球团工业大气污染物排放标准(GB28662-2012)","（表2）新建企业大气污染物排放浓度限值,烧结机球团焙烧设备","100","51845","136","2.5","12.16","2.8","二氧化硫","2024-09-23","14","5","mg/m3","200","","是","否",""]
["2024","09","23","新余市","","江西新钢环保科技有限公司","工业企业","42|废弃资源综合利用业","大气环境,土壤污染监管","5#排放口004(DA004)","国家标准","钢铁烧结、球团工业大气污染物排放标准(GB28662-2012)","（表2）新建企业大气污染物排放浓度限值,烧结机球团焙烧设备","100","44267","136","2.5","12.31","2.4","颗粒物","2024-09-23","7.6","2.6","mg/m3","50","","是","否",""]
["2024","09","11","新余市","","江西鑫德新科技有限公司","工业企业","3211|铜冶炼","大气环境","汽馏热解炉排口(DA001)","国家标准","危险废物焚烧污染控制标准(GB 18484—2020)","表 3 危险废物焚烧设施烟气污染物排放浓度限值,测定均值","90","10048","58.4","16.3","16.8","4.3","铬及其化合物","2024-09-11","<0.012","<0.012","mg/m3","0.5","","是","否",""]
["2024","09","11","新余市","","江西鑫德新科技有限公司","工业企业","3211|铜冶炼","大气环境","汽馏热解炉排口(DA001)","国家标准","危险废物焚烧污染控制标准(GB 18484—2020)","表 3 危险废物焚烧设施烟气污染物排放浓度限值,1 小时均值","90","10380","56.7","16.3","16.4","4.4","颗粒物","2024-09-11","<20","<20","mg/m3","30","","是","否",""]
["2024","09","11","新余市","","江西鑫德新科技有限公司","工业企业","3211|铜冶炼","大气环境","汽馏热解炉排口(DA001)","国家标准","危险废物焚烧污染控制标准(GB 18484—2020)","表 3 危险废物焚烧设施烟气污染物排放浓度限值,测定均值","90","10048","58.4","16.3","16.8","4.3","铅及其化合物","2024-09-11","<0.006","<0.006","mg/m3","0.5","","是","否",""]
["2024","09","11","新余市","","江西鑫德新科技有限公司","工业企业","3211|铜冶炼","大气环境","汽馏热解炉排口(DA001)","国家标准","危险废物焚烧污染控制标准(GB 18484—2020)","表 3 危险废物焚烧设施烟气污染物排放浓度限值,测定均值","90","10048","58.4","16.3","16.8","4.3","锡、锑、铜、锰、镍、钴及其化合物","2024-09-11","<0.006","<0.006","mg/m3","2.0","","是","否",""]
["2024","09","11","新余市","","江西鑫德新科技有限公司","工业企业","3211|铜冶炼","大气环境","汽馏热解炉排口(DA001)","地方标准","（上海市大气污染物综合排放标准）(DB31/933-2015)","表1大气污染物项目排放限值","90","10380","56.7","16.3","16.4","4.4","溴化氢","2024-09-11","0.08","0.08","mg/m3","5.0","","是","否",""]
["2024","09","11","新余市","","江西鑫德新科技有限公司","工业企业","3211|铜冶炼","大气环境","汽馏热解炉排口(DA001)","地方标准","天津市工业企业挥发性有机物排放控制标准(DB12 524-2020)","挥发性有机物有组织排放限值,其他行业","90","10380","56.7","16.3","16.4","4.4","挥发性有机物","2024-09-11","0.395","0.881","mg/m3","60","","是","否",""]
["2024","09","11","新余市","","江西鑫德新科技有限公司","工业企业","3211|铜冶炼","大气环境","汽馏热解炉排口(DA001)","国家标准","危险废物焚烧污染控制标准(GB 18484—2020)","表 3 危险废物焚烧设施烟气污染物排放浓度限值,24 小时均值或日均值","90","10380","56.7","16.3","16.4","4.4","氟化氢","2024-09-11","0.19","0.45","mg/m3","4.0","","是","否",""]
["2024","09","11","新余市","","江西鑫德新科技有限公司","工业企业","3211|铜冶炼","大气环境","汽馏热解炉排口(DA001)","国家标准","危险废物焚烧污染控制标准(GB 18484—2020)","表 3 危险废物焚烧设施烟气污染物排放浓度限值,测定均值","90","10048","58.4","16.3","16.8","4.3","镉及其化合物","2024-09-11","<0.0024","<0.0024","mg/m3","0.05","","是","否",""]
["2024","09","11","新余市","","江西鑫德新科技有限公司","工业企业","3211|铜冶炼","大气环境","汽馏热解炉排口(DA001)","国家标准","危险废物焚烧污染控制标准(GB 18484—2020)","表 3 危险废物焚烧设施烟气污染物排放浓度限值,测定均值","90","10048","58.4","16.3","16.8","4.3","砷及其化合物","2024-09-11","<0.0027","<0.0027","mg/m3","0.5","","是","否",""]
["2024","09","11","新余市","","江西鑫德新科技有限公司","工业企业","3211|铜冶炼","大气环境","汽馏热解炉排口(DA001)","国家标准","危险废物焚烧污染控制标准(GB 18484—2020)","表 3 危险废物焚烧设施烟气污染物排放浓度限值,测定均值","90","9972.3","58.3","16.3","16.3","4.3","汞及其化合物","2024-09-11","0.00107","0.00227","mg/m3","0.05","","是","否",""]
["2024","09","11","新余市","","江西鑫德新科技有限公司","工业企业","3211|铜冶炼","大气环境","汽馏热解炉排口(DA001)","国家标准","危险废物焚烧污染控制标准(GB 18484—2020)","表 3 危险废物焚烧设施烟气污染物排放浓度限值,1 小时均值","90","10380","56.7","16.3","16.4","4.4","氯化氢","2024-09-11","1.35","2.88","mg/m3","60","","是","否",""]
["2024","09","12","新余市","","江西鑫德新科技有限公司","工业企业","3211|铜冶炼","大气环境","CF炉烟气排口(DA002)","国家标准","再生铜、铝、铅、锌工业污染物排放标准(GB31574-2015)","（表5）企业边界大气污染物限值,所有","90","11800","51.97","5.12","","4.4","砷及其化合物","2024-09-12","<0.0027","<0.0027","mg/m3","0.4","","是","否",""]
["2024","09","12","新余市","","江西鑫德新科技有限公司","工业企业","3211|铜冶炼","大气环境","CF炉烟气排口(DA002)","国家标准","再生铜、铝、铅、锌工业污染物排放标准(GB31574-2015)","（表5）企业边界大气污染物限值,所有","90","11800","51.97","5.12","","4.4","锡及其化合物","2024-09-12","<0.006","<0.006","mg/m3","1","","是","否",""]
["2024","09","12","新余市","","江西鑫德新科技有限公司","工业企业","3211|铜冶炼","大气环境","CF炉烟气排口(DA002)","国家标准","再生铜、铝、铅、锌工业污染物排放标准(GB31574-2015)","（表3）大气污染物排放限值,车间或生产设施排气筒,所有","90","11800","51.97","5.12","","4.4","铬及其化合物","2024-09-12","<0.0012","<0.0012","mg/m3","1","","是","否",""]
["2024","09","12","新余市","","江西鑫德新科技有限公司","工业企业","3211|铜冶炼","大气环境","CF炉烟气排口(DA002)","国家标准","再生铜、铝、铅、锌工业污染物排放标准(GB31574-2015)","（表3）大气污染物排放限值,车间或生产设施排气筒,所有","90","11580","51.8","5.12","","4.3","颗粒物","2024-09-12","<20","<20","mg/m3","30","","是","否",""]
["2024","09","12","新余市","","江西鑫德新科技有限公司","工业企业","3211|铜冶炼","大气环境","CF炉烟气排口(DA002)","国家标准","再生铜、铝、铅、锌工业污染物排放标准(GB31574-2015)","（表5）企业边界大气污染物限值,所有","90","11800","51.97","5.12","","4.4","铅及其化合物","2024-09-12","<0.006","<0.006","mg/m3","2","","是","否",""]
["2024","09","12","新余市","","江西鑫德新科技有限公司","工业企业","3211|铜冶炼","大气环境","CF炉烟气排口(DA002)","国家标准","再生铜、铝、铅、锌工业污染物排放标准(GB31574-2015)","（表5）企业边界大气污染物限值,所有","90","11800","51.97","5.12","","4.4","镉及其化合物","2024-09-12","<0.0024","<0.0024","mg/m3","0.05","","是","否",""]
["2024","09","12","新余市","","江西鑫德新科技有限公司","工业企业","3211|铜冶炼","大气环境","CF炉烟气排口(DA002)","国家标准","再生铜、铝、铅、锌工业污染物排放标准(GB31574-2015)","（表5）企业边界大气污染物限值,再生铅、再生铜","90","11800","51.97","5.12","","4.4","锑及其化合物","2024-09-12","<0.0024","<0.0024","mg/m3","1","","是","否",""]
["2024","09","13","新余市","","江西鑫德新科技有限公司","工业企业","3211|铜冶炼","大气环境","汽馏热解炉排口(DA001)","国家标准","危险废物焚烧污染控制标准(GB 18484—2020)","表 3 危险废物焚烧设施烟气污染物排放浓度限值,测定均值","50","11972","53.4","14.5","16.2","4.97","二噁英类","2024-09-13","0.053","0.11","ng TEQ/Nm3","0.5","","是","否",""]
["2024","09","05","新余市","","新余市佳林香料有限责任公司","工业企业","2684|香料、香精制造","水环境,大气环境","锅炉废气排放口002(DA002)","国家标准","锅炉大气污染物排放标准(GB13271-2014)","（表2）新建锅炉大气污染物排放浓度限值（2014年7月1日起新建锅炉）,烟囱或烟道,燃煤锅炉","100","12103","98","2.3","15.7","9.3","氮氧化物","2024-09-05","86","195","mg/m3","300","","是","否",""]
["2024","09","05","新余市","","新余市佳林香料有限责任公司","工业企业","2684|香料、香精制造","水环境,大气环境","锅炉废气排放口002(DA002)","国家标准","锅炉大气污染物排放标准(GB13271-2014)","（表2）新建锅炉大气污染物排放浓度限值（2014年7月1日起新建锅炉）,烟囱或烟道,燃煤锅炉","100","11891","98","2.3","15.63","9.1","颗粒物","2024-09-05","6.6","14.9","mg/m3","50","","是","否",""]
["2024","09","05","新余市","","新余市佳林香料有限责任公司","工业企业","2684|香料、香精制造","水环境,大气环境","锅炉废气排放口002(DA002)","国家标准","锅炉大气污染物排放标准(GB13271-2014)","（表2）新建锅炉大气污染物排放浓度限值（2014年7月1日起新建锅炉）,烟囱排放口,燃煤锅炉","100","","","","","","林格曼黑度","2024-09-05","<1","<1","级","1","","是","否",""]
["2024","09","05","新余市","","新余市佳林香料有限责任公司","工业企业","2684|香料、香精制造","水环境,大气环境","锅炉废气排放口002(DA002)","国家标准","锅炉大气污染物排放标准(GB13271-2014)","（表2）新建锅炉大气污染物排放浓度限值（2014年7月1日起新建锅炉）,烟囱或烟道,燃煤锅炉","100","12103","98","2.3","15.7","9.3","二氧化硫","2024-09-05","28","64","mg/m3","300","","是","否",""]
["2024","09","10","新余市","","新余市佳林香料有限责任公司","工业企业","2684|香料、香精制造","水环境,大气环境","1#废气排放口001(DA001)","地方标准","挥发性有机物排放标准  第2部分：有机化工行业[地标](DB36/1101.2-2019)","表1  有组织挥发性有机物排放限值","100","3151","85.3","5.2","","9.7","非甲烷总烃","2024-09-10","0.25","0.25","mg/m3","80","","是","否",""]
["2024","09","10","新余市","","新余市佳林香料有限责任公司","工业企业","2684|香料、香精制造","水环境,大气环境","1#废气排放口001(DA001)","地方标准","挥发性有机物排放标准  第2部分：有机化工行业[地标](DB36/1101.2-2019)","表1  有组织挥发性有机物排放限值","100","3151","85.3","5.2","","9.7","二甲苯（总量）","2024-09-10","0.366","0.366","mg/m3","15","","是","否",""]
["2024","09","10","新余市","","新余市佳林香料有限责任公司","工业企业","2684|香料、香精制造","水环境,大气环境","1#废气排放口001(DA001)","地方标准","挥发性有机物排放标准  第2部分：有机化工行业[地标](DB36/1101.2-2019)","表1  有组织挥发性有机物排放限值","100","3151","85.3","5.2","","9.7","甲苯","2024-09-10","0.035","0.035","mg/m3","10","","是","否",""]
["2024","09","10","新余市","","新余市佳林香料有限责任公司","工业企业","2684|香料、香精制造","水环境,大气环境","1#废气排放口001(DA001)","地方标准","挥发性有机物排放标准  第2部分：有机化工行业[地标](DB36/1101.2-2019)","表1  有组织挥发性有机物排放限值","100","3151","85.3","5.2","","9.7","总挥发性有机物","2024-09-10","1.84","1.84","mg/m3","120","","是","否",""]
["2024","09","10","新余市","","新余市佳林香料有限责任公司","工业企业","2684|香料、香精制造","水环境,大气环境","1#废气排放口001(DA001)","地方标准","挥发性有机物排放标准  第2部分：有机化工行业[地标](DB36/1101.2-2019)","表1  有组织挥发性有机物排放限值","100","3151","85.3","5.2","","9.7","苯","2024-09-10","0.096","0.096","mg/m3","4","","是","否",""]

{"sheet":"废水排放","index":1,"n_rows":38,"n_cols":25,"rows_kept":38,"merged":[[0,0,0,24]],"flags":["formulas_cached_only"]}
["执法监测废水排放数据",null,"","","","","","","","","","","","","","","","","","","","","","",""]
["监测年","监测月","监测日","市","县","企业名称","企业类别","行业类别","名录类别","监测点名称","排放标准类型","排放标准名称","标准条目","废水工作负荷","废水流量","废水水温","监测项目","项目监测日期","排放浓度","取值单位","排放上限","排放下限","是否有评价限值","是否超标","超标倍数"]
["2024","09","03","新余市","渝水区","新余钢铁集团有限公司中心医院","工业企业","8411|综合医院","水环境","北院污水处理站废水排放口(DW004)","国家标准","医疗机构水污染物排放标准(GB18466-2005)","（表2）综合医疗机构和其他医疗机构水污染物排放限值（日均值）,含氯消毒剂,消毒接触池的接触时间大于等于1小时，接触池出口,预处理标准","82","","","粪大肠菌群数","2024-09-03","13","MPN/L","5000","","是","否",""]
["2024","09","09","新余市","渝水区","新余双胞胎猪业有限公司","畜禽养殖场","0313|猪的饲养","水环境","综合污水处理站排放口001(DW001)","国家标准","畜禽养殖业污染物排放标准(GB18596-2001)","（表5）集约化畜禽养殖业水污染物最高允许日均排放浓度","83","","31.4","五日生化需氧量（BOD5）","2024-09-09","0.8","mg/L","150","","是","否",""]
["2024","09","09","新余市","渝水区","新余双胞胎猪业有限公司","畜禽养殖场","0313|猪的饲养","水环境","综合污水处理站排放口001(DW001)","地方标准","鄱阳湖生态经济区水污染物排放标准(DB36/852-2015)","规模化畜禽养殖业,高效集约发展区","83","","31.4","悬浮物","2024-09-09","8","mg/L","150","","是","否",""]
["2024","09","09","新余市","渝水区","新余双胞胎猪业有限公司","畜禽养殖场","0313|猪的饲养","水环境","综合污水处理站排放口001(DW001)","地方标准","鄱阳湖生态经济区水污染物排放标准(DB36/852-2015)","规模化畜禽养殖业,高效集约发展区","83","","31.4","氨氮","2024-09-09","0.130","mg/L","40","","是","否",""]
["2024","09","09","新余市","渝水区","新余双胞胎猪业有限公司","畜禽养殖场","0313|猪的饲养","水环境","综合污水处理站排放口001(DW001)","国家标准","畜禽养殖业污染物排放标准(GB18596-2001)","（表5）集约化畜禽养殖业水污染物最高允许日均排放浓度","83","","31.4","粪大肠菌群数","2024-09-09","<1","个/100ml","1000","","是","否",""]
["2024","09","09","新余市","渝水区","新余双胞胎猪业有限公司","畜禽养殖场","0313|猪的饲养","水环境","综合污水处理站排放口001(DW001)","地方标准","鄱阳湖生态经济区水污染物排放标准(DB36/852-2015)","规模化畜禽养殖业,高效集约发展区","83","","31.4","化学需氧量","2024-09-09","6","mg/L","150","","是","否",""]
["2024","09","09","新余市","渝水区","新余双胞胎猪业有限公司","畜禽养殖场","0313|猪的饲养","水环境","综合污水处理站排放口001(DW001)","地方标准","鄱阳湖生态经济区水污染物排放标准(DB36/852-2015)","规模化畜禽养殖业,高效集约发展区","83","","31.4","总氮","2024-09-09","2.00","mg/L","70","","是","否",""]
["2024","09","09","新余市","渝水区","新余双胞胎猪业有限公司","畜禽养殖场","0313|猪的饲养","水环境","综合污水处理站排放口001(DW001)","国家标准","畜禽养殖业污染物排放标准(GB18596-2001)","（表5）集约化畜禽养殖业水污染物最高允许日均排放浓度","83","","31.4","蛔虫卵","2024-09-09","<0.5","个/L","2.0","","是","否",""]
["2024","09","09","新余市","渝水区","新余双胞胎猪业有限公司","畜禽养殖场","0313|猪的饲养","水环境","综合污水处理站排放口001(DW001)","地方标准","鄱阳湖生态经济区水污染物排放标准(DB36/852-2015)","规模化畜禽养殖业,高效集约发展区","83","","31.4","总磷","2024-09-09","3.40","mg/L","5","","是","否",""]
["2024","09","19","新余市","高新区","江西东鹏新材料有限责任公司阳光大道厂","工业企业","2613|无机盐制造","水环境,大气环境,土壤污染监管","生产废水排放口001","国家标准","无机化学工业污染物排放标准(GB31573-2015)"," （表1）水污染物排放限值,间接排放","100","","39","总磷（以P计）","2024-09-19","0.03","mg/L","2","","是","否",""]
["2024","09","19","新余市","高新区","江西东鹏新材料有限责任公司阳光大道厂","工业企业","2613|无机盐制造","水环境,大气环境,土壤污染监管","生产废水排放口001","国家标准","无机化学工业污染物排放标准(GB31573-2015)"," （表1）水污染物排放限值,间接排放","100","","39","总锑","2024-09-19","0.00187","mg/L","0.3","","是","否",""]
["2024","09","19","新余市","高新区","江西东鹏新材料有限责任公司阳光大道厂","工业企业","2613|无机盐制造","水环境,大气环境,土壤污染监管","生产废水排放口001","国家标准","无机化学工业污染物排放标准(GB31573-2015)"," （表1）水污染物排放限值,间接排放","100","","39","石油类","2024-09-19","<0.06","mg/L","6","","是","否",""]
["2024","09","19","新余市","高新区","江西东鹏新材料有限责任公司阳光大道厂","工业企业","2613|无机盐制造","水环境,大气环境,土壤污染监管","生产废水排放口001","国家标准","无机化学工业污染物排放标准(GB31573-2015)"," （表1）水污染物排放限值,间接排放","100","","39","pH值","2024-09-19","7.7","无量纲","9","6","是","否",""]
["2024","09","19","新余市","高新区","江西东鹏新材料有限责任公司阳光大道厂","工业企业","2613|无机盐制造","水环境,大气环境,土壤污染监管","生产废水排放口001","地方标准","新余高新区污水处理厂接管标准(001)","污水处理厂接管进水限值","100","","39","氨氮（NH3-N）","2024-09-19","0.261","mg/L","35","","是","否",""]
["2024","09","19","新余市","高新区","江西东鹏新材料有限责任公司阳光大道厂","工业企业","2613|无机盐制造","水环境,大气环境,土壤污染监管","生产废水排放口001","国家标准","无机化学工业污染物排放标准(GB31573-2015)"," （表1）水污染物排放限值,间接排放","100","","39","化学需氧量","2024-09-19","18","mg/L","200","","是","否",""]
["2024","09","19","新余市","高新区","江西东鹏新材料有限责任公司阳光大道厂","工业企业","2613|无机盐制造","水环境,大气环境,土壤污染监管","生产废水排放口001","国家标准","无机化学工业污染物排放标准(GB31573-2015)"," （表1）水污染物排放限值,间接排放","100","","39","悬浮物","2024-09-19","12","mg/L","100","","是","否",""]
["2024","09","19","新余市","高新区","江西东鹏新材料有限责任公司阳光大道厂","工业企业","2613|无机盐制造","水环境,大气环境,土壤污染监管","生产废水排放口001","国家标准","无机化学工业污染物排放标准(GB31573-2015)"," （表1）水污染物排放限值,间接排放","100","","39","总铊","2024-09-19","0.00075","mg/L","0.005","","是","否",""]
["2024","09","19","新余市","高新区","江西东鹏新材料有限责任公司阳光大道厂","工业企业","2613|无机盐制造","水环境,大气环境,土壤污染监管","生产废水排放口001","地方标准","新余高新区污水处理厂接管标准(001)","污水处理厂接管进水限值","100","","39","总氮（以N计）","2024-09-19","6.94","mg/L","50","","是","否",""]
["2024","09","24","新余市","高新区","江西怡顺环保新材料有限公司","工业企业","2661|化学试剂和助剂制造","水环境,大气环境","废水东排口","地方标准","新余高新区污水处理厂接管标准(001)","污水处理厂接管进水限值","75","","34.2","氨氮（NH3-N）","2024-09-24","1.42","mg/L","35","","是","否",""]
["2024","09","24","新余市","高新区","江西怡顺环保新材料有限公司","工业企业","2661|化学试剂和助剂制造","水环境,大气环境","废水东排口","地方标准","新余高新区污水处理厂接管标准(001)","污水处理厂接管进水限值","75","","34.2","pH值","2024-09-24","8.1","无量纲","9","6","是","否",""]
["2024","09","24","新余市","高新区","江西怡顺环保新材料有限公司","工业企业","2661|化学试剂和助剂制造","水环境,大气环境","废水东排口","地方标准","新余高新区污水处理厂接管标准(001)","污水处理厂接管进水限值","75","","34.2","悬浮物","2024-09-24","18","mg/L","300","","是","否",""]
["2024","09","24","新余市","高新区","江西怡顺环保新材料有限公司","工业企业","2661|化学试剂和助剂制造","水环境,大气环境","废水东排口","地方标准","新余高新区污水处理厂接管标准(001)","污水处理厂接管进水限值","75","","34.2","化学需氧量","2024-09-24","368","mg/L","500","","是","否",""]
["2024","09","24","新余市","高新区","江西怡顺环保新材料有限公司","工业企业","2661|化学试剂和助剂制造","水环境,大气环境","废水东排口","地方标准","新余高新区污水处理厂接管标准(001)","污水处理厂接管进水限值","75","","34.2","五日生化需氧量（BOD5）","2024-09-24","4.9","mg/L","250","","是","否",""]
["2024","09","24","新余市","高新区","江西怡顺环保新材料有限公司","工业企业","2661|化学试剂和助剂制造","水环境,大气环境","废水东排口","地方标准","新余高新区污水处理厂接管标准(001)","污水处理厂接管进水限值","75","","34.2","总氮（以N计）","2024-09-24","6.54","mg/L","50","","是","否",""]
["2024","09","24","新余市","高新区","江西怡顺环保新材料有限公司","工业企业","2661|化学试剂和助剂制造","水环境,大气环境","废水东排口","地方标准","新余高新区污水处理厂接管标准(001)","污水处理厂接管进水限值","75","","34.2","总磷（以P计）","2024-09-24","0.03","mg/L","7","","是","否",""]
["2024","09","24","新余市","高新区","江西怡顺环保新材料有限公司","工业企业","2661|化学试剂和助剂制造","水环境,大气环境","废水东排口","国家标准","污水综合排放标准(GB8978-1996)","（表4）第二类污染物最高允许排放浓度（1998年1月1日后建的单位）,一切排污单位 ,三级标准","75","","34.2","阴离子表面活性剂（LAS）","2024-09-24","0.34","mg/L","20","","是","否",""]
["2024","09","03","新余市","高新区","新余市人民医院","工业企业","8411|综合医院","水环境","废水排放口001(DW001)","地方标准","城东污水处理厂接管标准(009)","城东污水处理厂接管标准","67","","","氨氮","2024-09-03","6.52","mg/L","25","","是","否",""]
["2024","09","03","新余市","高新区","新余市人民医院","工业企业","8411|综合医院","水环境","废水排放口001(DW001)","国家标准","医疗机构水污染物排放标准(GB18466-2005)","（表2）综合医疗机构和其他医疗机构水污染物排放限值（日均值）,含氯消毒剂,消毒接触池的接触时间大于等于1小时，接触池出口,预处理标准","67","","","粪大肠菌群数","2024-09-03","163","MPN/L","5000","","是","否",""]
["2024","09","05","新余市","","新余市佳林香料有限责任公司","工业企业","2684|香料、香精制造","水环境,大气环境","综合废水排放口001","地方标准","新余高新区污水处理厂接管标准(001)","污水处理厂接管进水限值","56","","35.7","悬浮物","2024-09-05","21","mg/L","300","","是","否",""]
["2024","09","05","新余市","","新余市佳林香料有限责任公司","工业企业","2684|香料、香精制造","水环境,大气环境","综合废水排放口001","地方标准","新余高新区污水处理厂接管标准(001)","污水处理厂接管进水限值","56","","35.7","化学需氧量","2024-09-05","132","mg/L","500","","是","否",""]
["2024","09","05","新余市","","新余市佳林香料有限责任公司","工业企业","2684|香料、香精制造","水环境,大气环境","综合废水排放口001","国家标准","污水综合排放标准(GB8978-1996)","（表4）第二类污染物最高允许排放浓度（1998年1月1日后建的单位）,一切排污单位 ,一级标准","56","","35.7","动植物油","2024-09-05","<0.06","mg/L","10","","是","否",""]
["2024","09","05","新余市","","新余市佳林香料有限责任公司","工业企业","2684|香料、香精制造","水环境,大气环境","综合废水排放口001","地方标准","新余高新区污水处理厂接管标准(001)","污水处理厂接管进水限值","56","","35.7","五日生化需氧量（BOD5）","2024-09-05","3.7","mg/L","250","","是","否",""]
["2024","09","05","新余市","","新余市佳林香料有限责任公司","工业企业","2684|香料、香精制造","水环境,大气环境","综合废水排放口001","地方标准","新余高新区污水处理厂接管标准(001)","污水处理厂接管进水限值","56","","35.7","氨氮（NH3-N）","2024-09-05","1.72","mg/L","35","","是","否",""]
["2024","09","05","新余市","","新余市佳林香料有限责任公司","工业企业","2684|香料、香精制造","水环境,大气环境","综合废水排放口001","地方标准","新余高新区污水处理厂接管标准(001)","污水处理厂接管进水限值","56","","35.7","pH值","2024-09-05","8.6","无量纲","9","","是","否",""]
["2024","09","05","新余市","","新余市佳林香料有限责任公司","工业企业","2684|香料、香精制造","水环境,大气环境","综合废水排放口001","地方标准","新余高新区污水处理厂接管标准(001)","污水处理厂接管进水限值","56","","35.7","总磷（以P计）","2024-09-05","1.94","mg/L","7","","是","否",""]
["2024","09","05","新余市","","新余市佳林香料有限责任公司","工业企业","2684|香料、香精制造","水环境,大气环境","综合废水排放口001","国家标准","污水综合排放标准(GB8978-1996)","（表4）第二类污染物最高允许排放浓度（1998年1月1日后建的单位）,一切排污单位 ,一级标准","56","","35.7","甲苯","2024-09-05","<0.0003","mg/L","0.1","","是","否",""]